(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 242)
    (zones 0)
    (modules 3)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.381)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.635 0.254)
    (user_via 0.762 0.381)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots"))
  )
  (net 0 "")
  (net 1 /A7)
  (net 2 /A6)
  (net 3 /A5)
  (net 4 /A4)
  (net 5 /A3)
  (net 6 /A2)
  (net 7 /A1)
  (net 8 /A0)
  (net 9 /CE#)
  (net 10 /GND)
  (net 11 /OE#)
  (net 12 /Q0)
  (net 13 /Q8)
  (net 14 /Q1)
  (net 15 /Q9)
  (net 16 /Q2)
  (net 17 /Q10)
  (net 18 /Q3)
  (net 19 /Q11)
  (net 20 /VCC)
  (net 21 /Q4)
  (net 22 /Q12)
  (net 23 /Q5)
  (net 24 /Q13)
  (net 25 /Q6)
  (net 26 /Q14)
  (net 27 /Q7)
  (net 28 /Q15)
  (net 29 /A16)
  (net 30 /A15)
  (net 31 /A13)
  (net 32 /A12)
  (net 33 /A11)
  (net 34 /A10)
  (net 35 /A9)
  (net 36 /A8)
  (net 37 /A14)
  (net 38 /A17)
  (net 39 /PIN31)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CE#)
    (add_net /GND)
    (add_net /OE#)
    (add_net /PIN31)
    (add_net /Q0)
    (add_net /Q1)
    (add_net /Q10)
    (add_net /Q11)
    (add_net /Q12)
    (add_net /Q13)
    (add_net /Q14)
    (add_net /Q15)
    (add_net /Q2)
    (add_net /Q3)
    (add_net /Q4)
    (add_net /Q5)
    (add_net /Q6)
    (add_net /Q7)
    (add_net /Q8)
    (add_net /Q9)
    (add_net /VCC)
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.635)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Passive:JMP1608X55-3 (layer F.Cu) (tedit 58FA73AC)
    (at 110.6 78.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference JP1 (at 0 1.651) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 1.5) (layer F.Fab))
    (fp_text user 3 (at 2.6 0.1) (layer F.SilkS))
    (fp_text user 1 (at -2.55 0.05) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 /A17))
    (pad 2 smd rect (at 0 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 /A17))
    (pad 3 smd rect (at 1.5 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 /PIN31))
  )
  (module AmigaRomAdapter2:FlipPins40 (layer F.Cu) (tedit 5D0822D2)
    (at 101.6 76.20762)
    (fp_text reference U1 (at 7.62 -1.016) (layer F.SilkS) hide)
    (fp_text value 27C400 (at 7.62 -1.016) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 38 /A17))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 1 /A7))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 2 /A6))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 3 /A5))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 4 /A4))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 5 /A3))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 6 /A2))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 7 /A1))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 8 /A0))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 9 /CE#))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 10 /GND))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 11 /OE#))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 12 /Q0))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 13 /Q8))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 14 /Q1))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 15 /Q9))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 16 /Q2))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 17 /Q10))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 18 /Q3))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 19 /Q11))
    (pad 21 thru_hole circle (at 15.24 48.26) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 20 /VCC))
    (pad 22 thru_hole circle (at 15.24 45.72) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 21 /Q4))
    (pad 23 thru_hole circle (at 15.24 43.18) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 22 /Q12))
    (pad 24 thru_hole circle (at 15.24 40.64) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 23 /Q5))
    (pad 25 thru_hole circle (at 15.24 38.1) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 24 /Q13))
    (pad 26 thru_hole circle (at 15.24 35.56) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 25 /Q6))
    (pad 27 thru_hole circle (at 15.24 33.02) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 26 /Q14))
    (pad 28 thru_hole circle (at 15.24 30.48) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 27 /Q7))
    (pad 29 thru_hole circle (at 15.24 27.94) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 28 /Q15))
    (pad 30 thru_hole circle (at 15.24 25.4) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 10 /GND))
    (pad 31 thru_hole circle (at 15.24 22.86) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 39 /PIN31))
    (pad 32 thru_hole circle (at 15.24 20.32) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 29 /A16))
    (pad 33 thru_hole circle (at 15.24 17.78) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 30 /A15))
    (pad 34 thru_hole circle (at 15.24 15.24) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 37 /A14))
    (pad 35 thru_hole circle (at 15.24 12.7) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 31 /A13))
    (pad 36 thru_hole circle (at 15.24 10.16) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 32 /A12))
    (pad 37 thru_hole circle (at 15.24 7.62) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 33 /A11))
    (pad 38 thru_hole circle (at 15.24 5.08) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 34 /A10))
    (pad 39 thru_hole circle (at 15.24 2.54) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 35 /A9))
    (pad 40 thru_hole circle (at 15.24 0) (size 1.016 1.016) (drill 0.635) (layers *.Cu *.Mask)
      (net 36 /A8))
  )
  (module AmigaRomAdapter2:SkinnyDip40 (layer F.Cu) (tedit 5D08282C)
    (at 102.87 74.93)
    (fp_text reference U2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 27C4096 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 20 /VCC))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 9 /CE#))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 28 /Q15))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 26 /Q14))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 24 /Q13))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 22 /Q12))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 19 /Q11))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 17 /Q10))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 15 /Q9))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 13 /Q8))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 10 /GND))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 27 /Q7))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 25 /Q6))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 23 /Q5))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 21 /Q4))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 18 /Q3))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 16 /Q2))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 14 /Q1))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 12 /Q0))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 11 /OE#))
    (pad 21 thru_hole circle (at 15.24 48.26) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 8 /A0))
    (pad 22 thru_hole circle (at 15.24 45.72) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 7 /A1))
    (pad 23 thru_hole circle (at 15.24 43.18) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 6 /A2))
    (pad 24 thru_hole circle (at 15.24 40.64) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 5 /A3))
    (pad 25 thru_hole circle (at 15.24 38.1) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 4 /A4))
    (pad 26 thru_hole circle (at 15.24 35.56) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 3 /A5))
    (pad 27 thru_hole circle (at 15.24 33.02) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 2 /A6))
    (pad 28 thru_hole circle (at 15.24 30.48) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 1 /A7))
    (pad 29 thru_hole circle (at 15.24 27.94) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 36 /A8))
    (pad 30 thru_hole circle (at 15.24 25.4) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 10 /GND))
    (pad 31 thru_hole circle (at 15.24 22.86) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 35 /A9))
    (pad 32 thru_hole circle (at 15.24 20.32) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 34 /A10))
    (pad 33 thru_hole circle (at 15.24 17.78) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 33 /A11))
    (pad 34 thru_hole circle (at 15.24 15.24) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 32 /A12))
    (pad 35 thru_hole circle (at 15.24 12.7) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 31 /A13))
    (pad 36 thru_hole circle (at 15.24 10.16) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 37 /A14))
    (pad 37 thru_hole circle (at 15.24 7.62) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 30 /A15))
    (pad 38 thru_hole circle (at 15.24 5.08) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 29 /A16))
    (pad 39 thru_hole circle (at 15.24 2.54) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 38 /A17))
    (pad 40 thru_hole circle (at 15.24 0) (size 1.0414 1.0414) (drill 0.7874) (layers *.Cu *.Mask)
      (net 20 /VCC))
  )
  (dimension 51.6 (width 0.15) (layer Dwgs.User)
    (gr_text "51.600 mm" (at 97.9 99.7 90) (layer Dwgs.User))
    (feature1 (pts (xy 100.4 73.9) (xy 98.613579 73.9)))
    (feature2 (pts (xy 100.4 125.5) (xy 98.613579 125.5)))
    (crossbar (pts (xy 99.2 125.5) (xy 99.2 73.9)))
    (arrow1a (pts (xy 99.2 73.9) (xy 99.786421 75.026504)))
    (arrow1b (pts (xy 99.2 73.9) (xy 98.613579 75.026504)))
    (arrow2a (pts (xy 99.2 125.5) (xy 99.786421 124.373496)))
    (arrow2b (pts (xy 99.2 125.5) (xy 98.613579 124.373496)))
  )
  (gr_line (start 100.6 75.2) (end 101.8 73.9) (layer Edge.Cuts) (width 0.15))
  (dimension 3.3 (width 0.15) (layer Dwgs.User)
    (gr_text "3.300 mm" (at 118.45 67.8) (layer Dwgs.User))
    (feature1 (pts (xy 120.1 71.1) (xy 120.1 68.513579)))
    (feature2 (pts (xy 116.8 71.1) (xy 116.8 68.513579)))
    (crossbar (pts (xy 116.8 69.1) (xy 120.1 69.1)))
    (arrow1a (pts (xy 120.1 69.1) (xy 118.973496 69.686421)))
    (arrow1b (pts (xy 120.1 69.1) (xy 118.973496 68.513579)))
    (arrow2a (pts (xy 116.8 69.1) (xy 117.926504 69.686421)))
    (arrow2b (pts (xy 116.8 69.1) (xy 117.926504 68.513579)))
  )
  (dimension 18.4 (width 0.15) (layer Dwgs.User)
    (gr_text "18.400 mm" (at 109.8 128.414213) (layer Dwgs.User))
    (feature1 (pts (xy 119 125.7) (xy 119 127.700634)))
    (feature2 (pts (xy 100.6 125.7) (xy 100.6 127.700634)))
    (crossbar (pts (xy 100.6 127.114213) (xy 119 127.114213)))
    (arrow1a (pts (xy 119 127.114213) (xy 117.873496 127.700634)))
    (arrow1b (pts (xy 119 127.114213) (xy 117.873496 126.527792)))
    (arrow2a (pts (xy 100.6 127.114213) (xy 101.726504 127.700634)))
    (arrow2b (pts (xy 100.6 127.114213) (xy 101.726504 126.527792)))
  )
  (gr_text "27C4096\nADAPTER\n(C) 2019 ES" (at 110.1 117.8 90) (layer F.SilkS))
  (gr_text "1-2: A500 6, A2000 4+\n2-3: OLD" (at 111.8 95.4 90) (layer F.SilkS))
  (gr_line (start 119 73.9) (end 101.8 73.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 125.5) (end 119 73.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.6 125.5) (end 119 125.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.6 75.2) (end 100.6 125.5) (layer Edge.Cuts) (width 0.15))
)
