(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 10)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad3)")
  (net 3 "Net-(D1-Pad4)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(J2-Pad2)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EC1E517)
    (at 124.46 76.2)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EC1E4EC)
    (at 116.84 78.74 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 120.65 79.629 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value R_Small_US (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-PLCC4_3.2x2.8mm_CCW (layer F.Cu) (tedit 59D415EA)
    (at 120.65 76.2 180)
    (descr "3.2mm x 2.8mm PLCC4 LED, http://www.cree.com/led-components/media/documents/CLV1AFKB(874).pdf")
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference D1 (at 0 -2.65) (layer F.SilkS) hide)
    (fp_text value CLV1L-FKB (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -1.25 0.7 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 1.25 0.7 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 1.25 -0.7 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at -1.25 -0.7 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-PLCC4_3.2x2.8mm_CCW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 0805 (at 120.65 79.375) (layer B.SilkS))
  (gr_text PLCC4 (at 120.65 76.2) (layer B.SilkS))
  (gr_line (start 114.935 80.645) (end 114.935 74.295) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.365 80.645) (end 114.935 80.645) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.365 74.295) (end 126.365 80.645) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.935 74.295) (end 126.365 74.295) (layer Edge.Cuts) (width 0.05))
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 128.27 69.88) (layer Dwgs.User))
    (feature1 (pts (xy 129.54 68.58) (xy 129.54 69.166421)))
    (feature2 (pts (xy 127 68.58) (xy 127 69.166421)))
    (crossbar (pts (xy 127 68.58) (xy 129.54 68.58)))
    (arrow1a (pts (xy 129.54 68.58) (xy 128.413496 69.166421)))
    (arrow1b (pts (xy 129.54 68.58) (xy 128.413496 67.993579)))
    (arrow2a (pts (xy 127 68.58) (xy 128.126504 69.166421)))
    (arrow2b (pts (xy 127 68.58) (xy 128.126504 67.993579)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 123.19 69.88) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 68.58) (xy 124.46 69.166421)))
    (feature2 (pts (xy 121.92 68.58) (xy 121.92 69.166421)))
    (crossbar (pts (xy 121.92 68.58) (xy 124.46 68.58)))
    (arrow1a (pts (xy 124.46 68.58) (xy 123.333496 69.166421)))
    (arrow1b (pts (xy 124.46 68.58) (xy 123.333496 67.993579)))
    (arrow2a (pts (xy 121.92 68.58) (xy 123.046504 69.166421)))
    (arrow2b (pts (xy 121.92 68.58) (xy 123.046504 67.993579)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 118.11 69.88) (layer Dwgs.User))
    (feature1 (pts (xy 119.38 68.58) (xy 119.38 69.166421)))
    (feature2 (pts (xy 116.84 68.58) (xy 116.84 69.166421)))
    (crossbar (pts (xy 116.84 68.58) (xy 119.38 68.58)))
    (arrow1a (pts (xy 119.38 68.58) (xy 118.253496 69.166421)))
    (arrow1b (pts (xy 119.38 68.58) (xy 118.253496 67.993579)))
    (arrow2a (pts (xy 116.84 68.58) (xy 117.966504 69.166421)))
    (arrow2b (pts (xy 116.84 68.58) (xy 117.966504 67.993579)))
  )
)
