(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 731)
    (zones 0)
    (modules 43)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VIO)
  (net 3 /VDMX)
  (net 4 /DMX1GND)
  (net 5 /DMX512_1/DMXVCC)
  (net 6 /DMX512_2/DMXVCC)
  (net 7 /DMX2GND)
  (net 8 /DMX3GND)
  (net 9 /sheet5D7E7BD5/DMXVCC)
  (net 10 /sheet5D7E7C11/DMXVCC)
  (net 11 /DMX4GND)
  (net 12 /DMX1P)
  (net 13 /DMX1N)
  (net 14 /DMX2N)
  (net 15 /DMX2P)
  (net 16 /DMX3P)
  (net 17 /DMX3N)
  (net 18 /DMX4N)
  (net 19 /DMX4P)
  (net 20 /DMX1_TXEN)
  (net 21 /DMX1_TX)
  (net 22 /DMX1_RX)
  (net 23 /DMX2_TXEN)
  (net 24 /DMX2_TX)
  (net 25 /DMX2_RX)
  (net 26 /DMX3_TXEN)
  (net 27 /DMX3_TX)
  (net 28 /DMX3_RX)
  (net 29 /DMX4_TXEN)
  (net 30 /DMX4_TX)
  (net 31 /DMX4_RX)
  (net 32 "Net-(C101-Pad1)")
  (net 33 "Net-(C102-Pad1)")
  (net 34 "Net-(C103-Pad1)")
  (net 35 "Net-(C104-Pad1)")
  (net 36 /IO_SDA)
  (net 37 /IO_SCL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DMX1GND)
    (add_net /DMX1N)
    (add_net /DMX1P)
    (add_net /DMX1_RX)
    (add_net /DMX1_TX)
    (add_net /DMX1_TXEN)
    (add_net /DMX2GND)
    (add_net /DMX2N)
    (add_net /DMX2P)
    (add_net /DMX2_RX)
    (add_net /DMX2_TX)
    (add_net /DMX2_TXEN)
    (add_net /DMX3GND)
    (add_net /DMX3N)
    (add_net /DMX3P)
    (add_net /DMX3_RX)
    (add_net /DMX3_TX)
    (add_net /DMX3_TXEN)
    (add_net /DMX4GND)
    (add_net /DMX4N)
    (add_net /DMX4P)
    (add_net /DMX4_RX)
    (add_net /DMX4_TX)
    (add_net /DMX4_TXEN)
    (add_net /DMX512_1/DMXVCC)
    (add_net /DMX512_2/DMXVCC)
    (add_net /IO_SCL)
    (add_net /IO_SDA)
    (add_net /VDMX)
    (add_net /VIO)
    (add_net /sheet5D7E7BD5/DMXVCC)
    (add_net /sheet5D7E7C11/DMXVCC)
    (add_net GND)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C104-Pad1)")
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 117.25172 48.98136)
    (fp_text reference X2 (at -8.42542 20.56638) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 "Net-(C101-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 /DMX1P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 /DMX1N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /DMX1GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 141.25172 48.98136)
    (fp_text reference X3 (at -7.83314 20.16252) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(C102-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /DMX2P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 /DMX2N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 /DMX2GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 165.25172 48.98136)
    (fp_text reference X4 (at 11.29098 20.12696) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "Net-(C103-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 /DMX3P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 /DMX3N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 8 /DMX3GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 189.25172 48.93564)
    (fp_text reference X5 (at -8.86346 20.17268) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(C104-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 /DMX4P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /DMX4N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 /DMX4GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.96848 80.99298 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C303 (at -2.14376 -0.54864 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 112.19852 80.5434 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U203 (at 1 -3 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DMX1GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DMX512_1/DMXVCC))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 135.19852 80.5434 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U303 (at 2.78832 -3.02768 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DMX2GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 158.19852 80.5434 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U403 (at 2.04186 10.51052 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 /sheet5D7E7BD5/DMXVCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DMX3GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 181.19852 80.5434 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U503 (at 1 -3 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 /sheet5D7E7C11/DMXVCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 /DMX4GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 122.37884 77.16012 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U201 (at -7.00532 3.12764 180) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /DMX512_1/DMXVCC))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DMX1GND))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /DMX1P))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /DMX1N))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /DMX1N))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /DMX1P))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DMX1GND))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /DMX1_TX))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /DMX1_TXEN))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /DMX1_TXEN))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /DMX1_RX))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 145.37884 77.16012 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U301 (at -0.05334 6.34298 90) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /DMX2_RX))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /DMX2_TXEN))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /DMX2_TXEN))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /DMX2_TX))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DMX2GND))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /DMX2P))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /DMX2N))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /DMX2N))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /DMX2P))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DMX2GND))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 168.37884 77.48016 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -6.52018 1.66908 180) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /sheet5D7E7BD5/DMXVCC))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DMX3GND))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /DMX3P))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /DMX3N))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /DMX3N))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /DMX3P))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DMX3GND))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /DMX3_TX))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /DMX3_TXEN))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /DMX3_TXEN))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /DMX3_RX))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 191.37884 77.16012 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U501 (at -6.8453 1.68402 180) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /DMX4_RX))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /DMX4_TXEN))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /DMX4_TXEN))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /DMX4_TX))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /DMX4GND))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /DMX4P))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /DMX4N))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /DMX4N))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /DMX4P))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /DMX4GND))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /sheet5D7E7C11/DMXVCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at 3.68554 -0.5083 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C202 (at -2.1336 -0.26252) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /DMX512_1/DMXVCC))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at -2.08026 -0.71628) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C302 (at -2.13868 -0.31556) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C401 (at -2.00152 -0.8506) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 161.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C402 (at -2.1336 -0.26954) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DMX3GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /sheet5D7E7BD5/DMXVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 3.40868 -0.50486 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at -2.07518 -0.29972) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /sheet5D7E7C11/DMXVCC))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DMX4GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.25464 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R211 (at 1.26656 1.47828 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /DMX512_1/DMXVCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /DMX1P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.45504 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R212 (at 0.12356 1.38176 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /DMX1P))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /DMX1N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.54368 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R213 (at -2.00242 1.41224 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /DMX1N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.25464 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R311 (at 1.14748 1.4732 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /DMX2P))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.45504 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R312 (at 0.0502 1.4224 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /DMX2N))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /DMX2P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.54368 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R313 (at -1.33918 1.3462 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /DMX2N))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 165.25464 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R411 (at 1.40432 1.4224 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /DMX3P))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /sheet5D7E7BD5/DMXVCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.45504 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R412 (at 0.20544 1.397 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /DMX3N))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /DMX3P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 171.54368 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R413 (at -1.28554 1.4224 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /DMX3N))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DMX3GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.25464 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 1.11506 1.45288 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /sheet5D7E7C11/DMXVCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /DMX4P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 191.45504 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R512 (at -0.00762 1.42748 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /DMX4P))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /DMX4N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 194.54368 70.61708 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R513 (at -1.35382 1.37414 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DMX4GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /DMX4N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.5027 84.33816)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C203 (at 0.13562 1.86944) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 161.96564 81.3816 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C403 (at -2.96164 3.09118) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 187.5027 84.33816)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at -0.14214 1.78816) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 107.8103 62.1561 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C101-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.0579 62.0418 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 156.39034 63.59168 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C103 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C103-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DMX3GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 179.4383 62.6364 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C104 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DMX4GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:TE_2-84952-2_1x22-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5AEE14E3)
    (at 151.14778 86.76132)
    (descr "TE FPC connector, 22 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
    (tags "te fpc 84952")
    (attr smd)
    (fp_text reference X1 (at 0 -4) (layer F.SilkS))
    (fp_text value Conn_01x22_MountingPin (at 0 7.7) (layer F.Fab))
    (fp_text user %R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -10.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -9.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 22 /DMX1_RX))
    (pad 3 smd rect (at -8.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 20 /DMX1_TXEN))
    (pad 4 smd rect (at -7.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /DMX1_TX))
    (pad 5 smd rect (at -6.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 25 /DMX2_RX))
    (pad 7 smd rect (at -4.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 23 /DMX2_TXEN))
    (pad 8 smd rect (at -3.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 24 /DMX2_TX))
    (pad 9 smd rect (at -2.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 28 /DMX3_RX))
    (pad 11 smd rect (at -0.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 26 /DMX3_TXEN))
    (pad 12 smd rect (at 0.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 27 /DMX3_TX))
    (pad 13 smd rect (at 1.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /DMX4_RX))
    (pad 15 smd rect (at 3.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 29 /DMX4_TXEN))
    (pad 16 smd rect (at 4.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 30 /DMX4_TX))
    (pad 17 smd rect (at 5.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 6.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 36 /IO_SDA))
    (pad 19 smd rect (at 7.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 37 /IO_SCL))
    (pad 20 smd rect (at 8.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (pad 21 smd rect (at 9.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDMX))
    (pad 22 smd rect (at 10.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDMX))
    (pad MP smd rect (at -13.49 1) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad MP smd rect (at 13.49 1) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_2-84952-2_1x22-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.53178 83.97748 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R101 (at -0.08128 -3.00736 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /IO_SDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.53178 85.50656 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R102 (at -0.08128 -2.74574 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /IO_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DmxIO4-v1.0 (at 189.23 87.64524) (layer F.Mask))
  (gr_text llg.cubic.org (at 173.83252 87.74684) (layer F.Mask))
  (gr_line (start 106.31932 48.9712) (end 106.3244 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.2228 48.9712) (end 106.31932 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.2228 90.04046) (end 106.2228 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.866 90.04046) (end 106.2228 90.04046) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.866 48.9712) (end 197.866 90.04046) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.3244 48.9712) (end 197.866 48.9712) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.2736 77.3176) (xy 197.8152 77.3176) (xy 197.8152 90.00236) (xy 106.2736 90.00236)
      )
    )
  )
  (zone (net 4) (net_name /DMX1GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.31424 48.98136) (xy 106.30408 75.55484) (xy 128.6002 75.55484) (xy 128.6002 49.01184)
      )
    )
  )
  (zone (net 7) (net_name /DMX2GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.8674 49.07788) (xy 132.83184 75.67168) (xy 151.78532 75.67168) (xy 151.78532 49.01692)
      )
    )
  )
  (zone (net 8) (net_name /DMX3GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.9052 49.07788) (xy 155.86964 75.67168) (xy 174.82312 75.67168) (xy 174.82312 49.01692)
      )
    )
  )
  (zone (net 11) (net_name /DMX4GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.91252 49.07788) (xy 178.87696 75.67168) (xy 197.83044 75.67168) (xy 197.83044 49.01692)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.2736 77.3176) (xy 197.8152 77.3176) (xy 197.8152 90.00236) (xy 106.2736 90.00236)
      )
    )
  )
)
