(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Eurorack Mixer")
    (date "2022-12-22")
    (rev "1.0.1")
    (company "Len Popp")
    (comment 1 "Copyright © 2022 Len Popp CC BY")
    (comment 2 "Board settings comply with requirements of OSH Park https://oshpark.com/")
    (comment 3 "Eurorack 3:1 mixer module - 4HP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "GAIN")
  (net 3 "LED-RED")
  (net 4 "LED-GREEN")
  (net 5 "IN-1")
  (net 6 "IN-2")
  (net 7 "IN-3")
  (net 8 "OUT")
  (net 9 "IN-ATTEN-1")
  (net 10 "IN-ATTEN-2")
  (net 11 "IN-ATTEN-3")
  (net 12 "GAIN-ATTEN")
  (net 13 "unconnected-(J4-PadTN)")
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 130.72 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "Input 2")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 6 "IN-2") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 140.74 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "Input 3")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 7 "IN-3") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "LED_THT:LED_D5.0mm-3" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 133.18 113.175)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Kingbright/WP59SURKCGKW?qs=sGAEpiMZZMvHYEB9WUp7EhaldIk4dKK1HOS5sGoXrpo%3D")
    (property "DistributorPartNum" "604-WP59SURKCGKW")
    (property "Label" "Level")
    (property "Manufacturer" "Kingbright")
    (property "ManufacturerPartNum" "WP59SURKCGKW")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -2.37 0.109) (layer "F.SilkS"))
    (fp_text value "LED_Dual_5mm_ACA" (at 2.54 3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "LED-RED") (pinfunction "A1") (pintype "input"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "LED-GREEN") (pinfunction "A2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 133.18 106.68 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "Gain")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV4" (at -2.159 0.043 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 "GAIN-ATTEN") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GAIN") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 133.18 87.63 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "Input 3")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV3" (at -2.286 -0.084 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "IN-ATTEN-3") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "IN-3") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 140.74 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "Output")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 8 "OUT") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J4-PadTN)") (pintype "passive+no_connect"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 130.72 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "Input 1")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 5 "IN-1") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 133.18 68.58 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "Input 2")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV2" (at -2.286 -0.084 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "IN-ATTEN-2") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 "IN-2") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 133.18 49.53 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "Input 1")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.286 -0.084 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "IN-ATTEN-1") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "IN-1") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-misc:Logo_CC_BY" locked (layer "B.Cu")
    (tedit 0)
    (at 140.081 93.091 180)
    (attr through_hole)
    (fp_text reference "G2" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Logo_CC_BY" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "-lmp-misc:Logo_OSHW" locked (layer "B.Cu")
    (tedit 60F495A1)
    (at 131.572 92.964 180)
    (descr "Open Source Hardware logo")
    (tags "Open Source Hardware logo")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G4" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Logo_OSHW" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A431)
    (at 127 81.28 180)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (property "Distributor" "Adafruit")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.adafruit.com/product/598")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/Wurth-Elektronik/61303211821?qs=ZtY9WdtwX55M%2FH%2FSrHZ9xA%3D%3D")
    (property "DistributorPartNum" "598")
    (property "DistributorPartNum2" "710-61303211821")
    (property "Sheetfile" "Mixer1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 2.77) (layer "B.SilkS"))
    (fp_text value "Conn_PCB_Front" (at 0 -23.09) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -10.16 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "IN-ATTEN-1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "IN-ATTEN-2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "IN-ATTEN-3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GAIN") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "GAIN-ATTEN") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "LED-GREEN") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "LED-RED") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "OUT") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 145.730011 36.83) (end 145.730011 145.034) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 145.730011 145.034) (end 125.73 145.034) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 125.73 36.83) (end 145.730011 36.83) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 125.73 145.034) (end 125.73 36.83) (layer "Edge.Cuts") (width 0.1524))
  (gr_text "1Mix" (at 135.636 53.738) (layer "B.SilkS"))
  (gr_text "rev ${REVISION}" (at 135.636 56.642) (layer "B.SilkS"))
  (gr_text "© 2022 Len Popp" (at 135.636 73.787) (layer "B.SilkS"))
  (gr_text "https://len42.github.io/Synth/" (at 144.018 53.848 90) (layer "B.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.381) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 146.304 145.415)
        (xy 125.095 145.415)
        (xy 125.095 36.195)
        (xy 146.304 36.195)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.6534 126.2585)
        (xy 131.1169 126.1851)
        (xy 131.5351 125.972)
        (xy 131.8669 125.6402)
        (xy 132.08 125.222)
        (xy 132.1534 124.7585)
        (xy 132.08 124.295)
        (xy 131.8669 123.8768)
        (xy 131.5351 123.545)
        (xy 131.1169 123.3319)
        (xy 130.6534 123.2585)
        (xy 130.1899 123.3319)
        (xy 129.7717 123.545)
        (xy 129.4399 123.8768)
        (xy 129.2268 124.295)
        (xy 129.1534 124.7585)
        (xy 129.2268 125.222)
        (xy 129.4399 125.6402)
        (xy 129.7717 125.972)
        (xy 130.1899 126.1851)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.6534 140.312402)
        (xy 131.1169 140.239002)
        (xy 131.5351 140.025902)
        (xy 131.8669 139.694102)
        (xy 132.08 139.275902)
        (xy 132.1534 138.812402)
        (xy 132.08 138.348902)
        (xy 131.8669 137.930702)
        (xy 131.5351 137.598902)
        (xy 131.1169 137.385802)
        (xy 130.6534 137.312402)
        (xy 130.1899 137.385802)
        (xy 129.7717 137.598902)
        (xy 129.4399 137.930702)
        (xy 129.2268 138.348902)
        (xy 129.1534 138.812402)
        (xy 129.2268 139.275902)
        (xy 129.4399 139.694102)
        (xy 129.7717 140.025902)
        (xy 130.1899 140.239002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.74 126.341)
        (xy 141.2035 126.2676)
        (xy 141.6217 126.0545)
        (xy 141.9535 125.7227)
        (xy 142.1666 125.3045)
        (xy 142.24 124.841)
        (xy 142.1666 124.3775)
        (xy 141.9535 123.9593)
        (xy 141.6217 123.6275)
        (xy 141.2035 123.4144)
        (xy 140.74 123.341)
        (xy 140.2765 123.4144)
        (xy 139.8583 123.6275)
        (xy 139.5265 123.9593)
        (xy 139.3134 124.3775)
        (xy 139.24 124.841)
        (xy 139.3134 125.3045)
        (xy 139.5265 125.7227)
        (xy 139.8583 126.0545)
        (xy 140.2765 126.2676)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.74 140.311)
        (xy 141.2035 140.2376)
        (xy 141.6217 140.0245)
        (xy 141.9535 139.6927)
        (xy 142.1666 139.2745)
        (xy 142.24 138.811)
        (xy 142.1666 138.3475)
        (xy 141.9535 137.9293)
        (xy 141.6217 137.5975)
        (xy 141.2035 137.3844)
        (xy 140.74 137.311)
        (xy 140.2765 137.3844)
        (xy 139.8583 137.5975)
        (xy 139.5265 137.9293)
        (xy 139.3134 138.3475)
        (xy 139.24 138.811)
        (xy 139.3134 139.2745)
        (xy 139.5265 139.6927)
        (xy 139.8583 140.0245)
        (xy 140.2765 140.2376)
      )
    )
  )
)
