(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "PICSARR - Direct Drive")
    (date "6/3/2023")
    (rev "1.0")
    (company "UMBC AstroPol Designs")
  )
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" power)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-D1{slash}TX-Pad1)")
  (net 2 "unconnected-(A1-D0{slash}RX-Pad2)")
  (net 3 "unconnected-(A1-~{RESET}-Pad3)")
  (net 4 "GND")
  (net 5 "Net-(A1-D2)")
  (net 6 "Net-(A1-D3)")
  (net 7 "Net-(A1-D4)")
  (net 8 "Net-(A1-D5)")
  (net 9 "Net-(A1-D6)")
  (net 10 "Net-(A1-D7)")
  (net 11 "Net-(A1-D8)")
  (net 12 "unconnected-(A1-D9-Pad12)")
  (net 13 "unconnected-(A1-D10-Pad13)")
  (net 14 "unconnected-(A1-D11-Pad14)")
  (net 15 "unconnected-(A1-D12-Pad15)")
  (net 16 "unconnected-(A1-D13-Pad16)")
  (net 17 "unconnected-(A1-3V3-Pad17)")
  (net 18 "unconnected-(A1-AREF-Pad18)")
  (net 19 "unconnected-(A1-A0-Pad19)")
  (net 20 "unconnected-(A1-A1-Pad20)")
  (net 21 "unconnected-(A1-A2-Pad21)")
  (net 22 "unconnected-(A1-A3-Pad22)")
  (net 23 "unconnected-(A1-A4-Pad23)")
  (net 24 "unconnected-(A1-A5-Pad24)")
  (net 25 "unconnected-(A1-A6-Pad25)")
  (net 26 "unconnected-(A1-A7-Pad26)")
  (net 27 "+5V")
  (net 28 "unconnected-(A1-~{RESET}-Pad28)")
  (net 29 "unconnected-(A1-VIN-Pad30)")
  (net 30 "Net-(A2-1B)")
  (net 31 "Net-(A2-1A)")
  (net 32 "Net-(A2-2A)")
  (net 33 "Net-(A2-2B)")
  (net 34 "+24V")
  (net 35 "Net-(A2-~{RESET})")
  (net 36 "unconnected-(U1-Pad3)")
  (net 37 "unconnected-(U1-Pad4)")
  (net 38 "unconnected-(U1-Pad5)")
  (net 39 "unconnected-(U1-Pad6)")
  (net 40 "unconnected-(U1-Pad8)")
  (net 41 "unconnected-(U1-Pad9)")
  (net 42 "unconnected-(U1-Pad10)")
  (net 43 "unconnected-(U1-Pad11)")
  (net 44 "unconnected-(U1-Pad12)")
  (net 45 "unconnected-(U1-Pad13)")
  (net 46 "Net-(HE_Sensor1-Pin_3)")
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 122.3392 89.5808 -90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 8.81 0 -180) (layer "F.SilkS"))
    (fp_text value "470u" (at -3.89 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "+24V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 177.5292 74.5108)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Motor1" (at 2.54 3.81 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at -2.54 3.81 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(A2-2B)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(A2-2A)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(A2-1A)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(A2-1B)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (at 118.5292 130.5258)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (at 118.5292 67.5258)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Module:Pololu_Breakout-16_15.2x20.3mm" (layer "F.Cu")
    (at 149.6442 89.5808 -90)
    (descr "Pololu Breakout 16-pin 15.2x20.3mm 0.6x0.8\\")
    (tags "Pololu Breakout")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Pololu Breakout Board, Stepper Driver A4988")
    (property "ki_keywords" "Pololu Breakout Board Stepper Driver A4988")
    (attr through_hole)
    (fp_text reference "A2" (at 6.35 -2.54) (layer "F.SilkS"))
    (fp_text value "Pololu_Breakout_A4988" (at 6.35 20.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(A2-1B)") (pinfunction "1B") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(A2-1A)") (pinfunction "1A") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(A2-2A)") (pinfunction "2A") (pintype "output"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(A2-2B)") (pinfunction "2B") (pintype "output"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "+24V") (pinfunction "VMOT") (pintype "power_in"))
    (pad "9" thru_hole oval (at 12.7 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(A1-D8)") (pinfunction "~{ENABLE}") (pintype "input"))
    (pad "10" thru_hole oval (at 12.7 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(A1-D7)") (pinfunction "MS1") (pintype "input"))
    (pad "11" thru_hole oval (at 12.7 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(A1-D6)") (pinfunction "MS2") (pintype "input"))
    (pad "12" thru_hole oval (at 12.7 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(A1-D5)") (pinfunction "MS3") (pintype "input"))
    (pad "13" thru_hole oval (at 12.7 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(A2-~{RESET})") (pinfunction "~{RESET}") (pintype "input"))
    (pad "14" thru_hole oval (at 12.7 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(A2-~{RESET})") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "15" thru_hole oval (at 12.7 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(A1-D4)") (pinfunction "STEP") (pintype "input"))
    (pad "16" thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(A1-D3)") (pinfunction "DIR") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Pololu_Breakout-16_15.2x20.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (at 165.491 103.251)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Hex inverter schmitt trigger")
    (property "ki_keywords" "HCMOS not inverter")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.54) (layer "F.SilkS"))
    (fp_text value "74HC14" (at 3.81 17.78) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(HE_Sensor1-Pin_3)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(A1-D2)") (pintype "output"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U1-Pad3)") (pintype "input+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U1-Pad4)") (pintype "output+no_connect"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U1-Pad5)") (pintype "input+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U1-Pad6)") (pintype "output+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U1-Pad8)") (pintype "output+no_connect"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U1-Pad9)") (pintype "input+no_connect"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U1-Pad10)") (pintype "output+no_connect"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U1-Pad11)") (pintype "input+no_connect"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U1-Pad12)") (pintype "output+no_connect"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U1-Pad13)") (pintype "input+no_connect"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (at 177.5292 67.5258)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_BarrelJack:BarrelJack_GCT_DCJ200-10-A_Horizontal" (layer "F.Cu")
    (at 128.9312 76.8758 -90)
    (descr "Barrel jack connector (5.5 mm outer diameter, 2.05 inner diameter ), https://gct.co/files/drawings/dcj200-10.pdf")
    (tags "connector barrel jack")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "DC Barrel Jack with a mounting pin")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.5 -180) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at 0 15.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 4.6 2) (drill oval 3.6 1) (layers "*.Cu" "*.Mask")
      (net 34 "+24V") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6.3 270) (size 4.2 2) (drill oval 3.2 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (pad "3" thru_hole oval (at 4.8 2.9 270) (size 2 4.2) (drill oval 1 3.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_GCT_DCJ200-10-A_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 177.5842 103.251 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at -1.905 0) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 6.985 0 -180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Module:Arduino_Nano" (layer "F.Cu")
    (at 157.2642 109.2658 -90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Arduino Nano v3.x")
    (property "ki_keywords" "Arduino nano microcontroller module USB")
    (attr through_hole)
    (fp_text reference "A1" (at 7.62 -5.08) (layer "F.SilkS"))
    (fp_text value "Arduino_Nano_v3.x" (at 8.89 19.05) (layer "F.Fab"))
    (fp_text user "USB" (at 7.62 35.56 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.35 19.05) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(A1-D1{slash}TX-Pad1)") (pinfunction "D1/TX") (pintype "bidirectional+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(A1-D0{slash}RX-Pad2)") (pinfunction "D0/RX") (pintype "bidirectional+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(A1-~{RESET}-Pad3)") (pinfunction "~{RESET}") (pintype "input+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(A1-D2)") (pinfunction "D2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(A1-D3)") (pinfunction "D3") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(A1-D4)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(A1-D5)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(A1-D6)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(A1-D7)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(A1-D8)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(A1-D9-Pad12)") (pinfunction "D9") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(A1-D10-Pad13)") (pinfunction "D10") (pintype "bidirectional+no_connect"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(A1-D11-Pad14)") (pinfunction "D11") (pintype "bidirectional+no_connect"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(A1-D12-Pad15)") (pinfunction "D12") (pintype "bidirectional+no_connect"))
    (pad "16" thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(A1-D13-Pad16)") (pinfunction "D13") (pintype "bidirectional+no_connect"))
    (pad "17" thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(A1-3V3-Pad17)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "18" thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(A1-AREF-Pad18)") (pinfunction "AREF") (pintype "input+no_connect"))
    (pad "19" thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(A1-A0-Pad19)") (pinfunction "A0") (pintype "bidirectional+no_connect"))
    (pad "20" thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(A1-A1-Pad20)") (pinfunction "A1") (pintype "bidirectional+no_connect"))
    (pad "21" thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(A1-A2-Pad21)") (pinfunction "A2") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(A1-A3-Pad22)") (pinfunction "A3") (pintype "bidirectional+no_connect"))
    (pad "23" thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(A1-A4-Pad23)") (pinfunction "A4") (pintype "bidirectional+no_connect"))
    (pad "24" thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(A1-A5-Pad24)") (pinfunction "A5") (pintype "bidirectional+no_connect"))
    (pad "25" thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(A1-A6-Pad25)") (pinfunction "A6") (pintype "bidirectional+no_connect"))
    (pad "26" thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(A1-A7-Pad26)") (pinfunction "A7") (pintype "bidirectional+no_connect"))
    (pad "27" thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pinfunction "+5V") (pintype "power_out"))
    (pad "28" thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(A1-~{RESET}-Pad28)") (pinfunction "~{RESET}") (pintype "input+no_connect"))
    (pad "29" thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(A1-VIN-Pad30)") (pinfunction "VIN") (pintype "power_in+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P5.00mm" (layer "F.Cu")
    (at 168.021 130.175 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 7.747 0 180) (layer "F.SilkS"))
    (fp_text value "100u" (at 2.402651 -5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 177.5842 89.4458)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "HE_Sensor1" (at 2.54 2.54 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at -2.54 2.58 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(HE_Sensor1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 154.6842 84.1458 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -2.54 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.54 2.54) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (at 177.5292 130.5258)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 159.1692 101.0108 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 11.895 0 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(A1-D3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 155.9942 101.0108 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 11.895 0 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(A1-D4)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 171.8292 94.5258 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "PICSARR - DD PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 2.235 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 -2.21) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(HE_Sensor1-Pin_3)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 114.7192 130.5258) (end 114.7192 67.5258)
    (layer "Edge.Cuts"))
  (gr_line (start 118.5292 63.7158) (end 177.5292 63.7158)
    (layer "Edge.Cuts"))
  (gr_arc (start 177.5292 63.7158) (mid 180.223277 64.831723) (end 181.3392 67.5258)
    (layer "Edge.Cuts"))
  (gr_arc (start 118.5292 134.3358) (mid 115.835123 133.219877) (end 114.7192 130.5258)
    (layer "Edge.Cuts"))
  (gr_arc (start 181.339199 130.525799) (mid 180.223276 133.219876) (end 177.529199 134.335799)
    (layer "Edge.Cuts"))
  (gr_line (start 181.3392 67.5258) (end 181.339199 130.525799)
    (layer "Edge.Cuts"))
  (gr_line (start 177.529199 134.335799) (end 118.5292 134.3358)
    (layer "Edge.Cuts"))
  (gr_arc (start 114.7192 67.5258) (mid 115.835123 64.831723) (end 118.5292 63.7158)
    (layer "Edge.Cuts"))
  (gr_text "Arduino Nano" (at 143.2942 116.8858) (layer "F.SilkS"))
  (gr_text "PICSARR - Direct Drive" (at 148.0292 67.5258) (layer "F.SilkS"))
  (gr_text "REV 1.0" (at 148.0292 70.7008) (layer "F.SilkS"))
  (gr_text "UMBC - AstroPol Designs\n" (at 142.621 130.556) (layer "F.SilkS"))
  (gr_text "A4988" (at 140.7542 95.9308) (layer "F.SilkS"))
  (zone (net 4) (net_name "GND") (layer "B.Cu") (name "GND Plane") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.381) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.6096))
    (polygon
      (pts
        (xy 183.0532 61.9378)
        (xy 112.9492 61.8108)
        (xy 112.9492 136.1058)
        (xy 183.0532 136.2328)
      )
    )
  )
)
