<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="52.07" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="40.894" x2="0" y2="40.894" width="0" layer="20"/>
<wire x1="0" y1="40.894" x2="0" y2="0" width="0" layer="20"/>
<wire x1="52.07" y1="0" x2="54.61" y2="2.54" width="0" layer="20"/>
<wire x1="54.61" y1="2.54" x2="54.61" y2="10.16" width="0" layer="20"/>
<wire x1="54.61" y1="10.16" x2="15.24" y2="10.16" width="0" layer="20"/>
<wire x1="15.24" y1="10.16" x2="15.24" y2="30.48" width="0" layer="20"/>
<wire x1="15.24" y1="30.48" x2="54.61" y2="30.48" width="0" layer="20"/>
<wire x1="54.61" y1="30.48" x2="54.61" y2="37.084" width="0" layer="20"/>
<wire x1="54.61" y1="37.084" x2="50.8" y2="40.894" width="0" layer="20"/>
<wire x1="21" y1="23" x2="23" y2="25" width="0" layer="20"/>
<wire x1="23" y1="25" x2="43" y2="25" width="0" layer="20"/>
<wire x1="43" y1="25" x2="45" y2="23" width="0" layer="20"/>
<wire x1="45" y1="23" x2="45" y2="16" width="0" layer="20"/>
<wire x1="45" y1="16" x2="43" y2="14" width="0" layer="20"/>
<wire x1="43" y1="14" x2="23" y2="14" width="0" layer="20"/>
<wire x1="23" y1="14" x2="21" y2="16" width="0" layer="20"/>
<wire x1="21" y1="16" x2="21" y2="23" width="0" layer="20"/>
<text>TX</text>
<text>RX</text>
<text>BTN_1</text>
<text>BTN_2</text>
<text>BTN_3</text>
<text>GND</text>
<text>100Ω</text>
<text>  Only one of these
resistors are needed</text>
<text>5V</text>
<text>Blake Williams</text>
<text>LED_OUT</text>
<text>This side against TFT screen</text>
<text>GND</text>
<text>BTN_3</text>
<text>BTN_2</text>
<text>BTN_1</text>
</plain>
<libraries>
<library name="1teensy 4 adapter">
<packages>
<package name="TEENSY4">
</package>
<package name="TOUCH_SCREEN">
</package>
<package name="805_SMD">
</package>
<package name="805_VIA">
</package>
<package name="BUTTON">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="1teensy 4 adapter" package="TEENSY4" value="TEENSY4"/>
<element name="U$2" library="1teensy 4 adapter" package="TOUCH_SCREEN" value="TOUCH_SCREEN"/>
<element name="U$3" library="1teensy 4 adapter" package="805_SMD" value="RESISTORSMD"/>
<element name="U$4" library="1teensy 4 adapter" package="805_VIA" value="RESISTORVIA"/>
<element name="U$5" library="1teensy 4 adapter" package="BUTTON" value="BUTTON"/>
<element name="U$6" library="1teensy 4 adapter" package="BUTTON" value="BUTTON"/>
<element name="U$7" library="1teensy 4 adapter" package="BUTTON" value="BUTTON"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="S_SCK"/>
<contactref element="U$2" pad="S_SCK"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3_3V"/>
<contactref element="U$2" pad="S_RESET"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="S_MISO"/>
<contactref element="U$2" pad="S_MISO"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="S_MOSI"/>
<contactref element="U$2" pad="S_MOSI"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="S_DC"/>
<contactref element="U$2" pad="S_DC"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="S_CS"/>
<contactref element="U$2" pad="S_CS"/>
</signal>
<signal name="5V_PWR">
<contactref element="U$1" pad="5V_PWR"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$2" pad="5V"/>
</signal>
<signal name="LED_DATA">
<contactref element="U$1" pad="LED_OUT"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="RX"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="TX"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="T_CLK"/>
<contactref element="U$2" pad="T_CLK"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="T_CS"/>
<contactref element="U$2" pad="T_CS"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="T_IN"/>
<contactref element="U$2" pad="T_DIN"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="T_OUT"/>
<contactref element="U$2" pad="T_DO"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="T_IRQ"/>
<contactref element="U$2" pad="T_IRQ"/>
</signal>
<signal name="S_LED_PWR">
<contactref element="U$2" pad="LED"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="U$5" pad="2_2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="2_2"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$7" pad="2_2"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="BTN_2">
<contactref element="U$6" pad="1_1"/>
<contactref element="U$6" pad="1"/>
<contactref element="U$1" pad="BTN_2"/>
</signal>
<signal name="BTN_1">
<contactref element="U$5" pad="1_1"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$1" pad="BTN_1"/>
</signal>
<signal name="BTN_3">
<contactref element="U$7" pad="1_1"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$1" pad="BTN_3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
