(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6002)
    (drawings 6)
    (tracks 328)
    (zones 0)
    (modules 4)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.27)
    (user_trace_width 1.778)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (user_via 0.889 0.635)
    (user_via 1.016 0.762)
    (user_via 1.143 0.889)
    (user_via 1.27 1.016)
    (user_via 1.524 1.143)
    (user_via 1.778 1.27)
    (user_via 2.032 1.397)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /ML3_N)
  (net 2 GND)
  (net 3 /ML3_P)
  (net 4 /ML2_N)
  (net 5 /ML2_P)
  (net 6 /ML1_N)
  (net 7 /ML1_P)
  (net 8 /ML0_N)
  (net 9 /ML0_P)
  (net 10 /AUX_P)
  (net 11 /AUX_N)
  (net 12 /HPD)
  (net 13 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +3V3)
    (add_net /AUX_N)
    (add_net /AUX_P)
    (add_net /HPD)
    (add_net /ML0_N)
    (add_net /ML0_P)
    (add_net /ML1_N)
    (add_net /ML1_P)
    (add_net /ML2_N)
    (add_net /ML2_P)
    (add_net /ML3_N)
    (add_net /ML3_P)
    (add_net GND)
  )
  (module Custom_footprints:Displayport_male_PCB (layer F.Cu) (tedit 5F3DD7A0)
    (at 119.6 89.8 180)
    (zone_connect 0)
    (fp_text reference J1 (at 9.6 0.8) (layer F.SilkS))
    (fp_text value Conn_01x20_Male (at 0 -5.4) (layer F.Fab))
    (fp_text user 19 (at -4 2 180) (layer F.SilkS))
    (fp_text user 1 (at 5 2 180) (layer F.SilkS))
    (pad "" smd rect (at -8.5 0.5 180) (size 1.2 3) (layers B.Cu B.Paste B.Mask)
      (zone_connect 0))
    (pad "" smd rect (at 7.5 0.5 180) (size 1.2 3) (layers B.Cu B.Paste B.Mask)
      (zone_connect 0))
    (pad "" smd rect (at -8.5 0.5 180) (size 1.2 3) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad "" smd rect (at 7.5 0.5 180) (size 1.2 3) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 20 smd rect (at -4.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 13 +3V3) (zone_connect 0))
    (pad 19 smd rect (at -4 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 18 smd rect (at -3.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 12 /HPD) (zone_connect 0))
    (pad 17 smd rect (at -3 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /AUX_N) (zone_connect 0))
    (pad 16 smd rect (at -2.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 15 smd rect (at -2 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUX_P) (zone_connect 0))
    (pad 14 smd rect (at -1.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 13 smd rect (at -1 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 12 smd rect (at -0.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /ML3_N) (zone_connect 0))
    (pad 11 smd rect (at 0 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 10 smd rect (at 0.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /ML3_P) (zone_connect 0))
    (pad 9 smd rect (at 1 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /ML2_N) (zone_connect 0))
    (pad 8 smd rect (at 1.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 7 smd rect (at 2 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /ML2_P) (zone_connect 0))
    (pad 6 smd rect (at 2.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /ML1_N) (zone_connect 0))
    (pad 5 smd rect (at 3 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 4 smd rect (at 3.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /ML1_P) (zone_connect 0))
    (pad 3 smd rect (at 4 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /ML0_N) (zone_connect 0))
    (pad 2 smd rect (at 4.5 0 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 1 smd rect (at 5 0 180) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /ML0_P) (zone_connect 0))
  )
  (module "Mouser:20455-040E-12(IPEX)" (layer F.Cu) (tedit 5F308351)
    (at 114.85 79.756 180)
    (fp_text reference J2 (at 10.85 -2.244) (layer F.SilkS))
    (fp_text value Conn_01x40 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at -9.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -9.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -8.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /ML3_N))
    (pad 4 smd rect (at -8.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /ML3_P))
    (pad 5 smd rect (at -7.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -7.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /ML2_N))
    (pad 7 smd rect (at -6.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /ML2_P))
    (pad 8 smd rect (at -6.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -5.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /ML1_N))
    (pad 10 smd rect (at -5.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /ML1_P))
    (pad 11 smd rect (at -4.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -4.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /ML0_N))
    (pad 13 smd rect (at -3.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /ML0_P))
    (pad 14 smd rect (at -3.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -2.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUX_P))
    (pad 16 smd rect (at -2.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /AUX_N))
    (pad 17 smd rect (at -1.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at -1.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 19 smd rect (at -0.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 20 smd rect (at -0.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 21 smd rect (at 0.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 22 smd rect (at 0.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 1.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 1.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 2.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 2.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 3.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /HPD))
    (pad 28 smd rect (at 3.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 4.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 5.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 5.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 6.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 6.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 7.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 7.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 8.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 8.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 9.25 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 9.75 0 180) (size 0.25 0.9) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -10.75 0 180) (size 0.55 0.9) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 10.75 0 180) (size 0.55 0.9) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 11.35 2.82 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -11.35 2.82 180) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 111.5 84.3 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 107.8 84.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DP to eDP" (at 122 84.3) (layer F.SilkS))
  (gr_line (start 108 91) (end 102 85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129 75) (end 129 91) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102 75) (end 129 75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102 85) (end 102 75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129 91) (end 108 91) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 94) (xy 100 94) (xy 100 72) (xy 130 72)
      )
    )
  )
)
