(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 88)
    (tracks 816)
    (zones 0)
    (modules 38)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x01030_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "hog32a_svg"))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 RESET)
  (net 3 GND)
  (net 4 0)
  (net 5 +5V)
  (net 6 RTS)
  (net 7 DTR)
  (net 8 "Net-(J7-Pad1)")
  (net 9 25)
  (net 10 SAT_RING_INDICATOR)
  (net 11 SAT_NETWORK_AVAIL)
  (net 12 SAT_LION)
  (net 13 26)
  (net 14 "Net-(Q1-Pad2)")
  (net 15 "Net-(Q2-Pad2)")
  (net 16 +3V3)
  (net 17 32)
  (net 18 33)
  (net 19 27)
  (net 20 DIO2)
  (net 21 DIO1)
  (net 22 DIO0)
  (net 23 DIO4)
  (net 24 DIO3)
  (net 25 DIO5)
  (net 26 17)
  (net 27 16)
  (net 28 4)
  (net 29 15)
  (net 30 13)
  (net 31 34)
  (net 32 35)
  (net 33 RX0)
  (net 34 TX0)
  (net 35 22)
  (net 36 21)
  (net 37 19)
  (net 38 "Net-(C1-Pad1)")
  (net 39 VBUS)
  (net 40 12)
  (net 41 5:onewire)
  (net 42 18:DHT22)
  (net 43 23:SAT_SLEEP)
  (net 44 14:SCL)
  (net 45 2:SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 0)
    (add_net 12)
    (add_net 13)
    (add_net 14:SCL)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18:DHT22)
    (add_net 19)
    (add_net 21)
    (add_net 22)
    (add_net 23:SAT_SLEEP)
    (add_net 25)
    (add_net 26)
    (add_net 27)
    (add_net 2:SDA)
    (add_net 32)
    (add_net 33)
    (add_net 34)
    (add_net 35)
    (add_net 4)
    (add_net 5:onewire)
    (add_net DIO0)
    (add_net DIO1)
    (add_net DIO2)
    (add_net DIO3)
    (add_net DIO4)
    (add_net DIO5)
    (add_net DTR)
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net RESET)
    (add_net RTS)
    (add_net RX0)
    (add_net SAT_LION)
    (add_net SAT_NETWORK_AVAIL)
    (add_net SAT_RING_INDICATOR)
    (add_net TX0)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net VBUS)
    (add_net VIN)
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow placed (layer F.Cu) (tedit 5BABA2E1)
    (at 96.33712 76.08316 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 3.65252 -4.20624 180) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 3.6322 -4.20624 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 RESET))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 RTS))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module zom:ESP32-WROOM placed (layer F.Cu) (tedit 5BABA324)
    (at 107.315 43.18 180)
    (fp_text reference U1 (at -7.493 8.71728 180) (layer F.SilkS))
    (fp_text value ESP32-WROOM (at 5.715 14.224 180) (layer F.Fab))
    (fp_text user "Espressif Systems" (at -6.858 -0.889 270) (layer F.SilkS))
    (fp_text user ESP32-WROOM (at -5.207 0.254 270) (layer F.SilkS))
    (pad 38 smd oval (at -9 5.25 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 37 smd oval (at -9 3.98 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 23:SAT_SLEEP))
    (pad 36 smd oval (at -9 2.71 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 22))
    (pad 35 smd oval (at -9 1.44 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 TX0))
    (pad 34 smd oval (at -9 0.17 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 RX0))
    (pad 33 smd oval (at -9 -1.1 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 21))
    (pad 32 smd oval (at -9 -2.37 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd oval (at -9 -3.64 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 19))
    (pad 30 smd oval (at -9 -4.91 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 18:DHT22))
    (pad 29 smd oval (at -9 -6.18 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 5:onewire))
    (pad 28 smd oval (at -9 -7.45 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 17))
    (pad 27 smd oval (at -9 -8.72 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 16))
    (pad 26 smd oval (at -9 -9.99 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 4))
    (pad 25 smd oval (at -9 -11.26 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 0))
    (pad 24 smd oval (at -5.715 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 45 2:SDA))
    (pad 23 smd oval (at -4.445 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 15))
    (pad 22 smd oval (at -3.175 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd oval (at -1.905 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd oval (at -0.635 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd oval (at 0.635 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd oval (at 1.905 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd oval (at 3.175 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd oval (at 4.445 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 13))
    (pad 15 smd oval (at 5.715 -12.75 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd oval (at 9 -11.26 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 12))
    (pad 13 smd oval (at 9 -9.99 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 14:SCL))
    (pad 12 smd oval (at 9 -8.72 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 27))
    (pad 11 smd oval (at 9 -7.45 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 26))
    (pad 10 smd oval (at 9 -6.18 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 25))
    (pad 9 smd oval (at 9 -4.91 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 33))
    (pad 8 smd oval (at 9 -3.64 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 32))
    (pad 7 smd oval (at 9 -2.37 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 35))
    (pad 6 smd oval (at 9 -1.1 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 34))
    (pad 5 smd oval (at 9 0.17 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at 9 1.44 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd oval (at 9 2.71 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 RESET))
    (pad 2 smd oval (at 9 3.98 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 +3V3))
    (pad 1 smd oval (at 9 5.25 180) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 39 smd rect (at 0.3 -2.45 180) (size 6 6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5BABA820)
    (at 118.11 59.055 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at -2.0574 -0.11684) (layer F.SilkS))
    (fp_text value 4.7K (at 0.95 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 18:DHT22))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module zom:RFM95 placed (layer F.Cu) (tedit 5BABA340)
    (at 74.93 52.07 90)
    (fp_text reference U2 (at 12.32916 1.3462 180) (layer F.SilkS))
    (fp_text value RFM95HW (at 13.5 -1.8 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd oval (at 0 2 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 17 32))
    (pad 3 smd oval (at 0 4 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 18 33))
    (pad 4 smd oval (at 0 6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 25))
    (pad 5 smd oval (at 0 8 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 13 26))
    (pad 6 smd oval (at 0 10 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 19 27))
    (pad 7 smd oval (at 0 12 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 25 DIO5))
    (pad 8 smd oval (at 0 14 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd oval (at 16 14 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J7-Pad1)"))
    (pad 10 smd oval (at 16 12 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 11 smd oval (at 16 10 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 24 DIO3))
    (pad 12 smd oval (at 16 8 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 23 DIO4))
    (pad 13 smd oval (at 16 6 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 16 +3V3))
    (pad 14 smd oval (at 16 4 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 22 DIO0))
    (pad 15 smd oval (at 16 2 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 21 DIO1))
    (pad 16 smd oval (at 16 0 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 20 DIO2))
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm placed (layer F.Cu) (tedit 5BABA3A1)
    (at 114.3 95.25 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at -0.12192 17.4244 180) (layer F.SilkS))
    (fp_text value prog (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 VBUS))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 RX0))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 TX0))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 RTS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 DTR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm placed (layer F.Cu) (tedit 5BABD818)
    (at 106.045 95.25 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J4 (at 0.3048 17.7292 90) (layer F.SilkS))
    (fp_text value sdcard (at 0 17.57 270) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 15))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 4))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 16))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 17))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm placed (layer F.Cu) (tedit 5BABA80D)
    (at 100.33 60.325 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0.1016 10.22096 270) (layer F.SilkS))
    (fp_text value i2c-a (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 2:SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 14:SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm placed (layer F.Cu) (tedit 5BABA373)
    (at 112.6998 100.0506 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 2.96672 -0.56896) (layer F.SilkS))
    (fp_text value REG:5V (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm placed (layer F.Cu) (tedit 5BABD2CC)
    (at 92.075 36.83)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 1.13284 -2.60096) (layer F.SilkS))
    (fp_text value ANT (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm placed (layer F.Cu) (tedit 5BABA816)
    (at 114.3 59.255 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J12 (at -0.1238 10.47496) (layer F.SilkS))
    (fp_text value dht22 (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 18:DHT22))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm placed (layer F.Cu) (tedit 59650532)
    (at 79.375 90.805)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J14 (at 0 -2.33) (layer F.SilkS))
    (fp_text value satx (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SAT_RING_INDICATOR))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SAT_NETWORK_AVAIL))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 23:SAT_SLEEP))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SAT_LION))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow placed (layer F.Cu) (tedit 5BABA2D6)
    (at 96.22536 70.21576 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.3462 3.2258 180) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.3462 3.1496 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 0))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 DTR))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm placed (layer F.Cu) (tedit 5BABA838)
    (at 107.75 71.12)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 8.64804 2.11328 90) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 RESET))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 RESET))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm placed (layer F.Cu) (tedit 5BABA83C)
    (at 114.3 67.31 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at -2.25044 2.0066 270) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 180) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 0))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 104.14 74.295 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.11 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.11 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 RESET))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BABA2A7)
    (at 104.775 62.23 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C4 (at 1.00584 1.97612 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.11 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 0))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BABD812)
    (at 109.78896 93.31452 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C5 (at -0.39116 1.76784 270) (layer F.SilkS))
    (fp_text value "10 uF" (at 1.25 2.11 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BABD804)
    (at 108.03636 90.2208 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C6 (at 4.37896 0.00508 90) (layer F.SilkS))
    (fp_text value "22 uF" (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BABE0E7)
    (at 82.55 99.06 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at -1.79832 -0.01524) (layer F.SilkS))
    (fp_text value "10 uF" (at 1.25 2.11 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BABE0DA)
    (at 80.01 104.775)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 0.03048 -1.81356) (layer F.SilkS))
    (fp_text value "22 uF" (at 1.25 2.11) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 100.33 78.105 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 0.95 -1.86 90) (layer F.SilkS))
    (fp_text value 10K (at 0.95 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 RESET))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5BABA2EF)
    (at 89.535 73.66 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 0.8636 2.2098) (layer F.SilkS))
    (fp_text value 10K (at 0.95 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 RTS))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 87.63 69.85)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 0.95 -1.86) (layer F.SilkS))
    (fp_text value 10K (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 DTR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 102.235 67.945)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 0.95 -1.86) (layer F.SilkS))
    (fp_text value 10K (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 0))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5BABA2B9)
    (at 97.155 63.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 0.94996 1.97104) (layer F.SilkS))
    (fp_text value 4.7K (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 2:SDA))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5BABA2B0)
    (at 92.71 63.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 1.016 2.23012) (layer F.SilkS))
    (fp_text value 4.7K (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 14:SCL))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5BABA38A)
    (at 92.51188 100.05568 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.56032 -1.0414) (layer F.SilkS))
    (fp_text value REG:3V3 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 2.56032 -1.02108) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_2pol (layer F.Cu) (tedit 5BABA37B)
    (at 98.43008 100.56368)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J3 (at 4.2926 2.2098) (layer F.SilkS))
    (fp_text value VINS (at 1.75 6) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_3pol (layer F.Cu) (tedit 5BABA36B)
    (at 119.68 86.36 90)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J9 (at 4.71932 2.30604 180) (layer F.SilkS))
    (fp_text value 1wire (at 3.5 6 90) (layer F.Fab))
    (fp_text user %R (at 3.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 5:onewire))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 75.065 66.06)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J13 (at 0 -2.33) (layer F.SilkS))
    (fp_text value 9602-a (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0.19) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 34))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 13))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5BABE0F1)
    (at 75.08 83.185)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J19 (at -0.83072 20.9296 270) (layer F.SilkS))
    (fp_text value 9602-b (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -0.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SAT_RING_INDICATOR))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SAT_NETWORK_AVAIL))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 23:SAT_SLEEP))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SAT_LION))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5BABD74F)
    (at 105.22204 79.26832)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at -1.86436 0.13208 90) (layer F.SilkS))
    (fp_text value R (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 41 5:onewire))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5BABA33A)
    (at 75.565 58.42 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J16 (at 1.31064 8.509 180) (layer F.SilkS))
    (fp_text value LBO (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 33))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 32))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 26))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 25))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 DIO5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 27))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BABA2F8)
    (at 101.8794 84.92744)
    (descr "D, DO-201 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf")
    (tags "D DO-201 series Axial Vertical pin pitch 5.08mm  length 9.53mm diameter 5.21mm")
    (fp_text reference D1 (at 3.4036 -2.1336) (layer F.SilkS))
    (fp_text value D (at 2.54 3.665) (layer F.Fab))
    (fp_text user K (at -3.365 0) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 VBUS))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BABA31A)
    (at 84.836 94.234 90)
    (descr "D, DO-201 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf")
    (tags "D DO-201 series Axial Vertical pin pitch 5.08mm  length 9.53mm diameter 5.21mm")
    (fp_text reference D2 (at 7.6454 0.02032 180) (layer F.SilkS))
    (fp_text value D (at 2.54 3.665 90) (layer F.Fab))
    (fp_text user K (at -3.365 0 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 5BABA333)
    (at 75.0189 32.6898 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J10 (at 0.1778 18.61566 180) (layer F.SilkS))
    (fp_text value Conn_01x07 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 DIO2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 DIO1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 DIO0))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 DIO4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 DIO3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 122.2248 37.0332)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x16 (at 0 40.43) (layer F.Fab))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 35))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 23:SAT_SLEEP))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 22))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 21))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 19))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 18:DHT22))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 5:onewire))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 0))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 14:SCL))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 12))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 2:SDA))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_5pol (layer F.Cu) (tedit 5BABA397)
    (at 119.6721 104.5464 90)
    (descr "5-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J15 (at 4.8006 -2.05486 270) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 7 6 90) (layer F.Fab))
    (fp_text user %R (at 7 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 +3V3))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 21))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 19))
    (pad 5 thru_hole circle (at 14 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_5pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2 (at 100.41128 58.00852) (layer F.SilkS))
  (gr_text 14 (at 97.78492 57.99836) (layer F.SilkS))
  (gr_text GND (at 95.26524 58.02884) (layer F.SilkS))
  (gr_text 3V3 (at 92.63888 58.01868) (layer F.SilkS))
  (gr_circle (center 120.14708 32.84728) (end 121.39676 33.71596) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 76.6826 104.18064) (end 77.93228 105.04932) (layer Edge.Cuts) (width 0.15))
  (gr_text 27 (at 80.68564 53.68544) (layer F.SilkS))
  (gr_text 25 (at 77.96276 53.63972) (layer F.SilkS))
  (gr_text 32 (at 75.65644 53.721) (layer F.SilkS))
  (gr_text DIO5 (at 80.98536 61.17336) (layer F.SilkS))
  (gr_text 26 (at 78.17104 61.22416) (layer F.SilkS))
  (gr_text 33 (at 75.5142 61.1886) (layer F.SilkS))
  (gr_text 3V3 (at 122.54992 79.4512 90) (layer B.SilkS))
  (gr_text 5 (at 122.54484 82.81416 90) (layer B.SilkS))
  (gr_text GND (at 122.682 86.31936 90) (layer B.SilkS))
  (gr_text GND (at 122.682 90.58656 90) (layer B.SilkS))
  (gr_text 19 (at 122.6058 94.30512 90) (layer B.SilkS))
  (gr_text 21 (at 122.69724 97.59696 90) (layer B.SilkS))
  (gr_text VIN (at 122.72264 101.17328 90) (layer B.SilkS))
  (gr_text 3V3 (at 122.72772 104.56164 90) (layer B.SilkS))
  (gr_text 34 (at 77.89164 68.48856) (layer F.SilkS))
  (gr_text 13 (at 77.90688 71.20128) (layer F.SilkS))
  (gr_text 5V (at 77.9526 73.84796) (layer F.SilkS))
  (gr_text GND (at 78.4352 78.90256) (layer F.SilkS))
  (gr_text GND (at 78.19644 83.02752) (layer F.SilkS))
  (gr_text 5V (at 78.3336 85.77072) (layer F.SilkS))
  (gr_text + (at 101.85908 105.50144) (layer F.SilkS))
  (gr_text - (at 98.49104 105.51668) (layer F.SilkS))
  (gr_text 15 (at 105.82148 92.57284) (layer F.SilkS))
  (gr_text 4 (at 103.53548 92.61856) (layer F.SilkS))
  (gr_text GND (at 100.93452 92.62872) (layer F.SilkS))
  (gr_text 3V3 (at 98.26752 92.61348) (layer F.SilkS))
  (gr_text 16 (at 95.9358 92.64396) (layer F.SilkS))
  (gr_text GND (at 93.32468 92.66428) (layer F.SilkS))
  (gr_text 17 (at 90.72372 92.6592) (layer F.SilkS))
  (gr_text DTR (at 111.57712 79.73568 90) (layer F.SilkS))
  (gr_text RTS (at 111.64824 82.92592 90) (layer F.SilkS))
  (gr_text TX (at 111.67872 85.1916 90) (layer F.SilkS))
  (gr_text VBS (at 111.75492 90.11412 90) (layer F.SilkS))
  (gr_text GND (at 111.79556 95.24492 90) (layer F.SilkS))
  (gr_text RX (at 111.66348 87.58428 90) (layer F.SilkS))
  (gr_text RST (at 119.68988 37.16528 90) (layer F.SilkS))
  (gr_text 35 (at 119.63908 39.61892 90) (layer F.SilkS))
  (gr_text 23 (at 119.64924 42.0878 90) (layer F.SilkS))
  (gr_text 22 (at 119.634 44.75988 90) (layer F.SilkS))
  (gr_text 21 (at 119.75592 47.22876 90) (layer F.SilkS))
  (gr_text 19 (at 119.75592 49.78908 90) (layer F.SilkS))
  (gr_text 18 (at 119.84736 52.3494 90) (layer F.SilkS))
  (gr_text 5 (at 119.90324 54.89956 90) (layer F.SilkS))
  (gr_text 0 (at 119.96928 57.43956 90) (layer F.SilkS))
  (gr_text GND (at 119.99468 59.8932 90) (layer F.SilkS))
  (gr_text 14 (at 119.70512 62.50432 90) (layer F.SilkS))
  (gr_text 12 (at 119.6848 65.1256 90) (layer F.SilkS))
  (gr_text 2 (at 119.72544 67.60464 90) (layer F.SilkS))
  (gr_text 3V3 (at 119.72544 70.12432 90) (layer F.SilkS))
  (gr_text 5V (at 119.77116 72.67956 90) (layer F.SilkS))
  (gr_text VIN (at 119.75084 75.27036 90) (layer F.SilkS))
  (gr_text "ver 0.1" (at 95.64624 37.93236 90) (layer F.SilkS))
  (gr_text http://edgecollective.io/quahog (at 97.0788 44.0182) (layer B.SilkS))
  (gr_text QUAHOG (at 93.71076 47.72152 90) (layer F.SilkS))
  (gr_line (start 73.0504 106.426) (end 124.5616 106.426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.9996 106.426) (end 73.914 106.426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.9996 30.48) (end 72.9996 106.426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.5616 30.48) (end 72.9996 30.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.5616 106.426) (end 124.5616 30.48) (angle 90) (layer Edge.Cuts) (width 0.15))
)
