<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4.4">
<drawing>
<board>
<plain>
<wire x1="-11.43" y1="-5.08" x2="-1.27" y2="-5.08" width="0" layer="20"/>
<wire x1="-1.27" y1="-5.08" x2="-1.27" y2="-1.27" width="0" layer="20"/>
<wire x1="-1.27" y1="-1.27" x2="1.27" y2="-1.27" width="0" layer="20"/>
<wire x1="1.27" y1="-1.27" x2="1.27" y2="-5.08" width="0" layer="20"/>
<wire x1="1.27" y1="-5.08" x2="11.43" y2="-5.08" width="0" layer="20"/>
<wire x1="11.43" y1="-5.08" x2="11.43" y2="5.08" width="0" layer="20"/>
<wire x1="11.43" y1="5.08" x2="1.27" y2="5.08" width="0" layer="20"/>
<wire x1="1.27" y1="5.08" x2="1.27" y2="1.27" width="0" layer="20"/>
<wire x1="1.27" y1="1.27" x2="-1.27" y2="1.27" width="0" layer="20"/>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="5.08" width="0" layer="20"/>
<wire x1="-1.27" y1="5.08" x2="-11.43" y2="5.08" width="0" layer="20"/>
<wire x1="-11.43" y1="5.08" x2="-11.43" y2="-5.08" width="0" layer="20"/>
<hole x="-0.85" y="0.8" drill="0.4"/>
<hole x="-0.85" y="-0.8" drill="0.4"/>
<hole x="0.85" y="0.8" drill="0.4"/>
<hole x="0.85" y="-0.8" drill="0.4"/>
<hole x="-0.85" y="0" drill="0.4"/>
<hole x="0.85" y="0" drill="0.4"/>
</plain>
<libraries>
<library name="solder_on_sockets">
<packages>
<package name="SOCKET-08">
<description>&lt;b&gt;Dual In Line Socked&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="land">
<packages>
<package name="SOIC-08M-R">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
medium body 5.3 mm (207 mil), large round pads</description>
</package>
<package name="SOIC-08-R">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm (150 mil), large round pads</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="solder_on_sockets" package="SOCKET-08" value="SONS-DIL-08"/>
<element name="U$2" library="solder_on_sockets" package="SOCKET-08" value="SONS-DIL-08"/>
<element name="U$3" library="land" package="SOIC-08-R" value="SOIC-08-R"/>
<element name="U$4" library="land" package="SOIC-08M-R" value="SOIC-08M-R"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$3" pad="8"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="7"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U$4" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$4" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$4" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U$4" pad="4"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U$4" pad="5"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="U$4" pad="6"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="U$4" pad="7"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U$4" pad="8"/>
<contactref element="U$2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
