(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-4f2ed1b~58~ubuntu16.04.1)
  (general
    (links 18)
    (no_connects 0)
    (area 68.304999 44.675666 94.255001 74.951001)
    (thickness 1.6)
    (drawings 11)
    (tracks 60)
    (zones 0)
    (modules 5)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 +3V3)
  (net 3 NO2)
  (net 4 CO)
  (net 5 SDA)
  (net 6 SCL)
  (net 7 GND)
  (net 8 SCALE_2)
  (net 9 PWM)
  (net 10 SCALE_1)
  (net 11 VREF)
  (net 12 TX)
  (net 13 RX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CO)
    (add_net NO2)
    (add_net PWM)
    (add_net RX)
    (add_net SCALE_1)
    (add_net SCALE_2)
    (add_net SCL)
    (add_net SDA)
    (add_net TX)
    (add_net VREF)
  )
  (net_class POWER ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58B88119)
    (at 81.28 66.04 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.01 180) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 TX))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58B8811E)
    (at 86.329999 68.549999 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P3 (at 2.509999 -1.300001 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.55 180) (layer F.Fab) hide)
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SDA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SCL))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58B88110)
    (at 86.36 49.784 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.55 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VREF))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58B88124)
    (at 74.93 58.42)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.55) (layer F.Fab) hide)
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 NO2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCALE_2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SCALE_1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PWM))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Rmap:microduino (layer F.Cu) (tedit 58B8849A)
    (at 81.28 61.976)
    (tags "foont print ruotato mettere i comp su F Cu")
    (fp_text reference U1 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value Microduino (at -3.175 0.254 90) (layer F.SilkS) hide)
    (pad 27 thru_hole circle (at -10.16 -12.7) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 26 thru_hole circle (at -10.16 -10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 25 thru_hole circle (at -10.16 -7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 PWM))
    (pad 24 thru_hole circle (at -10.16 -5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 SCALE_1))
    (pad 23 thru_hole circle (at -10.16 -2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 SCALE_2))
    (pad 22 thru_hole circle (at -10.16 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole circle (at -10.16 2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at -10.16 5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at -10.16 7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at -10.16 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 VREF))
    (pad 17 thru_hole circle (at -7.62 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 3 NO2))
    (pad 16 thru_hole circle (at -5.08 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 CO))
    (pad 15 thru_hole circle (at -2.54 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 2.54 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 5 SDA))
    (pad 12 thru_hole circle (at 5.08 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 SCL))
    (pad 11 thru_hole circle (at 7.62 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 10.16 7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 10.16 5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 10.16 2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 RX))
    (pad 6 thru_hole circle (at 10.16 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 TX))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 10.16 -5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 10.16 -7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 10.16 -10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 10.16 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 10.16 -12.7) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
  )
  (gr_text "Rmap\n" (at 78.105 55.245 90) (layer F.SilkS))
  (gr_text "Ver. 2" (at 85.725 53.975) (layer F.SilkS))
  (gr_line (start 93.98 73.66) (end 93.345 74.295) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.215 74.295) (end 68.58 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 47.625) (end 69.215 46.99) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.345 46.99) (end 93.98 47.625) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 73.66) (end 68.58 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 47.625) (end 68.58 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.345 46.99) (end 69.215 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.98 73.66) (end 93.98 47.625) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.215 74.295) (end 93.345 74.295) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.58 47.625) (xy 69.215 46.99) (xy 93.345 46.99) (xy 93.98 47.625) (xy 93.98 73.66)
        (xy 93.345 74.295) (xy 69.215 74.295) (xy 68.58 73.66)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.58 47.625) (xy 69.215 46.99) (xy 93.345 46.99) (xy 93.98 47.625) (xy 93.98 73.66)
        (xy 93.345 74.295) (xy 69.215 74.295) (xy 68.58 73.66)
      )
    )
  )
)
