<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="54.229" y1="0" x2="54.229" y2="19.735" width="0" layer="20"/>
<wire x1="54.229" y1="19.735" x2="29.845" y2="19.735" width="0" layer="20"/>
<wire x1="29.845" y1="19.735" x2="27.94" y2="18.7825" width="0" layer="20"/>
<wire x1="27.94" y1="18.7825" x2="26.67" y2="18.7825" width="0" layer="20"/>
<wire x1="26.67" y1="18.7825" x2="24.4475" y2="19.735" width="0" layer="20"/>
<wire x1="24.4475" y1="19.735" x2="0" y2="19.735" width="0" layer="20"/>
<wire x1="0" y1="19.735" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="24.4475" y2="0" width="0" layer="20"/>
<wire x1="24.4475" y1="0" x2="26.67" y2="0.9525" width="0" layer="20"/>
<wire x1="26.67" y1="0.9525" x2="27.94" y2="0.9525" width="0" layer="20"/>
<wire x1="27.94" y1="0.9525" x2="30.1625" y2="0" width="0" layer="20"/>
<wire x1="30.1625" y1="0" x2="54.229" y2="0" width="0" layer="20"/>
<text>Copyright 2014, David R. Chase., (CC) BY-SA</text>
<text>http://creativecommons.org/licenses/by-sa/3.0</text>
<hole x="52.07" y="9.87" drill="2"/>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<hole x="52.07" y="2.25" drill="2"/>
<hole x="52.07" y="17.49" drill="2"/>
<wire x1="19.05" y1="11.37" x2="19.05" y2="8.37" width="0" layer="20"/>
<wire x1="19.05" y1="8.37" x2="44.7675" y2="8.37" width="0" layer="20"/>
<wire x1="44.7675" y1="8.37" x2="44.7675" y2="11.37" width="0" layer="20"/>
<wire x1="44.7675" y1="11.37" x2="19.05" y2="11.37" width="0" layer="20"/>
<text>AC0</text>
<text>AC1</text>
<text>AC0</text>
<text>AC1</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO201T15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.6 mm, horizontal, grid 15.24 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="rcl" package="E5-8,5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="E5-8,5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO201T15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="DO201T15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="DO201T15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="DO201T15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C+++1" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C---1" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C---2" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C+++2" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C+++3" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C---3" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value=""/>
<element name="P0" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="V+">
<contactref element="D5" pad="C"/>
<contactref element="C4" pad="+"/>
<contactref element="D4" pad="C"/>
<contactref element="C+++1" pad="1"/>
<contactref element="C+++2" pad="1"/>
<contactref element="C+++3" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="AC1">
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="JP1" pad="4"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="AC0">
<contactref element="D2" pad="C"/>
<contactref element="D5" pad="A"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="V-">
<contactref element="D2" pad="A"/>
<contactref element="C5" pad="-"/>
<contactref element="D3" pad="A"/>
<contactref element="C---1" pad="1"/>
<contactref element="C---2" pad="1"/>
<contactref element="C---3" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="+"/>
<contactref element="P0" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
