(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 7)
    (no_connects 0)
    (area 158.483299 104.127299 168.541701 114.312701)
    (thickness 1.6)
    (drawings 19)
    (tracks 17)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 165.1 105.918)
    (visible_elements FFFFBD5F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U1-Pad3)")
  (net 3 "Net-(U1-Pad4)")
  (net 4 /Vin)
  (net 5 /Vout)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /Vin)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58D976C4)
    (at 163.83 109.22 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 0 2.9 270) (layer B.Fab) hide)
    (fp_text value TPS709xx (at 0 -2.9 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vout))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 58D9780F)
    (at 159.766 106.68 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.Fab) hide)
    (fp_text value CONN_01X03 (at 0 -7.41 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 2.33 180) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Vin))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Vout))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58D97928)
    (at 163.83 105.918)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer B.Fab))
    (fp_text value 1u (at -2.2225 1.397 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.75) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58D9790A)
    (at 163.83 112.522)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer B.Fab))
    (fp_text value 2u2 (at -2.2225 -1.651 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.75) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vout))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5.0 (at 163.0045 111.506) (layer F.SilkS))
  (gr_text 3.3 (at 163.0045 109.982) (layer F.SilkS))
  (gr_text 3.0 (at 163.0045 108.458) (layer F.SilkS))
  (gr_text 1.8 (at 163.0045 106.934) (layer F.SilkS))
  (gr_line (start 158.496 104.902) (end 158.496 113.538) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 166.243 113.538) (end 158.496 113.538) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 166.243 104.902) (end 166.243 113.538) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 158.496 104.902) (end 166.243 104.902) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text OUT (at 161.29 111.76 270) (layer F.SilkS))
  (gr_text GND (at 161.29 109.22 270) (layer F.SilkS))
  (gr_text IN (at 161.29 106.68 270) (layer F.SilkS))
  (zone (net 4) (net_name /Vin) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.322 108.6485) (xy 163.322 105.283) (xy 158.877 105.283) (xy 158.877 107.95) (xy 158.877 108.6485)
      )
    )
  )
  (zone (net 5) (net_name /Vout) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.322 113.157) (xy 158.877 113.157) (xy 158.877 110.49) (xy 158.877 109.7915) (xy 163.322 109.7915)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.862 113.157) (xy 158.877 113.157) (xy 158.877 105.283) (xy 165.862 105.283)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.5125 105.283) (xy 163.5125 113.157) (xy 165.862 113.157) (xy 165.862 105.283)
      )
    )
  )
)
