(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "/CH1_HV")
  (net 4 "/CH2_HV")
  (net 5 "Net-(U1-3V3)")
  (net 6 "/CH2_LV")
  (net 7 "/CH1_LV")
  (net 8 "unconnected-(U1-D12-Pad27)")
  (net 9 "unconnected-(U1-D13-Pad28)")
  (net 10 "unconnected-(U2-LV3-Pad5)")
  (net 11 "unconnected-(U2-LV4-Pad6)")
  (net 12 "unconnected-(U2-HV4-Pad7)")
  (net 13 "unconnected-(U2-HV3-Pad8)")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 88.875 47.483 180)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "CH2" (at 0 7.85) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/CH2_HV") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "AmazonParts:MODULE_ESP32_DEVKIT_V1_1" (layer "F.Cu")
    (at 96.21 76.895)
    (property "MANUFACTURER" "DOIT")
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.8 mm")
    (property "PARTREV" "N/A")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -8.81 -23.895) (layer "F.SilkS"))
    (fp_text value "ESP32-DEVKIT-V1" (at 0 -2.25) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -12.28 -23.475) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 12.23 -23.475) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at -12.7 -15.515) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1-3V3)") (pinfunction "3V3") (pintype "output"))
    (pad "2" thru_hole circle (at -12.7 -12.975) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at -12.7 -10.435) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 6 "/CH2_LV") (pinfunction "D15") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -12.7 -7.895) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 7 "/CH1_LV") (pinfunction "D2") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 12.7 -7.895) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-D12-Pad27)") (pinfunction "D12") (pintype "bidirectional+no_connect"))
    (pad "28" thru_hole circle (at 12.7 -10.435) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(U1-D13-Pad28)") (pinfunction "D13") (pintype "bidirectional+no_connect"))
    (pad "29" thru_hole circle (at 12.7 -12.975) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole circle (at 12.7 -15.515) (size 2 2) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VIN") (pintype "input"))
  )
  (footprint "AmazonParts:KeeYees 4 Channel IIC I2C Logic Level Converter" (layer "F.Cu")
    (at 96.52 61.38)
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "GND" (at -4 1.5 270 unlocked) (layer "F.SilkS"))
    (fp_text user "LV4" (at -4 6.5 270 unlocked) (layer "F.SilkS"))
    (fp_text user "HV" (at 3 0 270 unlocked) (layer "F.SilkS"))
    (fp_text user "LV3" (at -4 4 270 unlocked) (layer "F.SilkS"))
    (fp_text user "LV" (at -4 0 270 unlocked) (layer "F.SilkS"))
    (fp_text user "LV1" (at -3.9 -6.1 270 unlocked) (layer "F.SilkS"))
    (fp_text user "LV2" (at -3.9 -3.5 270 unlocked) (layer "F.SilkS"))
    (fp_text user "HV3" (at 3 4 270 unlocked) (layer "F.SilkS"))
    (fp_text user "HV4" (at 3 6.5 270 unlocked) (layer "F.SilkS"))
    (fp_text user "HV1" (at 3 -6 270 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at 3 1.5 270 unlocked) (layer "F.SilkS"))
    (fp_text user "HV2" (at 3 -3.5 270 unlocked) (layer "F.SilkS"))
    (fp_text_box "\n\n\n\n4Ch Level Shifter"
    (start 7.62 -7.62) (end -7.62 10.16) (angle 270) (layer "F.SilkS")    )
    (pad "1" thru_hole circle (at -5.08 -5.08) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/CH1_LV") (pinfunction "LV1") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -5.08 -2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/CH2_LV") (pinfunction "LV2") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1-3V3)") (pinfunction "LV") (pintype "input"))
    (pad "4" thru_hole rect (at -5.08 2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "5" thru_hole circle (at -5.08 5.08) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U2-LV3-Pad5)") (pinfunction "LV3") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole circle (at -5.08 7.62) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U2-LV4-Pad6)") (pinfunction "LV4") (pintype "bidirectional+no_connect"))
    (pad "7" thru_hole circle (at 5.08 7.62) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U2-HV4-Pad7)") (pinfunction "HV4") (pintype "bidirectional+no_connect"))
    (pad "8" thru_hole circle (at 5.08 5.08) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U2-HV3-Pad8)") (pinfunction "HV3") (pintype "bidirectional+no_connect"))
    (pad "9" thru_hole rect (at 5.08 2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "10" thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "HV") (pintype "input"))
    (pad "11" thru_hole circle (at 5.08 -2.54) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/CH2_HV") (pinfunction "HV2") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 5.08 -5.08) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/CH1_HV") (pinfunction "HV1") (pintype "bidirectional"))
  )
  (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal" (layer "F.Cu")
    (at 108.458 48.418 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "DC Barrel Jack with a mounting pin")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J1" (at 5.75 8.45 90) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack_MountingPin" (at -5.5 6.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 96.266 47.579677 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 0.335677 -2.54 90) (layer "F.SilkS"))
    (fp_text value "C_Polarized" (at 2.5 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 84.545 47.505 180)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "ESP32 WLED - 2 Channel - Stubby.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "CH1" (at 0 7.85) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/CH1_HV") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "B.Cu")
    (at 100.6 63.3 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0 0) (layer "B.SilkS"))
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_rect (start 81.28 38.1) (end 111.252 71.64)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Ocho's WLED\nStubby Board\nV1.0" (at 96.5 55.2) (layer "B.SilkS"))
  (gr_text "D" (at 81.7 45.6) (layer "F.SilkS"))
  (gr_text "-" (at 83.092 41.732 180) (layer "F.SilkS"))
  (gr_text "+" (at 82.838 48.082 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 81.28 38.1)
        (xy 111.252 38.1)
        (xy 111.2 71.6)
        (xy 81.3 71.6)
      )
    )
  )
)
