<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-4.572" x2="49.784" y2="-4.572" width="0.1016" layer="20"/>
<wire x1="49.784" y1="-4.572" x2="49.784" y2="31.136778125" width="0.1016" layer="20"/>
<wire x1="49.784" y1="31.136778125" x2="48.916778125" y2="32.004" width="0.1016" layer="20" curve="90"/>
<wire x1="48.916778125" y1="32.004" x2="45.317221875" y2="32.004" width="0.1016" layer="20"/>
<wire x1="45.317221875" y1="32.004" x2="44.45" y2="31.136778125" width="0.1016" layer="20" curve="90"/>
<wire x1="44.45" y1="31.136778125" x2="44.45" y2="21.844" width="0.1016" layer="20"/>
<wire x1="44.45" y1="21.844" x2="5.334" y2="21.844" width="0.1016" layer="20"/>
<wire x1="5.334" y1="21.844" x2="5.334" y2="31.136778125" width="0.1016" layer="20"/>
<wire x1="5.334" y1="31.136778125" x2="4.466778125" y2="32.004" width="0.1016" layer="20" curve="90"/>
<wire x1="4.466778125" y1="32.004" x2="0.867221875" y2="32.004" width="0.1016" layer="20"/>
<wire x1="0.867221875" y1="32.004" x2="0" y2="31.136778125" width="0.1016" layer="20" curve="90"/>
<wire x1="0" y1="31.136778125" x2="0" y2="-4.572" width="0.1016" layer="20"/>
<text>Phantomic Labs, 2019
Breadboard Adapter w/ +3V VREG
for Adafruit PowerBoost 1000C</text>
<text>GROUND</text>
<text>5V</text>
<text>5V</text>
<text>3V3</text>
<text>3V3</text>
<text>POWERBOOST</text>
</plain>
<libraries>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="BREADBOARD-POWER-V1">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="EG1213">
</package>
</packages>
</library>
<library name="ptc-littlefuse">
<description>&lt;p&gt;&lt;b&gt;Littelfuse Inc&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href = "http://www.littelfuse.com/"&gt;http://www.littelfuse.com/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Fuse Type: PTC Resettable&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;3425L series
&lt;li&gt;1812L series
&lt;li&gt;1206L series
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;created by Shigeru Kobayashi (mayfair@iamas.ac.jp)&lt;/p&gt;</description>
<packages>
<package name="1206L">
</package>
</packages>
</library>
<library name="OPL_Connector">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="H8-2.54">
</package>
</packages>
</library>
<library name="ncp1117">
<packages>
<package name="SOT223-3-M">
</package>
</packages>
</library>
<library name="OPL_Capacitor">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="CalvEngIO-Connectors">
<packages>
<package name="USB-MICRO-01.BIGGERPADS.PWR">
</package>
</packages>
</library>
<library name="rc-master-smd">
<description>&lt;b&gt;R/C MASTER-SMD! - v1.01 (07/03/2007)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD ONLY resistors and capacitors by various manufacturers. The pad sizes, spacing and silkscreen widths have been tweaked for use in dense fine pitch layouts where space, alignment and precision are critical. In general these components are designed for routing in grid increments of 5 mils&lt;/p&gt;
&lt;p&gt;* Silkscreen line elements are a minimum of 8 mils in width. All components have text sizes of 0.032"  or 0.04".&lt;/p&gt;
&lt;p&gt;* A silkscreen text values use a ratio of 18 in all cases.&lt;/p&gt;
&lt;p&gt;* ALL PADS AND PART OUTLINES ARE SNAPPED TO A 5 MIL GRID!&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All components are prefixed using the following conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;
&lt;/author&gt;</description>
<packages>
<package name="CSV-D">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic D&lt;p&gt; 
6.3 mm dia</description>
</package>
</packages>
</library>
<library name="OPL_Optoelectronics">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="LED-0805">
</package>
</packages>
</library>
<library name="CalvEngIO-Passives">
<packages>
<package name="L0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="OPL_Connector" package="H8-2.54" value="8p-2.54">
<attribute name="MPN" value="F185-1108A1BSYC1"/>
<attribute name="NAME"/>
</element>
<element name="U$10" library="diy-modules" package="BREADBOARD-POWER-V1" value="B_Rail"/>
<element name="J1" library="adafruit" package="2X04" value="">
<attribute name="NAME"/>
</element>
<element name="F1" library="ptc-littlefuse" package="1206L" value="F1"/>
<element name="S1" library="adafruit" package="EG1213" value="EG1213">
<attribute name="NAME"/>
</element>
<element name="U1" library="ncp1117" package="SOT223-3-M" value="NCP1117ST">
<attribute name="MANUFACTURER_PART_NUMBER" value="NCP1117ST12T3G"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="ON Semiconductor"/>
</element>
<element name="C2" library="rc-master-smd" package="CSV-D" value="100uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="OPL_Capacitor" package="C0805" value="0.1uF">
<attribute name="MPN" value="CC0805KKX5R8BB106"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="OPL_Capacitor" package="C0805" value="0.1uF">
<attribute name="MPN" value="CC0805KKX5R8BB106"/>
<attribute name="NAME"/>
</element>
<element name="USB1" library="CalvEngIO-Connectors" package="USB-MICRO-01.BIGGERPADS.PWR" value="USB.MICRO">
<attribute name="NAME"/>
</element>
<element name="D1" library="OPL_Optoelectronics" package="LED-0805" value="PWR">
<attribute name="MPN" value="EL-17-215/BHC-AN1P2/3T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="CalvEngIO-Passives" package="L0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="CalvEngIO-Passives" package="L0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="OPL_Capacitor" package="C0805" value="10uF">
<attribute name="MPN" value="CC0805KKX5R8BB106"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="CalvEngIO-Passives" package="R0805" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="7"/>
<contactref element="U1" pad="1"/>
<contactref element="U$10" pad="A.M.5"/>
<contactref element="U$10" pad="A.M.4"/>
<contactref element="U$10" pad="A.M.3"/>
<contactref element="U$10" pad="A.M.2"/>
<contactref element="U$10" pad="A.M.1"/>
<contactref element="U$10" pad="B.M.5"/>
<contactref element="U$10" pad="B.M.4"/>
<contactref element="U$10" pad="B.M.3"/>
<contactref element="U$10" pad="B.M.2"/>
<contactref element="U$10" pad="B.M.1"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="USB1" pad="5"/>
<contactref element="D1" pad="-"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="ENABLE">
<contactref element="J2" pad="4"/>
</signal>
<signal name="LBO">
<contactref element="J2" pad="6"/>
</signal>
<signal name="VBUS">
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="VOUT1">
<contactref element="J2" pad="8"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="VOUT2">
<contactref element="U1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="J2" pad="3"/>
</signal>
<signal name="VLIPO">
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="F1" pad="P$2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="F1" pad="P$1"/>
<contactref element="USB1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="+"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VOUT2_I">
<contactref element="L1" pad="2"/>
<contactref element="U$10" pad="B.P.5"/>
<contactref element="U$10" pad="B.P.4"/>
<contactref element="U$10" pad="B.P.3"/>
<contactref element="U$10" pad="B.P.2"/>
<contactref element="U$10" pad="B.P.1"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VOUT1_I">
<contactref element="L2" pad="2"/>
<contactref element="U$10" pad="A.P.5"/>
<contactref element="U$10" pad="A.P.4"/>
<contactref element="U$10" pad="A.P.3"/>
<contactref element="U$10" pad="A.P.2"/>
<contactref element="U$10" pad="A.P.1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$21">
</signal>
<signal name="N$23">
</signal>
</signals>
</board>
</drawing>
</eagle>
