(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 161)
    (zones 0)
    (modules 27)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1527)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.1527)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.45 0.254)
    (user_via 0.6 0.4)
    (user_via 0.8 0.6)
    (user_via 1 0.8)
    (user_via 1.3 1)
    (user_via 1.5 1.2)
    (user_via 1.7 1.4)
    (user_via 1.9 1.6)
    (uvia_size 0.6)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.381)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 VSS)
  (net 3 VDDA)
  (net 4 VSSA)
  (net 5 GND)
  (net 6 "Net-(C2-Pad2)")
  (net 7 VBUS)
  (net 8 +BATT)
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 /VREG)
  (net 12 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1527)
    (trace_width 0.1527)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.6)
    (uvia_drill 0.3)
    (add_net +BATT)
    (add_net /VREG)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net VBUS)
    (add_net VDD)
    (add_net VDDA)
    (add_net VSS)
    (add_net VSSA)
  )
  (module SquantorProto:proto-TH-0254-09X05-P020SQ-H010 (layer F.Cu) (tedit 5C521CB7)
    (at 70.485 163.83 180)
    (fp_text reference J6 (at 0 -10.16 180) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 10.16 180) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -10.16 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 -7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 -5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 -2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -5.08 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 10.16 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -2.54 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 5.08 2.54 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -10.16 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 2.54 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -7.62 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 5.08 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 7.62 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 7.62 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (module SquantorRcl:R_0603_hand (layer F.Cu) (tedit 587552B0)
    (at 41.65 161.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.45 -2.05 180) (layer F.SilkS))
    (fp_text value 1k (at -0.45 -2.05 180) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5C51FF99)
    (at 46.7 166.35 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.7 0 90) (layer F.SilkS))
    (fp_text value 10u (at -2.75 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 VBUS) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
    (at 45.2 150.9 270)
    (descr "JST PH series connector, S4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J4 (at 6.5 -2.9) (layer F.SilkS))
    (fp_text value DevBoardUartInput (at 3 7.45 270) (layer F.Fab))
    (fp_text user %R (at 3 2.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 VBUS))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorIC:SOT89-ViaTab-Microchip-MB (layer F.Cu) (tedit 5C4DDA13)
    (at 51.183514 159.213584)
    (fp_text reference U1 (at 3.016486 -2.113584) (layer F.SilkS))
    (fp_text value MCP1702-MB (at 0 2) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0 0) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /VREG))
    (pad 3 smd rect (at 1.5 0) (size 0.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad TAB smd oval (at 0 -2.1) (size 2 3.05) (layers F.Cu F.Paste F.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at -0.3 -1.7) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at 0.3 -1.7) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at 0.3 -2.3) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at -0.3 -2.3) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at 0 -2.9) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
    (pad TAB thru_hole rect (at 0 -1.1) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 /VREG) (zone_connect 2))
  )
  (module SquantorDiodes:SOD_323_onsemi (layer F.Cu) (tedit 5C4D9C56)
    (at 48.05 153.7 90)
    (fp_text reference D1 (at -2.4 0.15 180) (layer F.SilkS))
    (fp_text value NSR0320 (at -2.4 -0.05 180) (layer F.Fab))
    (pad 2 smd rect (at 1.2 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VBUS))
    (pad 1 smd rect (at -1.2 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /VREG))
  )
  (module SquantorSpecial:power_joiner_2_conn_06mm (layer F.Cu) (tedit 5C4DDA5A)
    (at 52.7 163.5 270)
    (fp_text reference U5 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value power_joiner_2_nets (at 0 1.27 270) (layer F.Fab) hide)
    (pad 2 smd circle (at 0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 1 VDD))
    (pad 1 smd circle (at -0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 6 "Net-(C2-Pad2)"))
  )
  (module SquantorSpecial:power_joiner_2_conn_06mm (layer F.Cu) (tedit 5C4DDA5A)
    (at 51.7 163.5 270)
    (fp_text reference U4 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value power_joiner_2_nets (at 0 1.27 270) (layer F.Fab) hide)
    (pad 1 smd circle (at -0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 smd circle (at 0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 3 VDDA))
  )
  (module SquantorSpecial:power_joiner_2_conn_06mm (layer F.Cu) (tedit 5C4DDA5A)
    (at 50.7 163.5 270)
    (fp_text reference U2 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value power_joiner_2_nets (at 0 1.27 270) (layer F.Fab) hide)
    (pad 2 smd circle (at 0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 2 VSS))
    (pad 1 smd circle (at -0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 5 GND))
  )
  (module SquantorSpecial:power_joiner_2_conn_06mm (layer F.Cu) (tedit 5C4DDA5A)
    (at 49.7 163.5 270)
    (fp_text reference U3 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value power_joiner_2_nets (at 0 1.27 270) (layer F.Fab) hide)
    (pad 2 smd circle (at 0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 4 VSSA))
    (pad 1 smd circle (at -0.6 0 270) (size 0.6 0.6) (layers F.Cu)
      (net 5 GND))
  )
  (module SquantorPcbOutline:MountingHole_2.5mm_no_metal locked (layer F.Cu) (tedit 5C4DD761)
    (at 70.3 174.55)
    (fp_text reference MH2 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module SquantorPcbOutline:MountingHole_2.5mm_no_metal locked (layer F.Cu) (tedit 5C4DD76B)
    (at 50.3 151.05)
    (fp_text reference MH1 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module SquantorLabels:Label_version (layer F.Cu) (tedit 5B5A1E49)
    (at 51.75 171.1 90)
    (fp_text reference N2 (at 0 1.4 90) (layer F.Fab) hide)
    (fp_text value 20190130 (at -2 0.1 90) (layer B.SilkS))
    (fp_text user V: (at 2.495 0.1 90) (layer B.SilkS))
  )
  (module SquantorConnectors:Header-0127-2X10-H006 locked (layer F.Cu) (tedit 5BE1FFD9)
    (at 60.2996 150.1)
    (fp_text reference J1 (at 7.7004 0) (layer F.SilkS))
    (fp_text value DevBoardDigital (at 0 2.5) (layer F.Fab))
    (pad 20 thru_hole circle (at 5.715 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 5.715 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 4.445 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 4.445 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 3.175 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 3.175 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.905 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 1.905 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0.635 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0.635 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -0.635 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -0.635 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.905 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.905 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.175 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -3.175 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -4.445 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 VSS))
    (pad 3 thru_hole circle (at -4.445 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 VSS))
    (pad 2 thru_hole circle (at -5.715 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at -5.715 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module SquantorConnectors:Header-0127-2X10-H006 locked (layer F.Cu) (tedit 5BE1FFD9)
    (at 60.3 175.5)
    (fp_text reference J2 (at 7.8 0) (layer F.SilkS))
    (fp_text value DevBoardAnalog (at 0 2.5) (layer F.Fab))
    (pad 20 thru_hole circle (at 5.715 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 5.715 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 4.445 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 4.445 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 3.175 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 3.175 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.905 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 1.905 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 0.635 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0.635 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -0.635 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -0.635 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.905 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSSA))
    (pad 7 thru_hole circle (at -1.905 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSSA))
    (pad 6 thru_hole circle (at -3.175 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 VDDA))
    (pad 5 thru_hole circle (at -3.175 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 VDDA))
    (pad 4 thru_hole circle (at -4.445 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 +BATT))
    (pad 3 thru_hole circle (at -4.445 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 +BATT))
    (pad 2 thru_hole circle (at -5.715 -0.63911) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 /VREG))
    (pad 1 thru_hole rect (at -5.715 0.63089) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 /VREG))
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 51.183514 154.363584)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.866486 -1.563584) (layer F.SilkS))
    (fp_text value 1u (at 0.966486 -1.563584) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /VREG))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 51.083514 161.413584)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.066486 1.686416) (layer F.SilkS))
    (fp_text value 10u (at 0.066486 1.686416) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0603_hand (layer F.Cu) (tedit 587552B0)
    (at 47.85 149.95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.75 4.35) (layer F.SilkS))
    (fp_text value 100K (at 0.75 4.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VBUS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5C51FF8E)
    (at 39.7 165 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.8 -0.4 90) (layer F.SilkS))
    (fp_text value 10u (at -2.8 -0.4 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 44.2 160.15)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at -4.6 -0.05) (layer F.SilkS))
    (fp_text value LED (at -4.6 -0.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VBUS))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0603_hand (layer F.Cu) (tedit 587552B0)
    (at 43.95 161.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3.05 -1.85 180) (layer F.SilkS))
    (fp_text value 22K (at -3.15 -1.85 180) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.85 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorIC:SOT23-5-Microchip-OT (layer F.Cu) (tedit 5C51FD5F)
    (at 43.25486 164.534634 270)
    (fp_text reference U6 (at 2.365366 -0.04514) (layer F.SilkS))
    (fp_text value MCP738312-OT (at 0 3.3 270) (layer F.Fab) hide)
    (pad 5 smd rect (at -0.95 -1.4 270) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 4 smd rect (at 0.95 -1.4 270) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 VBUS) (zone_connect 2))
    (pad 3 smd rect (at 0.95 1.4 270) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT) (zone_connect 2))
    (pad 2 smd rect (at 0 1.4 270) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 GND) (zone_connect 2))
    (pad 1 smd rect (at -0.95 1.4 270) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad1)"))
  )
  (module SquantorIC:SOT23-3 (layer F.Cu) (tedit 5C51E14D)
    (at 47.25 161)
    (fp_text reference Q1 (at 0.85 -2.3 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at -0.2 5.1) (layer F.Fab) hide)
    (pad 3 smd rect (at 0 -1) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
    (pad 2 smd rect (at 0.95 1) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /VREG))
    (pad 1 smd rect (at -0.95 1) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VBUS))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 48.15 171.9 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference N1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OHWLOGO (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal (layer B.Cu) (tedit 5C51FEE7)
    (at 40.9 168.95)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J3 (at 5.3 -6.15) (layer B.SilkS))
    (fp_text value Battery_2pin (at 5.3 -6.45) (layer B.Fab))
    (fp_text user %R (at 1 -2.5) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208)
      (net 8 +BATT) (zone_connect 2))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorProto:proto-TH-0127-04X04-P010-H006 (layer F.Cu) (tedit 5C535C8E)
    (at 55.245 169.545)
    (fp_text reference J5 (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 3.175) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module SquantorProto:proto-TH-0127-04X04-P010-H006 (layer F.Cu) (tedit 5C535C8E)
    (at 71.755 152.4)
    (fp_text reference J7 (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value Proto (at 0 3.175) (layer F.Fab) hide)
    (pad NC thru_hole rect (at -1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 -0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 0.635) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -0.635 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at -1.905 1.905) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  )
  (gr_arc (start 41.55 174.05) (end 44.55 174.05) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 79.05 151.55) (end 76.05 151.55) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.3 171.05) (end 38.3 148.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.55 171.05) (end 38.3 171.05) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44.55 177.3) (end 44.55 174.05) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.3 177.3) (end 44.55 177.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.3 154.55) (end 82.3 177.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.05 154.55) (end 82.3 154.55) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.05 148.3) (end 76.05 151.55) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.3 148.3) (end 76.05 148.3) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.3 164.8) (xy 47.8 164.8) (xy 47.8 148.3) (xy 38.3 148.3)
      )
    )
  )
  (zone (net 8) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.3 165.2) (xy 38.3 170.5) (xy 43 170.5) (xy 43 165.2)
      )
    )
  )
  (zone (net 7) (net_name VBUS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.5 165.2) (xy 47.75 165.2) (xy 47.75 170.5) (xy 43.5 170.5)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.3 148.3) (xy 47.8 148.3) (xy 47.8 164.8) (xy 38.3 164.8)
      )
    )
  )
  (zone (net 7) (net_name VBUS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.7 165.2) (xy 47.7 170.5) (xy 43.5 170.5) (xy 43.5 165.2)
      )
    )
  )
  (zone (net 8) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.3 165.2) (xy 43 165.2) (xy 43 170.5) (xy 38.3 170.5)
      )
    )
  )
  (zone (net 11) (net_name /VREG) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.2 153.3) (xy 53 153.3) (xy 53 161.5) (xy 48.2 161.5)
      )
    )
  )
  (zone (net 2) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.3 177.3) (xy 82.3 154.5) (xy 79.1 154.5) (xy 76.1 151.5) (xy 76.1 148.3)
        (xy 52.2 148.3) (xy 52.2 152.9) (xy 53.4 152.9) (xy 53.4 161.5) (xy 70.2 161.5)
        (xy 70.2 177.3)
      )
    )
  )
)
