(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 1007)
    (zones 0)
    (modules 24)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.127)
    (via_min_drill 0.254)
    (user_via 0.51 0.254)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 1 0.5)
    (user_via 1.2 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/"))
  )
  (net 0 "")
  (net 1 "Net-(BT1-PadP)")
  (net 2 GND)
  (net 3 VBUS)
  (net 4 +5V)
  (net 5 /CAS_0)
  (net 6 "Net-(J1-PadB31)")
  (net 7 "Net-(J1-PadB30)")
  (net 8 "Net-(J1-PadB29)")
  (net 9 /LWR)
  (net 10 /VRES)
  (net 11 "Net-(J1-PadB26)")
  (net 12 "Net-(J1-PadB25)")
  (net 13 /D3)
  (net 14 "Net-(J1-PadB23)")
  (net 15 "Net-(J1-PadB22)")
  (net 16 "Net-(J1-PadB21)")
  (net 17 "Net-(J1-PadB20)")
  (net 18 "Net-(J1-PadB19)")
  (net 19 "Net-(J1-PadB18)")
  (net 20 /CEO)
  (net 21 "Net-(J1-PadB15)")
  (net 22 "Net-(J1-PadB14)")
  (net 23 "Net-(J1-PadB13)")
  (net 24 "Net-(J1-PadB12)")
  (net 25 "Net-(J1-PadB11)")
  (net 26 /A22)
  (net 27 /A21)
  (net 28 /A20)
  (net 29 /A19)
  (net 30 /A18)
  (net 31 /A10)
  (net 32 /A9)
  (net 33 "Net-(J1-PadB3)")
  (net 34 "Net-(J1-PadB2)")
  (net 35 "Net-(J1-PadB1)")
  (net 36 "Net-(J1-PadA30)")
  (net 37 /D4)
  (net 38 "Net-(J1-PadA27)")
  (net 39 /D2)
  (net 40 /D5)
  (net 41 "Net-(J1-PadA24)")
  (net 42 /D1)
  (net 43 /D6)
  (net 44 "Net-(J1-PadA21)")
  (net 45 /D0)
  (net 46 /D7)
  (net 47 /A1)
  (net 48 /A17)
  (net 49 /A2)
  (net 50 /A16)
  (net 51 /A3)
  (net 52 /A15)
  (net 53 /A4)
  (net 54 /A14)
  (net 55 /A5)
  (net 56 /A13)
  (net 57 /A6)
  (net 58 /A12)
  (net 59 /A7)
  (net 60 /A11)
  (net 61 /A8)
  (net 62 "Net-(R5-Pad2)")
  (net 63 "Net-(U1-Pad8)")
  (net 64 /SRAM_WE)
  (net 65 /SRCE)
  (net 66 "Net-(U3-Pad8)")
  (net 67 "Net-(U4-Pad15)")
  (net 68 "Net-(U4-Pad14)")
  (net 69 "Net-(U4-Pad13)")
  (net 70 "Net-(U4-Pad12)")
  (net 71 /TREN)
  (net 72 "Net-(U4-Pad10)")
  (net 73 "Net-(U4-Pad7)")
  (net 74 "Net-(U5-Pad9)")
  (net 75 /SRWE)
  (net 76 "Net-(U5-Pad3)")
  (net 77 "Net-(U6-Pad9)")
  (net 78 "Net-(U6-Pad8)")
  (net 79 "Net-(U6-Pad5)")
  (net 80 "Net-(J1-PadB32)")
  (net 81 "Net-(D1-Pad1)")
  (net 82 "Net-(J1-PadB24)")
  (net 83 "Net-(U5-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A22)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CAS_0)
    (add_net /CEO)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /LWR)
    (add_net /SRAM_WE)
    (add_net /SRCE)
    (add_net /SRWE)
    (add_net /TREN)
    (add_net /VRES)
    (add_net GND)
    (add_net "Net-(BT1-PadP)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-PadA21)")
    (add_net "Net-(J1-PadA24)")
    (add_net "Net-(J1-PadA27)")
    (add_net "Net-(J1-PadA30)")
    (add_net "Net-(J1-PadB1)")
    (add_net "Net-(J1-PadB11)")
    (add_net "Net-(J1-PadB12)")
    (add_net "Net-(J1-PadB13)")
    (add_net "Net-(J1-PadB14)")
    (add_net "Net-(J1-PadB15)")
    (add_net "Net-(J1-PadB18)")
    (add_net "Net-(J1-PadB19)")
    (add_net "Net-(J1-PadB2)")
    (add_net "Net-(J1-PadB20)")
    (add_net "Net-(J1-PadB21)")
    (add_net "Net-(J1-PadB22)")
    (add_net "Net-(J1-PadB23)")
    (add_net "Net-(J1-PadB24)")
    (add_net "Net-(J1-PadB25)")
    (add_net "Net-(J1-PadB26)")
    (add_net "Net-(J1-PadB29)")
    (add_net "Net-(J1-PadB3)")
    (add_net "Net-(J1-PadB30)")
    (add_net "Net-(J1-PadB31)")
    (add_net "Net-(J1-PadB32)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(U6-Pad9)")
    (add_net VBUS)
  )
  (module Symbol:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 146.2786 127.127 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:Symbol_CreativeCommonsPublicDomain_SilkScreenTop_Small (layer B.Cu) (tedit 0)
    (at 108.2548 108.204 180)
    (descr "Symbol, Creative Commons Public Domain, SilkScreenTop, Small,")
    (tags "Symbol, Creative Commons Public Domain, SilkScreen Top, Small,")
    (attr virtual)
    (fp_text reference REF** (at 0.254 -3.5814) (layer B.SilkS) hide)
    (fp_text value Symbol_CreativeCommonsPublicDomain_SilkScreenTop_Small (at 0.59944 -8.001) (layer B.Fab))
  )
  (module Symbol:KiCad-Logo2_12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 150.114 110.9726 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 7.747 3.7084) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_12mm_SilkScreen (at 1.27 -10.16) (layer F.Fab) hide)
  )
  (module BU2450SM:BAT_BU2450SM-JJ-G (layer F.Cu) (tedit 611D559B)
    (at 142.7226 119.1641 180)
    (fp_text reference BT1 (at 16.002 -6.223) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0.0635 0.889) (layer F.Fab))
    (fp_text user - (at -15.1765 0.0635) (layer F.SilkS))
    (fp_text user - (at -15.1765 0) (layer F.Fab))
    (fp_text user + (at 15.367 0.127) (layer F.Fab))
    (fp_text user + (at 15.367 0.1905) (layer F.SilkS))
    (pad P smd rect (at 19.05 0 180) (size 5.08 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-PadP)"))
    (pad N smd rect (at -19.05 0 180) (size 5.08 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:SOIC-16_W3.90mm locked (layer F.Cu) (tedit 5D28A5A1)
    (at 135.8011 139.2428 90)
    (attr smd)
    (fp_text reference U4 (at 0.5588 5.0419 90) (layer F.SilkS))
    (fp_text value 74LS138 (at 0 5 90) (layer F.Fab))
    (fp_text user REF** (at -0.0093 -0.0224 90) (layer F.Fab))
    (pad 16 smd rect (at -4.445 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 15 smd rect (at -3.175 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U4-Pad15)") (solder_mask_margin 0.07))
    (pad 14 smd rect (at -1.905 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U4-Pad14)") (solder_mask_margin 0.07))
    (pad 13 smd rect (at -0.635 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U4-Pad13)") (solder_mask_margin 0.07))
    (pad 12 smd rect (at 0.635 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U4-Pad12)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at 1.905 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 71 /TREN) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 3.175 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U4-Pad10)") (solder_mask_margin 0.07))
    (pad 9 smd rect (at 4.445 -2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 65 /SRCE) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 4.445 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.175 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U4-Pad7)") (solder_mask_margin 0.07))
    (pad 6 smd rect (at 1.905 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.635 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /CEO) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -0.635 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /CEO) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.905 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /A22) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -3.175 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /A21) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -4.445 2.7 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /A20) (solder_mask_margin 0.07))
  )
  (module "Sega CD RAM Cart:MountingHole_6.2mm" (layer F.Cu) (tedit 611F1438)
    (at 160.3111 131.7197)
    (descr "Mounting Hole 6.2mm, no annular")
    (tags "mounting hole 6.2mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module "Sega CD RAM Cart:MountingHole_6.2mm" (layer F.Cu) (tedit 611F1438)
    (at 90.4611 131.7197)
    (descr "Mounting Hole 6.2mm, no annular")
    (tags "mounting hole 6.2mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module Package_SO:SSOP-32_11.305x20.495mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 105.791 136.398 90)
    (descr "SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (attr smd)
    (fp_text reference U2 (at 0 -11.2 90) (layer F.SilkS))
    (fp_text value IS61C5128AS-25QLI (at 0 11.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 32 smd roundrect (at 6.55 -9.525 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 31 smd roundrect (at 6.55 -8.255 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /A16))
    (pad 30 smd roundrect (at 6.55 -6.985 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /A19))
    (pad 29 smd roundrect (at 6.55 -5.715 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /SRAM_WE))
    (pad 28 smd roundrect (at 6.55 -4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /A14))
    (pad 27 smd roundrect (at 6.55 -3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /A9))
    (pad 26 smd roundrect (at 6.55 -1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /A10))
    (pad 25 smd roundrect (at 6.55 -0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /A12))
    (pad 24 smd roundrect (at 6.55 0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /CAS_0))
    (pad 23 smd roundrect (at 6.55 1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /A11))
    (pad 22 smd roundrect (at 6.55 3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /SRCE))
    (pad 21 smd roundrect (at 6.55 4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /D7))
    (pad 20 smd roundrect (at 6.55 5.715 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /D6))
    (pad 19 smd roundrect (at 6.55 6.985 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /D5))
    (pad 18 smd roundrect (at 6.55 8.255 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /D4))
    (pad 17 smd roundrect (at 6.55 9.525 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /D3))
    (pad 16 smd roundrect (at -6.55 9.525 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 15 smd roundrect (at -6.55 8.255 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /D2))
    (pad 14 smd roundrect (at -6.55 6.985 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /D1))
    (pad 13 smd roundrect (at -6.55 5.715 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /D0))
    (pad 12 smd roundrect (at -6.55 4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /A1))
    (pad 11 smd roundrect (at -6.55 3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /A2))
    (pad 10 smd roundrect (at -6.55 1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /A3))
    (pad 9 smd roundrect (at -6.55 0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /A4))
    (pad 8 smd roundrect (at -6.55 -0.635 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /A5))
    (pad 7 smd roundrect (at -6.55 -1.905 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /A6))
    (pad 6 smd roundrect (at -6.55 -3.175 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /A7))
    (pad 5 smd roundrect (at -6.55 -4.445 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /A8))
    (pad 4 smd roundrect (at -6.55 -5.715 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /A13))
    (pad 3 smd roundrect (at -6.55 -6.985 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /A15))
    (pad 2 smd roundrect (at -6.55 -8.255 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /A17))
    (pad 1 smd roundrect (at -6.55 -9.525 90) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /A18))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-32_11.305x20.495mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 90.1065 141.4145 90)
    (attr smd)
    (fp_text reference D1 (at 0.1905 -2.667 90) (layer F.SilkS))
    (fp_text value MMBD1204 (at 0.254 2.667 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(D1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VBUS) (solder_mask_margin 0.07))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 90.17 144.5895 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 "Net-(BT1-PadP)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 81 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SSOP-20_W5.3mm (layer F.Cu) (tedit 5D28A69D)
    (at 150.4315 144.9705)
    (descr http://ww1.microchip.com/downloads/en/DeviceDoc/41606B.pdf)
    (attr smd)
    (fp_text reference U7 (at 4.7625 0.0127 90) (layer F.SilkS))
    (fp_text value 74LS245 (at 0 5.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at -2.925 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 19 smd rect (at -2.275 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 71 /TREN))
    (pad 18 smd rect (at -1.625 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at -0.975 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 16 smd rect (at -0.325 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 15 smd rect (at 0.325 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 0.975 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 1.625 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2.275 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.925 -3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.925 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.275 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.625 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.975 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.325 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -0.325 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.975 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 39 /D2))
    (pad 3 smd rect (at -1.625 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 42 /D1))
    (pad 2 smd rect (at -2.275 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 45 /D0))
    (pad 1 smd rect (at -2.925 3.6) (size 0.45 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:SOIC-14_W3.9mm (layer F.Cu) (tedit 5D28A598)
    (at 122.682 140.6525 180)
    (attr smd)
    (fp_text reference U6 (at 0 -4.79) (layer F.SilkS))
    (fp_text value 74LS74 (at 0 5.29) (layer F.Fab))
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at -3.81 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -2.54 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 12 smd rect (at -1.27 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.27 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.54 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U6-Pad9)") (solder_mask_margin 0.07))
    (pad 8 smd rect (at 3.81 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U6-Pad8)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.81 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.54 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U5-Pad9)") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.27 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U6-Pad5)") (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /VRES) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.27 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 75 /SRWE) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.54 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 45 /D0) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -3.81 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOIC-14_W3.9mm (layer F.Cu) (tedit 5D28A598)
    (at 122.7369 130.2169 180)
    (attr smd)
    (fp_text reference U5 (at -0.0721 5.2489) (layer F.SilkS))
    (fp_text value 74LS32 (at 0 5.29) (layer F.Fab))
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at -3.81 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -2.54 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 12 smd rect (at -1.27 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U5-Pad11)") (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.27 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /LWR) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.54 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U5-Pad9)") (solder_mask_margin 0.07))
    (pad 8 smd rect (at 3.81 -2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 /SRAM_WE) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.81 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.54 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 75 /SRWE) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.27 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U5-Pad3)") (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U4-Pad7)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.27 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U5-Pad3)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.54 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U3-Pad8)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -3.81 2.7 180) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad8)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOIC-14_W3.9mm (layer F.Cu) (tedit 5D28A598)
    (at 110.1725 120.523 270)
    (attr smd)
    (fp_text reference U3 (at 0 -4.79 90) (layer F.SilkS))
    (fp_text value 74LS30 (at 0 5.29 90) (layer F.Fab))
    (fp_text user REF** (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at -3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 12 smd rect (at -1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 53 /A4) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 55 /A5) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 8 smd rect (at 3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U3-Pad8)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 57 /A6) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 /A7) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 61 /A8) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /A9) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /A10) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 60 /A11) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOIC-14_W3.9mm (layer F.Cu) (tedit 5D28A598)
    (at 98.9965 120.4595 270)
    (attr smd)
    (fp_text reference U1 (at 0 -4.79 90) (layer F.SilkS))
    (fp_text value 74LS30 (at 0 5.29 90) (layer F.Fab))
    (fp_text user REF** (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at -3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 12 smd rect (at -1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 58 /A12) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 56 /A13) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 8 smd rect (at 3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad8)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 54 /A14) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 52 /A15) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 50 /A16) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 48 /A17) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 /A18) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /A19) (solder_mask_margin 0.07))
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 87.9475 152.146 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 1 -3.75) (layer F.SilkS))
    (fp_text value "22uF 25v" (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 143.9037 138.1637 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.0161 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 143.9545 144.9705 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (pad 1 smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 130.13222 132.76072)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0.03262 -1.78308) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 129.032 140.614 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 110.0455 114.427 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0.0635 1.651) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 98.958 114.4905 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0.0885 1.8415) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 89.9795 138.2395 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0.102 1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 3 VBUS))
    (pad 1 smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1886784905660377)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Sega CD RAM Cart:Genesis_Card_Edge" (layer F.Cu) (tedit 611EFFB7)
    (at 84.4931 164.7317)
    (descr "Sega Genesis 64-Pin Card Edge Connector")
    (tags "Genesis Edge")
    (attr virtual)
    (fp_text reference J1 (at 34.671 -9.398) (layer F.SilkS))
    (fp_text value Genesis_Edge_Connector (at 35.687 -12.954) (layer F.Fab))
    (fp_text user %R (at 34.671 -10.922) (layer F.Fab))
    (pad B16 connect rect (at 38.989 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 5 /CAS_0))
    (pad A32 connect rect (at 79.629 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad B32 connect rect (at 79.629 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 80 "Net-(J1-PadB32)"))
    (pad B31 connect rect (at 77.089 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 6 "Net-(J1-PadB31)"))
    (pad B30 connect rect (at 74.549 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 7 "Net-(J1-PadB30)"))
    (pad B29 connect rect (at 72.009 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-PadB29)"))
    (pad B28 connect rect (at 69.469 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 9 /LWR))
    (pad B27 connect rect (at 66.929 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 10 /VRES))
    (pad B26 connect rect (at 64.389 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 11 "Net-(J1-PadB26)"))
    (pad B25 connect rect (at 61.849 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 12 "Net-(J1-PadB25)"))
    (pad B24 connect rect (at 59.309 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 82 "Net-(J1-PadB24)"))
    (pad B23 connect rect (at 56.769 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 14 "Net-(J1-PadB23)"))
    (pad B22 connect rect (at 54.229 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 15 "Net-(J1-PadB22)"))
    (pad B21 connect rect (at 51.689 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 16 "Net-(J1-PadB21)"))
    (pad B20 connect rect (at 49.149 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 17 "Net-(J1-PadB20)"))
    (pad B19 connect rect (at 46.609 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 18 "Net-(J1-PadB19)"))
    (pad B18 connect rect (at 44.069 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 19 "Net-(J1-PadB18)"))
    (pad B17 connect rect (at 41.529 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 20 /CEO))
    (pad B15 connect rect (at 36.449 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 21 "Net-(J1-PadB15)"))
    (pad B14 connect rect (at 33.909 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 22 "Net-(J1-PadB14)"))
    (pad B13 connect rect (at 31.369 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 23 "Net-(J1-PadB13)"))
    (pad B12 connect rect (at 28.829 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 24 "Net-(J1-PadB12)"))
    (pad B11 connect rect (at 26.289 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 25 "Net-(J1-PadB11)"))
    (pad B10 connect rect (at 23.749 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 26 /A22))
    (pad B9 connect rect (at 21.209 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 27 /A21))
    (pad B8 connect rect (at 18.669 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 28 /A20))
    (pad B7 connect rect (at 16.129 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 29 /A19))
    (pad B6 connect rect (at 13.589 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 30 /A18))
    (pad B5 connect rect (at 11.049 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 31 /A10))
    (pad B4 connect rect (at 8.509 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 32 /A9))
    (pad B3 connect rect (at 5.969 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 33 "Net-(J1-PadB3)"))
    (pad B2 connect rect (at 3.429 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 34 "Net-(J1-PadB2)"))
    (pad B1 connect rect (at 0.889 -3) (size 1.78 6) (layers F.Cu F.Mask)
      (net 35 "Net-(J1-PadB1)"))
    (pad A31 connect rect (at 77.089 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 4 +5V))
    (pad A30 connect rect (at 74.549 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 36 "Net-(J1-PadA30)"))
    (pad A29 connect rect (at 72.009 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 13 /D3))
    (pad A28 connect rect (at 69.469 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 37 /D4))
    (pad A27 connect rect (at 66.929 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 38 "Net-(J1-PadA27)"))
    (pad A26 connect rect (at 64.389 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 39 /D2))
    (pad A25 connect rect (at 61.849 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 40 /D5))
    (pad A24 connect rect (at 59.309 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 41 "Net-(J1-PadA24)"))
    (pad A23 connect rect (at 56.769 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 42 /D1))
    (pad A22 connect rect (at 54.229 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 43 /D6))
    (pad A21 connect rect (at 51.689 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 44 "Net-(J1-PadA21)"))
    (pad A20 connect rect (at 49.149 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 45 /D0))
    (pad A19 connect rect (at 46.609 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 46 /D7))
    (pad A18 connect rect (at 44.069 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad A17 connect rect (at 41.529 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 47 /A1))
    (pad A16 connect rect (at 38.989 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 48 /A17))
    (pad A15 connect rect (at 36.449 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 49 /A2))
    (pad A14 connect rect (at 33.909 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 50 /A16))
    (pad A13 connect rect (at 31.369 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 51 /A3))
    (pad A12 connect rect (at 28.829 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 52 /A15))
    (pad A11 connect rect (at 26.289 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 53 /A4))
    (pad A10 connect rect (at 23.749 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 54 /A14))
    (pad A9 connect rect (at 21.209 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 55 /A5))
    (pad A8 connect rect (at 18.669 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 56 /A13))
    (pad A7 connect rect (at 16.129 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 57 /A6))
    (pad A6 connect rect (at 13.589 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 58 /A12))
    (pad A5 connect rect (at 11.049 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 59 /A7))
    (pad A4 connect rect (at 8.509 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 60 /A11))
    (pad A3 connect rect (at 5.969 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 61 /A8))
    (pad A2 connect rect (at 3.429 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 4 +5V))
    (pad A1 connect rect (at 0.889 -3) (size 1.78 6) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (gr_text "Sega CD Back-up RAM Cart (4Mbit) v1.1\nDesigned by WindDrake with help from Officer_Skidmark\nBased on l_oliveira's original research\ngithub.com/WindDrake/SegaCD_Ramcart" (at 83.4898 108.2802) (layer F.SilkS))
  (gr_line (start 166.6611 104.25) (end 82.8411 104.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 82.8411 104.25) (end 82.8411 164.4857) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 82.8411 164.4857) (end 83.6031 165.7557) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 165.8991 165.7557) (end 166.6611 164.4857) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 83.6031 165.7557) (end 165.8991 165.7557) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.6611 164.4857) (end 166.6611 104.25) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 166.37 157.554) (xy 83.058 157.554) (xy 83.058 129.487) (xy 83.058 104.4702) (xy 166.37 104.4702)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 157.554) (xy 83.058 157.554) (xy 83.058 104.4702) (xy 166.37 104.4702)
      )
    )
  )
)
