(kicad_pcb (version 20170123) (host pcbnew "(2017-05-14 revision 14bb238b3)-makepkg")
  (general
    (links 294)
    (no_connects 0)
    (area 25.891648 66.300001 119.49643 136.700001)
    (thickness 1.6)
    (drawings 31)
    (tracks 1586)
    (zones 0)
    (modules 107)
    (nets 88)
  )
  (page A)
  (title_block
    (title "pi-top Glimmer")
    (date 2017-06-26)
    (rev 1.0beta)
    (company C.Schnarel)
    (comment 1 "Based on pi-top_Template board definition")
    (comment 2 "Practice I2C Design & Programming")
    (comment 3 "Visual Distraction, Voltage Monitor, IR Receiver")
    (comment 4 "pi-top Accessory Buss Board")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 4.5)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 38 74)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 BCM-24)
  (net 2 MOSI_BCM-10)
  (net 3 BCM-22)
  (net 4 BCM-23)
  (net 5 PCM_D_BCM-27)
  (net 6 PCM_C_BCM-18)
  (net 7 GPCLK0-BCM-4)
  (net 8 BCM-17)
  (net 9 RXD_BCM-15)
  (net 10 HUB_3V3_PRST)
  (net 11 HUB_3V3)
  (net 12 HUB_5V)
  (net 13 HUB_PWR)
  (net 14 SPDIF_OUT)
  (net 15 SCL_BCM-3)
  (net 16 SDA_BCM-2)
  (net 17 ID_SC_BCM-1)
  (net 18 BCM-5)
  (net 19 ID_SD_BCM-0)
  (net 20 CE1_BCM-7)
  (net 21 MISO_BCM-9)
  (net 22 BCM-25)
  (net 23 CE0_BCM-8)
  (net 24 SCLK_BCM-11)
  (net 25 BCM-13)
  (net 26 MISO_BCM-19)
  (net 27 BCM-12)
  (net 28 BCM-6)
  (net 29 BCM-16)
  (net 30 BCM-26)
  (net 31 SCLK_BCM-21)
  (net 32 MOSI_BCM-20)
  (net 33 +5V)
  (net 34 GND)
  (net 35 +3V3)
  (net 36 "Net-(C5-Pad1)")
  (net 37 ~Reset)
  (net 38 DTR)
  (net 39 "Net-(D1-Pad1)")
  (net 40 "Net-(D1-Pad2)")
  (net 41 "Net-(D10-Pad2)")
  (net 42 "Net-(D11-Pad2)")
  (net 43 "Net-(D12-Pad2)")
  (net 44 "Net-(D13-Pad2)")
  (net 45 "Net-(D14-Pad2)")
  (net 46 "Net-(D15-Pad2)")
  (net 47 "Net-(D16-Pad2)")
  (net 48 "Net-(D10-Pad1)")
  (net 49 AVR_TXO)
  (net 50 AVR_RXI)
  (net 51 "Net-(J1-Pad3)")
  (net 52 AVR_MOSI)
  (net 53 AVR_SCK)
  (net 54 AVR_MISO)
  (net 55 TXD_BCM-14)
  (net 56 "Net-(J6-Pad1)")
  (net 57 "Net-(Q6-Pad1)")
  (net 58 PWR_SENS)
  (net 59 3V3_SENS)
  (net 60 5V_SENS)
  (net 61 "Net-(D17-Pad1)")
  (net 62 "Net-(D25-Pad1)")
  (net 63 "Net-(D33-Pad1)")
  (net 64 LED_C)
  (net 65 LED_D)
  (net 66 "Net-(U2-Pad8)")
  (net 67 "Net-(U2-Pad7)")
  (net 68 "Net-(D41-Pad1)")
  (net 69 "Net-(D49-Pad1)")
  (net 70 "Net-(D57-Pad1)")
  (net 71 "Net-(Q1-Pad1)")
  (net 72 "Net-(Q2-Pad1)")
  (net 73 "Net-(Q3-Pad1)")
  (net 74 "Net-(Q4-Pad1)")
  (net 75 "Net-(Q5-Pad1)")
  (net 76 "Net-(Q7-Pad1)")
  (net 77 "Net-(Q8-Pad1)")
  (net 78 "Net-(U2-Pad32)")
  (net 79 "Net-(U2-Pad13)")
  (net 80 "Net-(U2-Pad11)")
  (net 81 "Net-(U2-Pad10)")
  (net 82 "Net-(U2-Pad9)")
  (net 83 "Net-(U2-Pad2)")
  (net 84 "Net-(U2-Pad1)")
  (net 85 ADC3)
  (net 86 ADC7)
  (net 87 ADC6)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net 3V3_SENS)
    (add_net 5V_SENS)
    (add_net ADC3)
    (add_net ADC6)
    (add_net ADC7)
    (add_net AVR_MISO)
    (add_net AVR_MOSI)
    (add_net AVR_RXI)
    (add_net AVR_SCK)
    (add_net AVR_TXO)
    (add_net BCM-12)
    (add_net BCM-13)
    (add_net BCM-16)
    (add_net BCM-17)
    (add_net BCM-22)
    (add_net BCM-23)
    (add_net BCM-24)
    (add_net BCM-25)
    (add_net BCM-26)
    (add_net BCM-5)
    (add_net BCM-6)
    (add_net CE0_BCM-8)
    (add_net CE1_BCM-7)
    (add_net DTR)
    (add_net GND)
    (add_net GPCLK0-BCM-4)
    (add_net HUB_3V3)
    (add_net HUB_3V3_PRST)
    (add_net HUB_5V)
    (add_net HUB_PWR)
    (add_net ID_SC_BCM-1)
    (add_net ID_SD_BCM-0)
    (add_net LED_C)
    (add_net LED_D)
    (add_net MISO_BCM-19)
    (add_net MISO_BCM-9)
    (add_net MOSI_BCM-10)
    (add_net MOSI_BCM-20)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D33-Pad1)")
    (add_net "Net-(D41-Pad1)")
    (add_net "Net-(D49-Pad1)")
    (add_net "Net-(D57-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net PCM_C_BCM-18)
    (add_net PCM_D_BCM-27)
    (add_net PWR_SENS)
    (add_net RXD_BCM-15)
    (add_net SCLK_BCM-11)
    (add_net SCLK_BCM-21)
    (add_net SCL_BCM-3)
    (add_net SDA_BCM-2)
    (add_net SPDIF_OUT)
    (add_net TXD_BCM-14)
    (add_net ~Reset)
  )
  (module MyLogos:S_Silk (layer B.Cu) (tedit 0)
    (at 48.922 118.45 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Socket_Strips:Socket_Strip_Angled_2x17_Pitch2.00mm locked (layer B.Cu) (tedit 58CD5450)
    (at 92.85 86 180)
    (descr "Through hole angled socket strip, 2x17, 2.00mm pitch, 6.35mm socket length, double rows")
    (tags "Through hole angled socket strip THT 2x17 2.00mm double row")
    (fp_text reference J5 (at -4.31 2 180) (layer B.SilkS))
    (fp_text value CONN_02X17 (at -4.31 -34 180) (layer B.Fab))
    (fp_text user %R (at -4.31 2 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 HUB_PWR))
    (pad 2 thru_hole oval (at -2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HUB_5V))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 HUB_3V3_PRST))
    (pad 4 thru_hole oval (at -2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 HUB_3V3))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 6 thru_hole oval (at -2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 SPDIF_OUT))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 SDA_BCM-2))
    (pad 8 thru_hole oval (at -2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 SCL_BCM-3))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GPCLK0-BCM-4))
    (pad 10 thru_hole oval (at -2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 TXD_BCM-14))
    (pad 11 thru_hole oval (at 0 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 RXD_BCM-15))
    (pad 12 thru_hole oval (at -2 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 BCM-17))
    (pad 13 thru_hole oval (at 0 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 PCM_C_BCM-18))
    (pad 14 thru_hole oval (at -2 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 PCM_D_BCM-27))
    (pad 15 thru_hole oval (at 0 -14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 BCM-22))
    (pad 16 thru_hole oval (at -2 -14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 BCM-23))
    (pad 17 thru_hole oval (at 0 -16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 BCM-24))
    (pad 18 thru_hole oval (at -2 -16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 MOSI_BCM-10))
    (pad 19 thru_hole oval (at 0 -18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 MISO_BCM-9))
    (pad 20 thru_hole oval (at -2 -18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 BCM-25))
    (pad 21 thru_hole oval (at 0 -20 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 SCLK_BCM-11))
    (pad 22 thru_hole oval (at -2 -20 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 CE0_BCM-8))
    (pad 23 thru_hole oval (at 0 -22 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 CE1_BCM-7))
    (pad 24 thru_hole oval (at -2 -22 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 ID_SD_BCM-0))
    (pad 25 thru_hole oval (at 0 -24 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 ID_SC_BCM-1))
    (pad 26 thru_hole oval (at -2 -24 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 BCM-5))
    (pad 27 thru_hole oval (at 0 -26 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 BCM-6))
    (pad 28 thru_hole oval (at -2 -26 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 BCM-12))
    (pad 29 thru_hole oval (at 0 -28 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 BCM-13))
    (pad 30 thru_hole oval (at -2 -28 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 MISO_BCM-19))
    (pad 31 thru_hole oval (at 0 -30 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 BCM-16))
    (pad 32 thru_hole oval (at -2 -30 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 BCM-26))
    (pad 33 thru_hole oval (at 0 -32 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 MOSI_BCM-20))
    (pad 34 thru_hole oval (at -2 -32 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SCLK_BCM-21))
    (model C:/Users/Chip/Documents/KiCad_Workspace/libraries/3dmodels/Samtec_socket_34pin_THT.step
      (at (xyz -0.3543307086614174 0.03937007874015748 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x17_Pitch2.00mm locked (layer B.Cu) (tedit 58CD4ECD)
    (at 43 86 180)
    (descr "Through hole angled pin header, 2x17, 2.00mm pitch, 4mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x17 2.00mm double row")
    (fp_text reference J3 (at 4 2 180) (layer B.SilkS))
    (fp_text value CONN_02X17 (at 4 -34 180) (layer B.Fab))
    (fp_text user %R (at 4 2 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 HUB_PWR))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HUB_5V))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 HUB_3V3_PRST))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 HUB_3V3))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 SPDIF_OUT))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 SDA_BCM-2))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 SCL_BCM-3))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GPCLK0-BCM-4))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 TXD_BCM-14))
    (pad 11 thru_hole oval (at 0 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 RXD_BCM-15))
    (pad 12 thru_hole oval (at 2 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 BCM-17))
    (pad 13 thru_hole oval (at 0 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 PCM_C_BCM-18))
    (pad 14 thru_hole oval (at 2 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 PCM_D_BCM-27))
    (pad 15 thru_hole oval (at 0 -14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 BCM-22))
    (pad 16 thru_hole oval (at 2 -14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 BCM-23))
    (pad 17 thru_hole oval (at 0 -16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 BCM-24))
    (pad 18 thru_hole oval (at 2 -16 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 MOSI_BCM-10))
    (pad 19 thru_hole oval (at 0 -18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 MISO_BCM-9))
    (pad 20 thru_hole oval (at 2 -18 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 BCM-25))
    (pad 21 thru_hole oval (at 0 -20 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 SCLK_BCM-11))
    (pad 22 thru_hole oval (at 2 -20 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 CE0_BCM-8))
    (pad 23 thru_hole oval (at 0 -22 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 CE1_BCM-7))
    (pad 24 thru_hole oval (at 2 -22 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 ID_SD_BCM-0))
    (pad 25 thru_hole oval (at 0 -24 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 ID_SC_BCM-1))
    (pad 26 thru_hole oval (at 2 -24 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 BCM-5))
    (pad 27 thru_hole oval (at 0 -26 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 BCM-6))
    (pad 28 thru_hole oval (at 2 -26 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 BCM-12))
    (pad 29 thru_hole oval (at 0 -28 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 BCM-13))
    (pad 30 thru_hole oval (at 2 -28 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 MISO_BCM-19))
    (pad 31 thru_hole oval (at 0 -30 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 BCM-16))
    (pad 32 thru_hole oval (at 2 -30 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 BCM-26))
    (pad 33 thru_hole oval (at 0 -32 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 MOSI_BCM-20))
    (pad 34 thru_hole oval (at 2 -32 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SCLK_BCM-21))
    (model C:/Users/Chip/Documents/KiCad_Workspace/libraries/3dmodels/3M_951-series_34pin_THT.step
      (at (xyz 0.187007874015748 -1.269685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC6)
    (at 94.896 125.054 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J4 (at -1.778 -2.54) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 1.27 50.59 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 SCLK_BCM-21))
    (pad 39 thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 38 thru_hole oval (at 2.54 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 MOSI_BCM-20))
    (pad 37 thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 BCM-26))
    (pad 36 thru_hole oval (at 2.54 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 BCM-16))
    (pad 35 thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 MISO_BCM-19))
    (pad 34 thru_hole oval (at 2.54 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 33 thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 BCM-13))
    (pad 32 thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 BCM-12))
    (pad 31 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 BCM-6))
    (pad 30 thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 29 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 BCM-5))
    (pad 28 thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 ID_SC_BCM-1))
    (pad 27 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 ID_SD_BCM-0))
    (pad 26 thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CE1_BCM-7))
    (pad 25 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 24 thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 CE0_BCM-8))
    (pad 23 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 SCLK_BCM-11))
    (pad 22 thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 BCM-25))
    (pad 21 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 MISO_BCM-9))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 MOSI_BCM-10))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 BCM-24))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 BCM-23))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 BCM-22))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PCM_D_BCM-27))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 PCM_C_BCM-18))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 BCM-17))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 RXD_BCM-15))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 TXD_BCM-14))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GPCLK0-BCM-4))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 SCL_BCM-3))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 HUB_5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 SDA_BCM-2))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 HUB_5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 78 113.5 270)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0.124 -3.688 270) (layer B.SilkS))
    (fp_text value 74LV164 (at 0 -3.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.95 1.95 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 65 LED_D))
    (pad 2 smd rect (at -2.95 1.3 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 3 smd rect (at -2.95 0.65 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at -2.95 0 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (pad 5 smd rect (at -2.95 -0.65 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 6 smd rect (at -2.95 -1.3 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (pad 7 smd rect (at -2.95 -1.95 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 8 smd rect (at 2.95 -1.95 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 64 LED_C))
    (pad 9 smd rect (at 2.95 -1.3 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 10 smd rect (at 2.95 -0.65 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 11 smd rect (at 2.95 0 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (pad 12 smd rect (at 2.95 0.65 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 13 smd rect (at 2.95 1.3 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (pad 14 smd rect (at 2.95 1.95 270) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 64.5 113.5)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at -2.878 3.426) (layer B.SilkS))
    (fp_text value 74LV164 (at 0 -3.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 14 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 13 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(Q8-Pad1)"))
    (pad 12 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(Q7-Pad1)"))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(Q6-Pad1)"))
    (pad 10 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(Q5-Pad1)"))
    (pad 9 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 8 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 64 LED_C))
    (pad 7 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 6 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(Q4-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(Q3-Pad1)"))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(Q2-Pad1)"))
    (pad 3 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 1 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 48.5 117.5 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D18 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380_Pad locked (layer F.Cu) (tedit 59264ECD)
    (at 99.5 126.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380_Pad (at 0 3.25) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380_Pad locked (layer F.Cu) (tedit 59264EDF)
    (at 41.5 126.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380_Pad (at 0 3.25) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380_Pad locked (layer F.Cu) (tedit 59264EBA)
    (at 99.5 77.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380_Pad (at 0 3.25) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380_Pad locked (layer F.Cu) (tedit 59264E9B)
    (at 41.5 77.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380_Pad (at 0 3.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 50.446 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.502 0 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 50.5 93)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.502 -0.05 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 50.5 102)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.5 0 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 50.5 105)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.5 0 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 60.7 93.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.356 -0.094 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 67 81 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.414 0.044) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 37 ~Reset))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 38 DTR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53.1 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D12 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D14 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D15 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 58 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D16 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 49.5 76.5 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at -0.04 -4.134 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 DTR))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 AVR_TXO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 AVR_RXI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 86.5 79 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 ~Reset))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 AVR_MOSI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 AVR_SCK))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 AVR_MISO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer B.Cu) (tedit 58307B90)
    (at 50.5 87)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at -3.502 0 90) (layer B.SilkS))
    (fp_text value 2.2uH (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 HUB_5V))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (model Inductors_SMD.3dshapes\L_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 64 81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.414 0.092) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 ~Reset))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 58 81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.414 -0.066) (layer B.SilkS))
    (fp_text value 4.48k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 HUB_PWR))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 PWR_SENS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 61 81 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.414 0.114 180) (layer B.SilkS))
    (fp_text value 715R (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 PWR_SENS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 46 81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.414 0.126) (layer B.SilkS))
    (fp_text value 300R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 3V3_SENS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 HUB_3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 49 81 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.414 -0.078 180) (layer B.SilkS))
    (fp_text value 3k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 3V3_SENS))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 52 81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.414 0.03) (layer B.SilkS))
    (fp_text value 2.2k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 5V_SENS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 HUB_5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 55 81 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.414 0.018 180) (layer B.SilkS))
    (fp_text value 3.3k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 5V_SENS))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Opto-Devices:IRReceiver_Vishay_MINICAST-3pin (layer F.Cu) (tedit 588C7248)
    (at 73 79)
    (descr "IR Receiver Vishay TSOP-xxxx, MINICAST package")
    (tags "IR Receiver Vishay TSOP-xxxx MINICAST")
    (fp_text reference U5 (at 2.338 -2.46) (layer F.SilkS))
    (fp_text value TSOP38238 (at 2.55 -2.4 -180) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(J6-Pad1)"))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D17 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D19 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D20 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D21 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 63 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D24 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D25 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D26 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D27 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D28 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D29 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D30 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D31 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 68 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D32 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D33 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D34 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer B.Cu) (tedit 58CC9A48)
    (at 68.2 94 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 6.05 180) (layer B.SilkS))
    (fp_text value ATMEGA328P-AU (at 0 -6.05 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 32 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(U2-Pad32)"))
    (pad 31 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 AVR_TXO))
    (pad 30 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 50 AVR_RXI))
    (pad 29 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 37 ~Reset))
    (pad 28 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 SCL_BCM-3))
    (pad 27 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 SDA_BCM-2))
    (pad 26 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 85 ADC3))
    (pad 25 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 58 PWR_SENS))
    (pad 24 smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 60 5V_SENS))
    (pad 23 smd rect (at 4.25 2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 59 3V3_SENS))
    (pad 22 smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 86 ADC7))
    (pad 21 smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 20 smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 19 smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 87 ADC6))
    (pad 18 smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 17 smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 53 AVR_SCK))
    (pad 16 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 54 AVR_MISO))
    (pad 15 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 52 AVR_MOSI))
    (pad 14 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 64 LED_C))
    (pad 13 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 65 LED_D))
    (pad 11 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U2-Pad8)"))
    (pad 7 smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 5 smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 4 smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 3 smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 2 smd rect (at -4.25 2 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(U2-Pad1)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D35 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D36 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D37 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D38 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D39 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 73 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D40 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D41 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D42 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D43 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D44 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D45 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D46 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D47 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 78 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D48 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D49 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D50 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D51 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D52 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D53 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D54 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D55 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 83 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D56 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 84.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D57 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 89.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D58 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 94.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D59 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 99.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D60 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D12-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 104.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D61 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 109.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D62 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 114.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D63 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D15-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 88 119.5)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D64 (at 0 -1.45) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module pi-top:Resonator_SMD_muRata_CSTCE_3.2mm_1.3mm (layer B.Cu) (tedit 5945AE29)
    (at 76.2 96.5 90)
    (fp_text reference Y1 (at 0 2 90) (layer B.SilkS))
    (fp_text value 8MHz (at 0 2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.2 0 90) (size 0.4 1.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U2-Pad8)"))
    (pad 2 smd rect (at 0 0 90) (size 0.4 1.6) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 3 smd rect (at 1.2 0 90) (size 0.4 1.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U2-Pad7)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 48.5 107.5 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 48.5 97.5 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D17-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 48.5 87.5 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 99 88 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D33-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5929C190)
    (at 99 97 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5929C174)
    (at 99 107 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D49-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5929C180)
    (at 99 117 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRFML8244 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D57-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 61.114 99.908 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 76.354 92.034 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 73.814 115.148 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.524 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.524 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 67.464 118.958 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-89-3_Handsoldering (layer B.Cu) (tedit 58CE4E7F)
    (at 49.378 97.09 180)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference U1 (at 3.25 2.008 180) (layer B.SilkS))
    (fp_text value AP7215-33YG (at 0.5 -3.15 180) (layer B.Fab))
    (fp_text user %R (at 0.38 0 180) (layer B.Fab))
    (pad 2 smd trapezoid (at -0.37 0 90) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 2 smd rect (at 1.98 0 270) (size 2 4) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 3 smd rect (at -1.98 -1.5 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at -1.98 0 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 33 +5V))
    (pad 1 smd rect (at -1.98 1.5 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 34 GND))
    (model C:/Users/Chip/Documents/KiCad_Workspace/libraries/3dmodels/SOT-89-3.step
      (at (xyz 0.01968503937007874 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SolderJumpers:SPST_Jumper (layer B.Cu) (tedit 595179E2)
    (at 69.496 77.683 270)
    (fp_text reference J6 (at -1.651 0) (layer B.SilkS))
    (fp_text value SPST_Jumper (at -0.254 4.572 270) (layer B.Fab))
    (pad 1 smd rect (at -0.635 0 270) (size 0.381 0.3556) (layers B.Cu)
      (net 56 "Net-(J6-Pad1)"))
    (pad 2 smd rect (at 0.508 0 270) (size 0.635 0.3556) (layers B.Cu)
      (net 8 BCM-17))
  )
  (gr_text ADC3 (at 66.194 86.192) (layer F.SilkS))
  (gr_text ADC7 (at 62.638 86.192) (layer F.SilkS))
  (gr_text GRN (at 64.67 76.54 90) (layer F.SilkS))
  (gr_text BLK (at 47.144 76.54 90) (layer F.SilkS))
  (gr_text 39 (at 46.636 123.022) (layer F.SilkS))
  (gr_text 1 (at 94.896 123.022) (layer F.SilkS))
  (gr_text 2 (at 94.896 84.16) (layer B.SilkS))
  (gr_text 1 (at 92.864 84.16) (layer B.SilkS))
  (gr_text 34 (at 40.794 120) (layer B.SilkS))
  (gr_text 33 (at 43.08 120) (layer B.SilkS))
  (gr_text 1 (at 43.08 84) (layer B.SilkS))
  (gr_text 2 (at 41.048 84) (layer B.SilkS))
  (dimension 24.5 (width 0.15) (layer Dwgs.User)
    (gr_text "24.5 mm" (at 83.15 89.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 87 102) (xy 81.8 102)))
    (feature2 (pts (xy 87 77.5) (xy 81.8 77.5)))
    (crossbar (pts (xy 84.5 77.5) (xy 84.5 102)))
    (arrow1a (pts (xy 84.5 102) (xy 83.913579 100.873496)))
    (arrow1b (pts (xy 84.5 102) (xy 85.086421 100.873496)))
    (arrow2a (pts (xy 84.5 77.5) (xy 83.913579 78.626504)))
    (arrow2b (pts (xy 84.5 77.5) (xy 85.086421 78.626504)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 34.5 135 270) (layer Dwgs.User))
    (feature1 (pts (xy 37 130) (xy 31.8 130)))
    (feature2 (pts (xy 37 126.5) (xy 31.8 126.5)))
    (crossbar (pts (xy 34.5 126.5) (xy 34.5 130)))
    (arrow1a (pts (xy 34.5 130) (xy 33.913579 128.873496)))
    (arrow1b (pts (xy 34.5 130) (xy 35.086421 128.873496)))
    (arrow2a (pts (xy 34.5 126.5) (xy 33.913579 127.626504)))
    (arrow2b (pts (xy 34.5 126.5) (xy 35.086421 127.626504)))
  )
  (dimension 49 (width 0.15) (layer Dwgs.User)
    (gr_text "49.0 mm" (at 110.35 102 270) (layer Dwgs.User))
    (feature1 (pts (xy 104 126.5) (xy 111.7 126.5)))
    (feature2 (pts (xy 104 77.5) (xy 111.7 77.5)))
    (crossbar (pts (xy 109 77.5) (xy 109 126.5)))
    (arrow1a (pts (xy 109 126.5) (xy 108.413579 125.373496)))
    (arrow1b (pts (xy 109 126.5) (xy 109.586421 125.373496)))
    (arrow2a (pts (xy 109 77.5) (xy 108.413579 78.626504)))
    (arrow2b (pts (xy 109 77.5) (xy 109.586421 78.626504)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 46.5 134) (layer Dwgs.User))
    (feature1 (pts (xy 41.5 131) (xy 41.5 136.7)))
    (feature2 (pts (xy 38 131) (xy 38 136.7)))
    (crossbar (pts (xy 38 134) (xy 41.5 134)))
    (arrow1a (pts (xy 41.5 134) (xy 40.373496 134.586421)))
    (arrow1b (pts (xy 41.5 134) (xy 40.373496 133.413579)))
    (arrow2a (pts (xy 38 134) (xy 39.126504 134.586421)))
    (arrow2b (pts (xy 38 134) (xy 39.126504 133.413579)))
  )
  (gr_text 33 (at 92.864 120) (layer B.SilkS))
  (gr_text 34 (at 95.15 119.974) (layer B.SilkS))
  (dimension 56 (width 0.15) (layer Dwgs.User)
    (gr_text "56.0 mm" (at 114.35 102 270) (layer Dwgs.User))
    (feature1 (pts (xy 104 130) (xy 115.7 130)))
    (feature2 (pts (xy 104 74) (xy 115.7 74)))
    (crossbar (pts (xy 113 74) (xy 113 130)))
    (arrow1a (pts (xy 113 130) (xy 112.413579 128.873496)))
    (arrow1b (pts (xy 113 130) (xy 113.586421 128.873496)))
    (arrow2a (pts (xy 113 74) (xy 112.413579 75.126504)))
    (arrow2b (pts (xy 113 74) (xy 113.586421 75.126504)))
  )
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 70.5 67.650001) (layer Dwgs.User))
    (feature1 (pts (xy 38 73) (xy 38 66.300001)))
    (feature2 (pts (xy 103 73) (xy 103 66.300001)))
    (crossbar (pts (xy 103 69.000001) (xy 38 69.000001)))
    (arrow1a (pts (xy 38 69.000001) (xy 39.126504 68.41358)))
    (arrow1b (pts (xy 38 69.000001) (xy 39.126504 69.586422)))
    (arrow2a (pts (xy 103 69.000001) (xy 101.873496 68.41358)))
    (arrow2b (pts (xy 103 69.000001) (xy 101.873496 69.586422)))
  )
  (gr_text "C.Schnarel\n2017JUN26\nRev 1.0beta" (at 89.562 99.146 90) (layer B.Cu))
  (gr_text "pi-top Glimmer" (at 46.5 80.096) (layer F.SilkS))
  (gr_arc (start 100 77) (end 100 74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100 127) (end 103 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 41 127) (end 41 130) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 41 77) (end 38 77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38 127) (end 38 77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 130) (end 41 130) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103 77) (end 103 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41 74) (end 100 74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 34) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 38 74) (xy 103 74) (xy 103 130) (xy 38 130)
      )
    )
  )
  (zone (net 34) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 38 130) (xy 38 74) (xy 103 74) (xy 103 130)
      )
    )
  )
  (zone (net 34) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 38 129.88) (xy 38 74) (xy 103.024 74) (xy 103.024 129.88)
      )
    )
  )
  (zone (net 34) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 38 129.88) (xy 38 74) (xy 103.024 74) (xy 103.024 129.88)
      )
    )
  )
)
