(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 102)
    (no_connects 0)
    (area 146.2322 74.214999 232.503321 133.152476)
    (thickness 1.6)
    (drawings 4)
    (tracks 636)
    (zones 0)
    (modules 31)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 /ETH_NETPWR)
  (net 7 /SBB_DATA+)
  (net 8 /SBB_DATA-)
  (net 9 /ETH_TX+)
  (net 10 /ETH_TX-)
  (net 11 /ETH_RX+)
  (net 12 /ETH_RX-)
  (net 13 "Net-(J3-Pad9)")
  (net 14 /ETH_L1)
  (net 15 "Net-(J3-Pad11)")
  (net 16 /ETH_L2)
  (net 17 /Omega_RX)
  (net 18 /Omega_TX)
  (net 19 /I2C_SCL)
  (net 20 /I2C_SDA)
  (net 21 /G9)
  (net 22 /G19)
  (net 23 /G8)
  (net 24 /G17)
  (net 25 /G16)
  (net 26 /Omega_TX1)
  (net 27 /Omega_RX1)
  (net 28 "Net-(P6-Pad3)")
  (net 29 "Net-(P6-Pad4)")
  (net 30 /RS485_TXEN)
  (net 31 /RS485_RXEN)
  (net 32 /TOUCH_RST)
  (net 33 /TOUCH_CHG)
  (net 34 /ETH_PWR+)
  (net 35 /ETH_PWR-)
  (net 36 /I2C_SCL1)
  (net 37 /I2C_SCL2)
  (net 38 /RESET_BTN)
  (net 39 /TOUCH_SEL)
  (net 40 "Net-(U4-Pad13)")
  (net 41 "Net-(U4-Pad4)")
  (net 42 "Net-(MH1-Pad1)")
  (net 43 "Net-(MH2-Pad1)")
  (net 44 "Net-(P2-Pad2)")
  (net 45 "Net-(P2-Pad3)")
  (net 46 "Net-(P2-Pad6)")
  (net 47 "Net-(U1-PadB3)")
  (net 48 "Net-(U1-PadB4)")
  (net 49 "Net-(U1-PadA2)")
  (net 50 "Net-(U1-PadA16)")
  (net 51 /WS2813_DATA_5V)
  (net 52 /WS2813_DATA_3V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ETH_L1)
    (add_net /ETH_L2)
    (add_net /ETH_NETPWR)
    (add_net /ETH_RX+)
    (add_net /ETH_RX-)
    (add_net /ETH_TX+)
    (add_net /ETH_TX-)
    (add_net /G16)
    (add_net /G17)
    (add_net /G19)
    (add_net /G8)
    (add_net /G9)
    (add_net /I2C_SCL)
    (add_net /I2C_SCL1)
    (add_net /I2C_SCL2)
    (add_net /I2C_SDA)
    (add_net /Omega_RX)
    (add_net /Omega_RX1)
    (add_net /Omega_TX)
    (add_net /Omega_TX1)
    (add_net /RESET_BTN)
    (add_net /RS485_RXEN)
    (add_net /RS485_TXEN)
    (add_net /SBB_DATA+)
    (add_net /SBB_DATA-)
    (add_net /TOUCH_CHG)
    (add_net /TOUCH_RST)
    (add_net /TOUCH_SEL)
    (add_net /WS2813_DATA_3V)
    (add_net /WS2813_DATA_5V)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(MH1-Pad1)")
    (add_net "Net-(MH2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(U1-PadA16)")
    (add_net "Net-(U1-PadA2)")
    (add_net "Net-(U1-PadB3)")
    (add_net "Net-(U1-PadB4)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 1.2)
    (uvia_drill 0.6)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net GND)
  )
  (module plan44-ONION-2MM-2X16 (layer F.Cu) (tedit 588C9D1E)
    (at 183.388 107.95)
    (descr "FOOTPRINT FÜR ONION OMEGA")
    (tags "FOOTPRINT FÜR ONION OMEGA")
    (attr virtual)
    (fp_text reference U1 (at -0.1016 -19.7612) (layer F.SilkS))
    (fp_text value ONION-OMEGA2 (at -4.9276 -19.6596) (layer F.Fab))
    (pad B1 thru_hole rect (at 12.39774 -13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad B2 thru_hole circle (at 12.39774 -11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +3V3))
    (pad B3 thru_hole circle (at 12.39774 -9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 47 "Net-(U1-PadB3)"))
    (pad B4 thru_hole circle (at 12.39774 -7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 48 "Net-(U1-PadB4)"))
    (pad B5 thru_hole circle (at 12.39774 -5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 17 /Omega_RX))
    (pad B6 thru_hole circle (at 12.39774 -3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 18 /Omega_TX))
    (pad B7 thru_hole circle (at 12.39774 -1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 38 /RESET_BTN))
    (pad B8 thru_hole circle (at 12.39774 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad B9 thru_hole circle (at 12.39774 1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH_TX-))
    (pad B10 thru_hole circle (at 12.39774 3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH_TX+))
    (pad B11 thru_hole circle (at 12.39774 5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /ETH_RX-))
    (pad B12 thru_hole circle (at 12.39774 7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 /ETH_RX+))
    (pad B13 thru_hole circle (at 12.39774 9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 52 /WS2813_DATA_3V))
    (pad B14 thru_hole circle (at 12.39774 11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 22 /G19))
    (pad B15 thru_hole circle (at 12.39774 13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 19 /I2C_SCL))
    (pad B16 thru_hole circle (at 12.39774 15.99946) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 20 /I2C_SDA))
    (pad A1 thru_hole rect (at -11.99896 -13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad A2 thru_hole circle (at -11.99896 -11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 49 "Net-(U1-PadA2)"))
    (pad A3 thru_hole circle (at -11.99896 -9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 30 /RS485_TXEN))
    (pad A4 thru_hole circle (at -11.99896 -7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 /RS485_RXEN))
    (pad A5 thru_hole circle (at -11.99896 -5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 /G17))
    (pad A6 thru_hole circle (at -11.99896 -3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /G16))
    (pad A7 thru_hole circle (at -11.99896 -1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 33 /TOUCH_CHG))
    (pad A8 thru_hole circle (at -11.99896 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 26 /Omega_TX1))
    (pad A9 thru_hole circle (at -11.99896 1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /Omega_RX1))
    (pad A10 thru_hole circle (at -11.99896 3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 21 /G9))
    (pad A11 thru_hole circle (at -11.99896 5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 23 /G8))
    (pad A12 thru_hole circle (at -11.99896 7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 39 /TOUCH_SEL))
    (pad A13 thru_hole circle (at -11.99896 9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 32 /TOUCH_RST))
    (pad A14 thru_hole circle (at -11.99896 11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 14 /ETH_L1))
    (pad A15 thru_hole circle (at -11.99896 13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /ETH_L2))
    (pad A16 thru_hole circle (at -11.99896 15.99946) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 50 "Net-(U1-PadA16)"))
  )
  (module plan44:plan44-HLJ-6115ANL (layer F.Cu) (tedit 581B6BD3)
    (at 209.042 90.678)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J3 (at -1.27 -4.318 180) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.90754 2.9591 180) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 /ETH_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /ETH_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 34 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 35 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 13 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 14 /ETH_L1))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 15 "Net-(J3-Pad11)"))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /ETH_L2))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module plan44-Recom-R78Cxx (layer F.Cu) (tedit 588C9BE9)
    (at 167.894 94.742 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U2 (at 2.4892 4.2672 270) (layer F.SilkS))
    (fp_text value Recom_R78Cxx (at 2.4 -3.2 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module plan44:plan44-STELVIO-4P-508 (layer F.Cu) (tedit 588C9BA7)
    (at 159.004 120.904 90)
    (attr virtual)
    (fp_text reference J2 (at 17.5768 -0.1524 180) (layer F.SilkS))
    (fp_text value SBB (at 7.62 -11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 /SBB_DATA+))
    (pad 4 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 /SBB_DATA-))
  )
  (module plan44:plan44-STELVIO-2P-508 (layer F.Cu) (tedit 588C9BB3)
    (at 159.004 109.22 90)
    (attr virtual)
    (fp_text reference J1 (at 17.7292 0.0508 180) (layer F.SilkS))
    (fp_text value STELVIO-2P-508 (at 12.7 -11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 +5V))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57FE27BF)
    (at 214.376 127.254 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57FE27FA)
    (at 169.672 85.598 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 209.55 115.316)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57FE27EC)
    (at 196.85 90.17 90)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 588C997E)
    (at 191.008 119.38 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 2.5908 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 588C9978)
    (at 182.372 119.38 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 2.5908 -0.1524 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57FE27C7)
    (at 209.804 103.378)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 588C9BCE)
    (at 159.766 128.016 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.5908 0 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /WS2813_DATA_5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer F.Cu) (tedit 57FE27F6)
    (at 176.53 85.09 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.254 -2.794 90) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P2-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03 (layer F.Cu) (tedit 57FE27B1)
    (at 209.55 106.68)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -2.286 0 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /I2C_SCL1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /TOUCH_RST))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /I2C_SDA))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /TOUCH_CHG))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03 (layer F.Cu) (tedit 57FE27B9)
    (at 209.55 118.618)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /I2C_SCL2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /TOUCH_RST))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /I2C_SDA))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /TOUCH_CHG))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 588C99DE)
    (at 201.168 110.49)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -2.6924 0.1016 90) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /RESET_BTN))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /G9))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /G19))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /G8))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /G17))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /G16))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57FE2828)
    (at 164.338 113.538)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -2.54 -0.254 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /Omega_TX1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /Omega_RX1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /Omega_TX))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /Omega_RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 588C99CF)
    (at 201.168 106.172 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0.0508 -2.7432 90) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /ETH_PWR-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 165.608 123.444 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ADM3485E (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 /SBB_DATA-))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 /SBB_DATA+))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P6-Pad3)"))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 /RS485_TXEN))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 /RS485_RXEN))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P6-Pad4)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10BF)
    (at 177.8 109.22)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 /ETH_TX+))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10C6)
    (at 177.8 114.046)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 /ETH_TX-))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10CB)
    (at 178.308 104.14)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 /ETH_RX+))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10D1)
    (at 178.308 100.838)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.08 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 /ETH_RX-))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10DF)
    (at 188.468 91.186 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.334 0 180) (layer F.SilkS))
    (fp_text value 1k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(J3-Pad9)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57FE10D8)
    (at 188.468 94.488 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1k (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(J3-Pad11)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57FE2A1A)
    (at 160.02 87.63)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(MH1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57FE2A14)
    (at 202.438 126.492)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(MH2-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D7.5_L11.2_P2.5 (layer F.Cu) (tedit 588C9BE0)
    (at 165.608 108.712 90)
    (descr "Radial Electrolytic Capacitor Diameter 7.5mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at 0.1524 2.3368 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 5.1 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D7.5_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791)
    (at 183.388 125.476 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -5.375 270) (layer F.SilkS))
    (fp_text value 7400 (at 0 5.375 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /I2C_SCL))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /I2C_SCL))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad13)"))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad13)"))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /I2C_SCL1))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad4)"))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TOUCH_SEL))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TOUCH_SEL))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /I2C_SCL2))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TOUCH_SEL))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 588C9996)
    (at 173.99 127.762 180)
    (descr SOT353)
    (attr smd)
    (fp_text reference U5 (at 0.1016 2.032 360) (layer F.SilkS))
    (fp_text value 74AHCT1G125 (at 0.09906 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -1.016 0 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 52 /WS2813_DATA_3V))
    (pad 4 smd rect (at 1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 51 /WS2813_DATA_5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 217.932 83.82) (end 156.464 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 130.302) (end 156.464 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.932 130.302) (end 156.464 130.302) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.932 83.82) (end 217.932 130.302) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 84.836) (xy 216.916 84.836) (xy 216.916 129.54) (xy 157.48 129.286) (xy 157.48 126.746)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 84.836) (xy 216.916 84.836) (xy 216.916 129.54) (xy 157.48 129.286) (xy 157.48 126.746)
      )
    )
  )
)
