(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "GNS589x Carrier")
		(date "2024-03-03")
		(rev "1.0")
		(company "Wegmatt LLC")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010f8_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "/RF_VDD")
	(net 2 "GND")
	(net 3 "/VSYS")
	(net 4 "/GNS_FRAME")
	(net 5 "/RF_IN")
	(net 6 "/PICO_IO3")
	(net 7 "/GNS_RX")
	(net 8 "/GNS_CTS")
	(net 9 "/~{GNS_RESET}")
	(net 10 "/GNS_TX")
	(net 11 "/PICO_IO2")
	(net 12 "/PICO_TX")
	(net 13 "/SWDIO")
	(net 14 "/VBATT")
	(net 15 "/PICO_RX")
	(net 16 "/EN")
	(net 17 "/~{PICO_RST}")
	(net 18 "/SWCLK")
	(net 19 "/GNS_RTS")
	(net 20 "Net-(Q1-G)")
	(net 21 "/VBUS")
	(net 22 "unconnected-(U2-NC-Pad4)")
	(net 23 "unconnected-(U3-GPIO16-Pad21)")
	(net 24 "unconnected-(U3-GPIO27_ADC1-Pad32)")
	(net 25 "unconnected-(U3-GPIO21-Pad27)")
	(net 26 "unconnected-(U3-GPIO17-Pad22)")
	(net 27 "unconnected-(U3-GPIO19-Pad25)")
	(net 28 "unconnected-(U3-3V3-Pad36)")
	(net 29 "unconnected-(U3-GPIO22-Pad29)")
	(net 30 "unconnected-(U3-GPIO28_ADC2-Pad34)")
	(net 31 "unconnected-(U3-GPIO10-Pad14)")
	(net 32 "unconnected-(U3-GPIO11-Pad15)")
	(net 33 "unconnected-(U3-GPIO20-Pad26)")
	(net 34 "unconnected-(U3-ADC_VREF-Pad35)")
	(net 35 "unconnected-(U3-GPIO18-Pad24)")
	(net 36 "unconnected-(U3-GPIO26_ADC0-Pad31)")
	(net 37 "unconnected-(U3-GPIO14-Pad19)")
	(net 38 "unconnected-(U3-GPIO12-Pad16)")
	(net 39 "unconnected-(U3-GPIO13-Pad17)")
	(net 40 "unconnected-(U3-GPIO15-Pad20)")
	(net 41 "/RF_GND")
	(net 42 "Net-(D1-K)")
	(net 43 "Net-(D2-K)")
	(footprint "_project:SMA-Edge"
		(layer "F.Cu")
		(at 107.53 114.59 180)
		(property "Reference" "J1"
			(at 0 1 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 -5.5 180)
			(layer "F.Fab")
		)
		(property "Footprint" "_project:SMA-Edge"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(solder_paste_ratio -1)
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -2.25 180)
			(size 1 4.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/RF_IN")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.75 -2.25 180)
			(size 1.5 4.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/RF_GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.75 -2.25 180)
			(size 1.5 4.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "/RF_GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2.25 180)
			(size 1.5 4.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/RF_GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.75 -2.25 180)
			(size 1.5 4.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "/RF_GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/_project.pretty/SMA-J-P-H-ST-EM1.stp"
			(offset
				(xyz 0 6.4 0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 -90 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x13_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88.9 76.2)
		(descr "Through hole straight pin header, 1x13, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x13 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x16"
			(at 0 32.81 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x13_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 15.24 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/VBATT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/EN")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/PICO_RX")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/PICO_TX")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/PICO_IO2")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/PICO_IO3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GNS_RX")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/GNS_TX")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/GNS_CTS")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/GNS_RTS")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/~{GNS_RESET}")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/GNS_FRAME")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x13_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 146.6 89 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 180)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/RF_VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 98.1 116.8 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 2.48 0.0075 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/RF_VDD")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 96.2 116.8 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 2.5 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/GNS_FRAME")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 149.86 101.6)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 9.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/~{PICO_RST}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SWCLK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SWDIO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 88.9 68.58)
		(descr "Mounting Hole 2.5mm, no annular")
		(tags "mounting hole 2.5mm no annular")
		(property "Reference" "H1"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 146.6 86.1 -90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "MIC5504-3.3YM5"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MIC550X.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "300mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?5*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/VSYS")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/EN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "unconnected-(U2-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/RF_VDD")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 88.9 116.84)
		(descr "Mounting Hole 2.5mm, no annular")
		(tags "mounting hole 2.5mm no annular")
		(property "Reference" "H4"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.5 80.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0.1 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113.3 98.7 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/RF_VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 99.7 116.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 115 98.7 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/RF_VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 149.86 68.58)
		(descr "Mounting Hole 2.5mm, no annular")
		(tags "mounting hole 2.5mm no annular")
		(property "Reference" "H2"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 94.6 116.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.4 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 149.86 116.84)
		(descr "Mounting Hole 2.5mm, no annular")
		(tags "mounting hole 2.5mm no annular")
		(property "Reference" "H3"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.4 85.3 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/VSYS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 147 83.1)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -2.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/VSYS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "_project:RPi_Pico_SMD_NoSilk"
		(layer "F.Cu")
		(at 130.9 91.6)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "U3"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pico"
			(at 0 2.159 0)
			(layer "F.Fab")
		)
		(property "Footprint" "_project:RPi_Pico_SMD_NoSilk"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(solder_paste_ratio -1)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at -2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 15 "/PICO_RX")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 12 "/PICO_TX")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 11 "/PICO_IO2")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 6 "/PICO_IO3")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 7 "/GNS_RX")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 10 "/GNS_TX")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at -8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 8 "/GNS_CTS")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 19 "/GNS_RTS")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 9 "/~{GNS_RESET}")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 4 "/GNS_FRAME")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at -8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 31 "unconnected-(U3-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 32 "unconnected-(U3-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 38 "unconnected-(U3-GPIO12-Pad16)")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 39 "unconnected-(U3-GPIO13-Pad17)")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 37 "unconnected-(U3-GPIO14-Pad19)")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 40 "unconnected-(U3-GPIO15-Pad20)")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 23 "unconnected-(U3-GPIO16-Pad21)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 26 "unconnected-(U3-GPIO17-Pad22)")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" smd rect
			(at 8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 35 "unconnected-(U3-GPIO18-Pad24)")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 27 "unconnected-(U3-GPIO19-Pad25)")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 33 "unconnected-(U3-GPIO20-Pad26)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 25 "unconnected-(U3-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at 8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 29 "unconnected-(U3-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 17 "/~{PICO_RST}")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "31" smd rect
			(at 8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 36 "unconnected-(U3-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 24 "unconnected-(U3-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 30 "unconnected-(U3-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at 8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 34 "unconnected-(U3-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "unspecified")
		)
		(pad "36" smd rect
			(at 8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 28 "unconnected-(U3-3V3-Pad36)")
			(pinfunction "3V3")
			(pintype "unspecified")
		)
		(pad "37" smd rect
			(at 8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 16 "/EN")
			(pinfunction "3V3_EN")
			(pintype "input")
		)
		(pad "38" smd rect
			(at 8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "/VSYS")
			(pinfunction "VSYS")
			(pintype "unspecified")
		)
		(pad "40" smd rect
			(at 8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 21 "/VBUS")
			(pinfunction "VBUS")
			(pintype "unspecified")
		)
		(pad "41" smd rect
			(at -2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 18 "/SWCLK")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(pad "42" smd rect
			(at 0 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" smd rect
			(at 2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 13 "/SWDIO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 127.1 66.6) (xy 134.7 66.6) (xy 134.7 71.5) (xy 127.1 71.5)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 127.3 73) (xy 129.5 73) (xy 129.5 80.2) (xy 127.3 80.2)
				)
			)
		)
		(model "${KIPRJMOD}/_project.pretty/Pico.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "_project:GNS589x"
		(layer "F.Cu")
		(at 102.2 94.14 90)
		(property "Reference" "U1"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "GNS5892R"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "_project:GNS589x"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.gns-electronics.de/wp-content/uploads/2021/06/GNS5892R_ADSBModul_datasheet_V10.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "low-power low-cost ADS-B receiver"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(solder_paste_ratio -1)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -11.43 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/RF_GND")
			(pinfunction "RF_GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -8.89 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/RF_IN")
			(pinfunction "RF_IN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -6.35 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.81 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/RF_VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -1.27 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GNS_FRAME")
			(pinfunction "F_IND")
			(pintype "output")
		)
		(pad "6" smd rect
			(at 1.27 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/~{GNS_RESET}")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 3.81 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/GNS_RTS")
			(pinfunction "RTS")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 6.35 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/GNS_CTS")
			(pinfunction "CTS")
			(pintype "input")
		)
		(pad "9" smd rect
			(at 8.89 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/GNS_TX")
			(pinfunction "UART_TX")
			(pintype "output")
		)
		(pad "10" smd rect
			(at 11.43 7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/GNS_RX")
			(pinfunction "UART_RX")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 12.38 5.1 90)
			(size 2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "12" smd rect
			(at 12.38 4 90)
			(size 2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "13" smd rect
			(at 12.38 2.9 90)
			(size 2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "14" smd rect
			(at 12.38 1.8 90)
			(size 2 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "MP" smd rect
			(at -13 0 180)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -11.43 -7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 11.43 -7.62 90)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 13 0 180)
			(size 1.75 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/_project.pretty/5892R.STP"
			(offset
				(xyz 3.81 -1.1 1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 146.8 79.9 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178D.PDF inferred 3-pin variant), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.4 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Q_PMOS_GSD"
			(at 0 2.4 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "P-MOSFET transistor, gate/source/drain"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/VSYS")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/VBATT")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.5 77.7 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 1.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "GNS589x-carrier.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/VBUS")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 152.4 68.04)
		(end 152.4 117.38)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 86.36 68.04)
		(mid 86.945786 66.625786)
		(end 88.36 66.04)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.36 117.38)
		(end 86.36 68.04)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.4 117.38)
		(mid 151.814214 118.794214)
		(end 150.4 119.38)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.4 66.04)
		(mid 151.814214 66.625786)
		(end 152.4 68.04)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.36 66.04)
		(end 150.4 66.04)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.36 119.38)
		(mid 86.945786 118.794214)
		(end 86.36 117.38)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.4 119.38)
		(end 88.36 119.38)
		(layer "Edge.Cuts")
	)
	(gr_text "TX >"
		(at 90.3 96.4 0)
		(layer "B.SilkS")
	)
	(gr_text "RTS >"
		(at 90.3 101.6 0)
		(layer "B.SilkS")
	)
	(gr_text "RX <"
		(at 90.3 83.8 0)
		(layer "B.SilkS")
	)
	(gr_text "IO2"
		(at 90.3 88.9 0)
		(layer "B.SilkS")
	)
	(gr_text "~{RESET}"
		(at 90.3 104.2 0)
		(layer "B.SilkS")
	)
	(gr_text "PICO DEBUG"
		(at 141.736905 105.5 90)
		(layer "B.SilkS")
	)
	(gr_text "FRAME"
		(at 90.3 106.7 0)
		(layer "B.SilkS")
	)
	(gr_text "CTS <"
		(at 90.3 99 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 148.5 101.6 0)
		(layer "B.SilkS")
	)
	(gr_text "3.5V-5.5V"
		(at 90.3 76.2 0)
		(layer "B.SilkS")
	)
	(gr_text "IO3"
		(at 90.3 91.4 0)
		(layer "B.SilkS")
	)
	(gr_text "SWCLK"
		(at 148.5 106.7 0)
		(layer "B.SilkS")
	)
	(gr_text "ADSB-MODULE"
		(at 97.1 100.4 270)
		(layer "B.SilkS")
	)
	(gr_text "ENABLE"
		(at 90.3 81.3 0)
		(layer "B.SilkS")
	)
	(gr_text "RX <"
		(at 90.3 93.9 0)
		(layer "B.SilkS")
	)
	(gr_text "©2024 Wegmatt LLC"
		(at 150.7 79.8 0)
		(layer "B.SilkS")
	)
	(gr_text "GNS589x ADS-B Carrier"
		(at 150.7 76.4 0)
		(layer "B.SilkS")
	)
	(gr_text "~{RST}"
		(at 148.5 104.1 0)
		(layer "B.SilkS")
	)
	(gr_text "v${REVISION}"
		(at 104.8 79.8 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 90.3 78.7 0)
		(layer "B.SilkS")
	)
	(gr_text "PICO I/O"
		(at 97.063095 87.6 270)
		(layer "B.SilkS")
	)
	(gr_text "SWDIO"
		(at 148.5 109.2 0)
		(layer "B.SilkS")
	)
	(gr_text "TX >"
		(at 90.3 86.3 0)
		(layer "B.SilkS")
	)
	(gr_text "ADS-B"
		(at 96.2 115.1 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "POWER"
		(at 98.1 115.1 90)
		(layer "F.SilkS" knockout)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 88.9 68.58) (xy 88.9 76.2)
		)
		(height 8.128)
		(gr_text "0.30 in"
			(at 79.622 72.39 90)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 86.36 119.38) (xy 107.442 119.38)
		)
		(height 11.684)
		(gr_text "0.83 in"
			(at 96.901 129.914 0)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 86.36 119.38) (xy 152.4 119.38)
		)
		(height 8.62)
		(gr_text "2.60 in"
			(at 119.38 126.85 0)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 152.4 66.04) (xy 152.4 119.38)
		)
		(height -9.1)
		(gr_text "2.10 in"
			(at 160.35 92.71 90)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 88.9 116.84) (xy 149.86 116.84)
		)
		(height 6.86)
		(gr_text "2.40 in"
			(at 119.38 122.55 0)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 149.86 68.58) (xy 149.86 116.84)
		)
		(height -7.24)
		(gr_text "1.90 in"
			(at 155.95 92.71 90)
			(layer "User.1")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 86.36 66.04) (xy 152.4 66.04) (xy 152.4 119.38) (xy 86.36 119.38)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/RF_GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 103.8 119.4) (xy 103.8 104.4) (xy 106.6 101.6) (xy 113 101.6) (xy 113 112.7) (xy 111.2 114.5)
				(xy 111.2 119.4)
			)
		)
	)
)