(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 15)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P2-Pad1)")
  (net 4 "Net-(P2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
  )
  (module encoder:Potentiometer_Trimmer-EVM3S_R (layer F.Cu) (tedit 5BFA3248)
    (at 148.5392 106.934)
    (descr http://www.comkey.in/sites/default/files/attachments/EVM3ESX50B15.pdf)
    (tags "trimmer SMD")
    (attr smd)
    (fp_text reference SW1 (at -22.75 4.956) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at -20.066 -9.652) (layer F.Fab))
    (pad 4 thru_hole circle (at -2.5 -7.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 5 thru_hole circle (at 2.5 -7.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at -2.5 7) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(P2-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 7) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at 0 7) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5E23B940)
    (at 147.32 111.76 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.794 -21.59 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -0.508 -24.384 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5E23B932)
    (at 147.32 101.6 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 6.604 -21.336 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.762 -22.098 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(P2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module osh-logo:osh-logo_silkscreen-back_4mm (layer B.Cu) (tedit 0)
    (at 147.2184 106.8832 270)
    (fp_text reference G*** (at 0 -2.1209 270) (layer B.SilkS) hide)
    (fp_text value osh-logo_silkscreen-back_4mm (at 0 2.1209 270) (layer B.SilkS) hide)
  )
  (gr_text enc2pi (at 150.5458 106.7562 90) (layer B.SilkS))
  (gr_text mincepi (at 148.3614 106.9848 90) (layer F.SilkS))
  (gr_line (start 144.78 98.044) (end 144.78 115.3922) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 152.4 98.044) (end 144.78 98.044) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 152.4 115.3922) (end 152.4 98.044) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 144.78 115.3922) (end 152.4 115.3922) (angle 90) (layer Edge.Cuts) (width 0.0254))
)
