<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<hole x="28.75" y="75" drill="3"/>
<hole x="128.75" y="75" drill="3"/>
<wire x1="-4" y1="80" x2="-4" y2="38" width="0.0762" layer="20"/>
<wire x1="-4" y1="38" x2="161.5" y2="38" width="0.0762" layer="20"/>
<wire x1="161.5" y1="38" x2="161.5" y2="80" width="0.0762" layer="20"/>
<wire x1="161.5" y1="80" x2="-4" y2="80" width="0.0762" layer="20"/>
<wire x1="-4" y1="80" x2="-3.66651875" y2="79.66348125" width="0.0762" layer="20"/>
<wire x1="-3.66651875" y1="79.66348125" x2="-3.66651875" y2="77.83021875" width="0.0762" layer="20"/>
<wire x1="-3.66651875" y1="77.83021875" x2="-2.666559375" y2="77.83021875" width="0.0762" layer="20"/>
<hole x="45.5" y="42" drill="3"/>
<hole x="112" y="42" drill="3"/>
<wire x1="-3.999840625" y1="58.331" x2="-3.999840625" y2="59.9976" width="0.008" layer="46"/>
<text>For 4 pin LED Tape   ...   Jeremy Wagner</text>
<text>For 4 pin LED Tape   ...   Jeremy Wagner</text>
<hole x="0" y="58.75" drill="3.16"/>
<hole x="157.5" y="58.75" drill="3.16"/>
<wire x1="0" y1="57.16438125" x2="157.4937" y2="57.16438125" width="0.008" layer="20"/>
<wire x1="157.4937" y1="57.16438125" x2="157.4937" y2="60.33091875" width="0.008" layer="20"/>
<wire x1="0" y1="60.33091875" x2="157.4937" y2="60.33091875" width="0.008" layer="20"/>
<wire x1="0" y1="57.16438125" x2="0" y2="60.33091875" width="0.008" layer="20"/>
</plain>
<libraries>
<library name="LED_TAPE_SMD">
<packages>
<package name="LED-TAPE">
<description>Termination for 4 conductor LED Tape</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$5" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$6" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$7" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$8" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$9" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$10" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$11" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$12" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$13" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$14" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$15" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$16" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$17" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$18" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$19" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$20" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$21" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$22" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$23" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="U$24" library="LED_TAPE_SMD" package="LED-TAPE" value="LED-TAPE"/>
<element name="GND" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B0" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D0" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+12V" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+12" library="wirepad" package="3,81/1,4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$6" pad="GND"/>
<contactref element="U$5" pad="GND"/>
</signal>
<signal name="N$2">
<contactref element="U$6" pad="B0"/>
<contactref element="U$5" pad="B0"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="D0"/>
<contactref element="U$5" pad="D0"/>
</signal>
<signal name="N$4">
<contactref element="U$6" pad="+12V"/>
<contactref element="U$5" pad="+12V"/>
</signal>
<signal name="N$5">
<contactref element="U$7" pad="GND"/>
<contactref element="U$8" pad="GND"/>
</signal>
<signal name="N$6">
<contactref element="U$7" pad="B0"/>
<contactref element="U$8" pad="B0"/>
</signal>
<signal name="N$7">
<contactref element="U$7" pad="D0"/>
<contactref element="U$8" pad="D0"/>
</signal>
<signal name="N$8">
<contactref element="U$7" pad="+12V"/>
<contactref element="U$8" pad="+12V"/>
</signal>
<signal name="N$9">
<contactref element="U$9" pad="GND"/>
<contactref element="U$10" pad="GND"/>
</signal>
<signal name="N$10">
<contactref element="U$9" pad="B0"/>
<contactref element="U$10" pad="B0"/>
</signal>
<signal name="N$11">
<contactref element="U$9" pad="D0"/>
<contactref element="U$10" pad="D0"/>
</signal>
<signal name="N$12">
<contactref element="U$9" pad="+12V"/>
<contactref element="U$10" pad="+12V"/>
</signal>
<signal name="N$13">
<contactref element="U$11" pad="GND"/>
<contactref element="U$12" pad="GND"/>
</signal>
<signal name="N$14">
<contactref element="U$11" pad="B0"/>
<contactref element="U$12" pad="B0"/>
</signal>
<signal name="N$15">
<contactref element="U$11" pad="D0"/>
<contactref element="U$12" pad="D0"/>
</signal>
<signal name="N$16">
<contactref element="U$11" pad="+12V"/>
<contactref element="U$12" pad="+12V"/>
</signal>
<signal name="N$17">
<contactref element="U$13" pad="GND"/>
<contactref element="U$14" pad="GND"/>
</signal>
<signal name="N$18">
<contactref element="U$13" pad="B0"/>
<contactref element="U$14" pad="B0"/>
</signal>
<signal name="N$19">
<contactref element="U$13" pad="D0"/>
<contactref element="U$14" pad="D0"/>
</signal>
<signal name="N$20">
<contactref element="U$13" pad="+12V"/>
<contactref element="U$14" pad="+12V"/>
</signal>
<signal name="N$21">
<contactref element="U$15" pad="GND"/>
<contactref element="U$16" pad="GND"/>
</signal>
<signal name="N$22">
<contactref element="U$15" pad="B0"/>
<contactref element="U$16" pad="B0"/>
</signal>
<signal name="N$23">
<contactref element="U$15" pad="D0"/>
<contactref element="U$16" pad="D0"/>
</signal>
<signal name="N$24">
<contactref element="U$15" pad="+12V"/>
<contactref element="U$16" pad="+12V"/>
</signal>
<signal name="N$25">
<contactref element="U$17" pad="GND"/>
<contactref element="U$18" pad="GND"/>
</signal>
<signal name="N$26">
<contactref element="U$17" pad="B0"/>
<contactref element="U$18" pad="B0"/>
</signal>
<signal name="N$27">
<contactref element="U$17" pad="D0"/>
<contactref element="U$18" pad="D0"/>
</signal>
<signal name="N$28">
<contactref element="U$17" pad="+12V"/>
<contactref element="U$18" pad="+12V"/>
</signal>
<signal name="N$29">
<contactref element="U$19" pad="GND"/>
<contactref element="U$20" pad="GND"/>
</signal>
<signal name="N$30">
<contactref element="U$19" pad="B0"/>
<contactref element="U$20" pad="B0"/>
</signal>
<signal name="N$31">
<contactref element="U$19" pad="D0"/>
<contactref element="U$20" pad="D0"/>
</signal>
<signal name="N$32">
<contactref element="U$19" pad="+12V"/>
<contactref element="U$20" pad="+12V"/>
</signal>
<signal name="N$33">
<contactref element="U$21" pad="GND"/>
<contactref element="U$22" pad="GND"/>
</signal>
<signal name="N$34">
<contactref element="U$21" pad="B0"/>
<contactref element="U$22" pad="B0"/>
</signal>
<signal name="N$35">
<contactref element="U$21" pad="D0"/>
<contactref element="U$22" pad="D0"/>
</signal>
<signal name="N$36">
<contactref element="U$21" pad="+12V"/>
<contactref element="U$22" pad="+12V"/>
</signal>
<signal name="N$37">
<contactref element="U$23" pad="GND"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U$23" pad="B0"/>
<contactref element="B0" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U$23" pad="D0"/>
<contactref element="D0" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="U$23" pad="+12V"/>
<contactref element="+12V" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="G" pad="1"/>
<contactref element="U$24" pad="GND"/>
</signal>
<signal name="N$42">
<contactref element="B" pad="1"/>
<contactref element="U$24" pad="B0"/>
</signal>
<signal name="N$43">
<contactref element="D" pad="1"/>
<contactref element="U$24" pad="D0"/>
</signal>
<signal name="N$44">
<contactref element="+12" pad="1"/>
<contactref element="U$24" pad="+12V"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
