(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 76)
    (no_connects 1)
    (area 98.576001 112.616 174.22 162.212001)
    (thickness 1.6)
    (drawings 15)
    (tracks 321)
    (zones 0)
    (modules 39)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.3302)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.4 2.55)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 118.364 121.412)
    (grid_origin 118.364 121.412)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Plot/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 VCC)
  (net 9 Vdd)
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C9-Pad2)")
  (net 12 "Net-(C10-Pad1)")
  (net 13 "Net-(C10-Pad2)")
  (net 14 "Net-(C11-Pad2)")
  (net 15 "Net-(C12-Pad2)")
  (net 16 "Net-(D1-Pad2)")
  (net 17 D-)
  (net 18 D+)
  (net 19 "Net-(P1-Pad4)")
  (net 20 "Net-(R3-Pad2)")
  (net 21 "Net-(R4-Pad2)")
  (net 22 "Net-(R11-Pad1)")
  (net 23 "Net-(S1-Pad2)")
  (net 24 "Net-(S2-Pad2)")
  (net 25 "Net-(S3-Pad2)")
  (net 26 "Net-(S4-Pad2)")
  (net 27 "Net-(S5-Pad2)")
  (net 28 "Net-(U1-Pad14)")
  (net 29 "Net-(S1-Pad4)")
  (net 30 "Net-(S1-Pad3)")
  (net 31 "Net-(S2-Pad4)")
  (net 32 "Net-(S2-Pad3)")
  (net 33 "Net-(S3-Pad4)")
  (net 34 "Net-(S3-Pad3)")
  (net 35 "Net-(S4-Pad4)")
  (net 36 "Net-(S4-Pad3)")
  (net 37 "Net-(S5-Pad4)")
  (net 38 "Net-(S5-Pad3)")
  (net 39 "Net-(U1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S2-Pad2)")
    (add_net "Net-(S2-Pad3)")
    (add_net "Net-(S2-Pad4)")
    (add_net "Net-(S3-Pad2)")
    (add_net "Net-(S3-Pad3)")
    (add_net "Net-(S3-Pad4)")
    (add_net "Net-(S4-Pad2)")
    (add_net "Net-(S4-Pad3)")
    (add_net "Net-(S4-Pad4)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(S5-Pad3)")
    (add_net "Net-(S5-Pad4)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad6)")
    (add_net VCC)
    (add_net Vdd)
  )
  (module ECS-120-20-3X-TR:Crystal (layer B.Cu) (tedit 589F720C)
    (at 141.224 148.59)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, hand-soldering, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.794) (layer B.SilkS))
    (fp_text value Crystal (at 0 -3.55) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0) (size 3.5 1.2) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.75 0) (size 3.5 1.2) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AE5CB1)
    (at 128.778 133.858 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 0.022uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TL3305CF260QG:TL3305CF260QG (layer F.Cu) (tedit 58B0D502)
    (at 142.748 148.336 90)
    (fp_text reference "S4 Vol-" (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value switch (at -0.04 -3.34 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(S4-Pad2)"))
    (pad 4 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(S4-Pad4)"))
    (pad 3 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(S4-Pad3)"))
  )
  (module SJ-3523:CUI_SJ-3523-SMT-TR (layer B.Cu) (tedit 58B0C366)
    (at 120.65 146.812 270)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference J1 (at -7.874 0 360) (layer B.SilkS))
    (fp_text value SJ-3523-SMT-TR (at -2.825 -6.365 270) (layer B.Fab))
    (pad 1 smd rect (at -4.6 -3.675 270) (size 2.4 2.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 2 smd rect (at 4.7 -3.675 270) (size 2.9 2.55) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C10-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at -2.7 3.675 270) (size 2.4 2.55) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C9-Pad2)") (solder_mask_margin 0.2))
    (pad "" np_thru_hole circle (at 3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu))
    (pad "" np_thru_hole circle (at -3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu))
  )
  (module PCM2706:pcm2706-TQFP32-08 (layer F.Cu) (tedit 58B0E26E)
    (at 142.24 134.62)
    (descr "THIN PLASIC QUAD FLAT PACKAGE GRID 0.8 MM")
    (tags "THIN PLASIC QUAD FLAT PACKAGE GRID 0.8 MM")
    (attr smd)
    (fp_text reference U1 (at 3.302 -0.508 90) (layer F.SilkS))
    (fp_text value PCM2706 (at -0.173673 0.590515) (layer F.Fab))
    (pad 11 smd rect (at -0.788353 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 26 smd rect (at 2.409507 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at -1.588453 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 1.609407 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad14)"))
    (pad 23 smd rect (at 4.703127 -2.272065) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad2)"))
    (pad 22 smd rect (at 4.703127 -1.471965) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad2)"))
    (pad 20 smd rect (at 4.703127 0.125695) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 4.703127 2.525995) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 2.409507 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R11-Pad1)"))
    (pad 9 smd rect (at -2.388553 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 5 smd rect (at -3.882073 0.125695) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(S3-Pad4)"))
    (pad 19 smd rect (at 4.703127 0.925795) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(S1-Pad4)"))
    (pad 18 smd rect (at 4.703127 1.725895) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -3.882073 -0.671865) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(S2-Pad4)"))
    (pad 6 smd rect (at -3.882073 0.925795) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -3.882073 1.725895) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(S5-Pad4)"))
    (pad 8 smd rect (at -3.882073 2.525995) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(S4-Pad4)"))
    (pad 3 smd rect (at -3.882073 -1.471965) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 1 smd rect (at -3.882073 -3.072165) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 3.209607 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 10 smd rect (at -1.588453 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 24 smd rect (at 4.703127 -3.072165) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 27 smd rect (at 1.609407 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at -3.882073 -2.272065) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 30 smd rect (at -0.788353 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 32 smd rect (at -2.388553 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 21 smd rect (at 4.703127 -0.671865) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 28 smd rect (at 0.809307 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad1)"))
    (pad 29 smd rect (at 0.011747 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 12 smd rect (at 0.011747 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 13 smd rect (at 0.809307 4.019515) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 25 smd rect (at 3.209607 -4.565685) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D7B7)
    (at 119.634 134.366 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 3.3k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D7C0)
    (at 130.556 128.27 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 16 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58A4FC62)
    (at 121.412 124.46)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 131.826 148.59 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value 20pF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 150.368 148.59)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 20pF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 589D1684)
    (at 139.7 125.73 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58ABB08B)
    (at 144.526 125.984 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5893F357)
    (at 134.112 132.588 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AD127D)
    (at 154.686 138.684)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.254 -1.778) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AD1060)
    (at 152.908 135.128 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58ABB0AB)
    (at 122.936 130.322 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -0.02 1.778 270) (layer F.SilkS))
    (fp_text value .022uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58AE4281)
    (at 154.94 143.51)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58307B90)
    (at 142.24 141.732 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 589D13A9)
    (at 154.686 130.81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 D+))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5893F551)
    (at 151.13 130.81 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 22 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 D+))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 589D13B3)
    (at 158.242 131.064 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 22 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 D-))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D7BC)
    (at 126.746 128.27 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 16 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D79E)
    (at 131.318 140.97)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 3.3k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D7AE)
    (at 118.364 138.684 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 3.3k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58B0D7C8)
    (at 117.348 150.034 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -0.08 -1.524 90) (layer F.SilkS))
    (fp_text value 3.3k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 589D249E)
    (at 147.828 141.478)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 1.5k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58AD1275)
    (at 159.512 137.16 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58A511DF)
    (at 157.988 150.368)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58B0D854)
    (at 147.574 127.762)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference 5V (at -1.524 0 90) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 VCC))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58B0D842)
    (at 147.574 125.222)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference 3.3 (at -1.524 0 90) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 Vdd))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58B0D850)
    (at 147.574 122.936)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference GND (at -2.54 0 180) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module USB:USB (layer F.Cu) (tedit 58AE436E)
    (at 154.94 122.936 180)
    (fp_text reference P1 (at 5.08 0.254 270) (layer F.SilkS))
    (fp_text value 10118193-0001LF (at 0 2.54 360) (layer F.Fab))
    (pad "" thru_hole circle (at -3.375 0 180) (size 2 2) (drill 1.55) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.7 -2.5 180) (size 1.75 1.75) (drill 1.25) (layers *.Cu *.Mask))
    (pad 5 smd rect (at 1.3 -2.625 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -2.625 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad4)"))
    (pad 3 smd rect (at 0 -2.625 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 18 D+))
    (pad 2 smd rect (at -0.65 -2.625 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 17 D-))
    (pad 1 smd rect (at -1.3 -2.625 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 6 smd rect (at -1.25 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.25 0 180) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask))
    (pad "" thru_hole circle (at 2.7 -2.5 180) (size 1.75 1.75) (drill 1.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 3.375 0 180) (size 2 2) (drill 1.55) (layers *.Cu *.Mask))
  )
  (module "Tantalum cap:CP_Tantalum_Case-A" (layer F.Cu) (tedit 58B0AF9B)
    (at 135.89 127 90)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C6 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -1.31 0 90) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.31 0 90) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Tantalum cap:CP_Tantalum_Case-A" (layer F.Cu) (tedit 58B0AF9B)
    (at 124.714 137.414 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C9 (at -0.254 1.778 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C9-Pad2)"))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Tantalum cap:CP_Tantalum_Case-A" (layer F.Cu) (tedit 58B0AF9B)
    (at 124.46 141.224 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C10 (at -0.254 1.778 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad2)"))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TL3305CF260QG:TL3305CF260QG (layer F.Cu) (tedit 58B0E159)
    (at 124.46 148.336 90)
    (fp_text reference S1prev (at 1.524 -3.048 90) (layer F.SilkS))
    (fp_text value switch (at -0.04 -3.34 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(S1-Pad2)"))
    (pad 4 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(S1-Pad4)"))
    (pad 3 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(S1-Pad3)"))
  )
  (module TL3305CF260QG:TL3305CF260QG (layer F.Cu) (tedit 58B0D4F5)
    (at 130.556 148.336 90)
    (fp_text reference "S2 Play" (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value switch (at -0.04 -3.34 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(S2-Pad2)"))
    (pad 4 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(S2-Pad4)"))
    (pad 3 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(S2-Pad3)"))
  )
  (module TL3305CF260QG:TL3305CF260QG (layer F.Cu) (tedit 58B0D4FC)
    (at 136.652 148.336 90)
    (fp_text reference "S3 Next" (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value switch (at -0.04 -3.34 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(S3-Pad2)"))
    (pad 4 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(S3-Pad4)"))
    (pad 3 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(S3-Pad3)"))
  )
  (module TL3305CF260QG:TL3305CF260QG (layer F.Cu) (tedit 58B0D508)
    (at 148.844 148.336 90)
    (fp_text reference "S5 Vol+" (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value switch (at -0.04 -3.34 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 Vdd))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(S5-Pad2)"))
    (pad 4 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(S5-Pad4)"))
    (pad 3 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(S5-Pad3)"))
  )
  (dimension 43.688 (width 0.3) (layer Eco1.User)
    (gr_text "43.688 mm" (at 140.208 113.966) (layer Eco1.User))
    (feature1 (pts (xy 162.052 121.412) (xy 162.052 112.616)))
    (feature2 (pts (xy 118.364 121.412) (xy 118.364 112.616)))
    (crossbar (pts (xy 118.364 115.316) (xy 162.052 115.316)))
    (arrow1a (pts (xy 162.052 115.316) (xy 160.925496 115.902421)))
    (arrow1b (pts (xy 162.052 115.316) (xy 160.925496 114.729579)))
    (arrow2a (pts (xy 118.364 115.316) (xy 119.490504 115.902421)))
    (arrow2b (pts (xy 118.364 115.316) (xy 119.490504 114.729579)))
  )
  (dimension 3.556 (width 0.3) (layer Eco1.User)
    (gr_text "3.556 mm" (at 116.586 118.03) (layer Eco1.User))
    (feature1 (pts (xy 118.364 132.842) (xy 118.364 116.68)))
    (feature2 (pts (xy 114.808 132.842) (xy 114.808 116.68)))
    (crossbar (pts (xy 114.808 119.38) (xy 118.364 119.38)))
    (arrow1a (pts (xy 118.364 119.38) (xy 117.237496 119.966421)))
    (arrow1b (pts (xy 118.364 119.38) (xy 117.237496 118.793579)))
    (arrow2a (pts (xy 114.808 119.38) (xy 115.934504 119.966421)))
    (arrow2b (pts (xy 114.808 119.38) (xy 115.934504 118.793579)))
  )
  (dimension 11.43 (width 0.3) (layer Eco1.User)
    (gr_text "11.430 mm" (at 105.076 127.127 90) (layer Eco1.User))
    (feature1 (pts (xy 118.364 121.412) (xy 103.726 121.412)))
    (feature2 (pts (xy 118.364 132.842) (xy 103.726 132.842)))
    (crossbar (pts (xy 106.426 132.842) (xy 106.426 121.412)))
    (arrow1a (pts (xy 106.426 121.412) (xy 107.012421 122.538504)))
    (arrow1b (pts (xy 106.426 121.412) (xy 105.839579 122.538504)))
    (arrow2a (pts (xy 106.426 132.842) (xy 107.012421 131.715496)))
    (arrow2b (pts (xy 106.426 132.842) (xy 105.839579 131.715496)))
  )
  (dimension 21.336 (width 0.3) (layer Eco1.User)
    (gr_text "21.336 mm" (at 108.124 143.51 90) (layer Eco1.User))
    (feature1 (pts (xy 114.808 132.842) (xy 106.774 132.842)))
    (feature2 (pts (xy 114.808 154.178) (xy 106.774 154.178)))
    (crossbar (pts (xy 109.474 154.178) (xy 109.474 132.842)))
    (arrow1a (pts (xy 109.474 132.842) (xy 110.060421 133.968504)))
    (arrow1b (pts (xy 109.474 132.842) (xy 108.887579 133.968504)))
    (arrow2a (pts (xy 109.474 154.178) (xy 110.060421 153.051496)))
    (arrow2b (pts (xy 109.474 154.178) (xy 108.887579 153.051496)))
  )
  (dimension 47.244 (width 0.3) (layer Eco1.User)
    (gr_text "47.244 mm" (at 138.43 160.862) (layer Eco1.User))
    (feature1 (pts (xy 114.808 154.178) (xy 114.808 162.212)))
    (feature2 (pts (xy 162.052 154.178) (xy 162.052 162.212)))
    (crossbar (pts (xy 162.052 159.512) (xy 114.808 159.512)))
    (arrow1a (pts (xy 114.808 159.512) (xy 115.934504 158.925579)))
    (arrow1b (pts (xy 114.808 159.512) (xy 115.934504 160.098421)))
    (arrow2a (pts (xy 162.052 159.512) (xy 160.925496 158.925579)))
    (arrow2b (pts (xy 162.052 159.512) (xy 160.925496 160.098421)))
  )
  (dimension 32.766 (width 0.3) (layer Eco1.User)
    (gr_text "32.766 mm" (at 167.72 137.795 270) (layer Eco1.User))
    (feature1 (pts (xy 162.052 154.178) (xy 169.07 154.178)))
    (feature2 (pts (xy 162.052 121.412) (xy 169.07 121.412)))
    (crossbar (pts (xy 166.37 121.412) (xy 166.37 154.178)))
    (arrow1a (pts (xy 166.37 154.178) (xy 165.783579 153.051496)))
    (arrow1b (pts (xy 166.37 154.178) (xy 166.956421 153.051496)))
    (arrow2a (pts (xy 166.37 121.412) (xy 165.783579 122.538504)))
    (arrow2b (pts (xy 166.37 121.412) (xy 166.956421 122.538504)))
  )
  (gr_line (start 114.808 154.178) (end 162.052 154.178) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.808 132.842) (end 114.808 154.178) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.364 132.842) (end 114.808 132.842) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.364 132.842) (end 118.364 121.412) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.808 154.178) (end 114.808 132.842) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.052 121.412) (end 118.364 121.412) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.052 121.666) (end 162.052 121.412) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.052 121.92) (end 162.052 121.666) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.052 154.178) (end 162.052 121.92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.002 121.412) (xy 162.052 121.412) (xy 161.798 154.178) (xy 139.192 154.178) (xy 139.192 151.384)
        (xy 142.748 151.384) (xy 142.748 121.412) (xy 143.256 121.412)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.192 121.412) (xy 118.364 121.412) (xy 118.364 132.842) (xy 114.808 132.842) (xy 114.808 154.178)
        (xy 139.192 154.178) (xy 139.192 121.412) (xy 138.938 121.412)
      )
    )
  )
)
