(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 24)
    (no_connects 2)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 27)
    (tracks 44)
    (zones 0)
    (modules 11)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.027)
    (via_drill 0.013)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0.03)
    (uvia_min_drill 0.02)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(100k1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(100K1-Pad2)")
  (net 4 "Net-(10M1-Pad1)")
  (net 5 "Net-(10M1-Pad2)")
  (net 6 "Net-(10M2-Pad1)")
  (net 7 "Net-(10M2-Pad2)")
  (net 8 "Net-(100k1-Pad1)")
  (net 9 "Net-(100K1-Pad1)")
  (net 10 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.2)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(100K1-Pad1)")
    (add_net "Net-(100K1-Pad2)")
    (add_net "Net-(100k1-Pad1)")
    (add_net "Net-(100k1-Pad2)")
    (add_net "Net-(10M1-Pad1)")
    (add_net "Net-(10M1-Pad2)")
    (add_net "Net-(10M2-Pad1)")
    (add_net "Net-(10M2-Pad2)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 143.4 101.17 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Output (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(100K1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(100k1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564D2)
    (at 146.29 109.41 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 10k1 (at 2.6 -0.05 90) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(100k1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564E6)
    (at 160.88 104.22 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 10k2 (at 2.23 0.09 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(100K1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564CB)
    (at 146.34 96.89 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 10M1 (at 2.49 0.07 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(10M1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(10M1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564E1)
    (at 164.47 104.2 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 10M2 (at 1.89 0.02 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(10M2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(10M2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564D6)
    (at 142.6 104.27 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 100k1 (at 1.96 -0.03 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(100k1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(100k1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58F564EB)
    (at 160.93 96.9 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference 100K1 (at 1.9 0 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(100K1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(100K1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 58F564F6)
    (at 143.11 112.32 180)
    (descr "Through hole straight socket strip, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x01 2.54mm double row")
    (fp_text reference D1 (at -1.33 2.59 180) (layer F.SilkS))
    (fp_text value D_Photo (at -1.27 2.33 180) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(10M1-Pad2)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5448)
    (at 164.03 112.32)
    (descr "Through hole straight socket strip, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x01 2.54mm double row")
    (fp_text reference D2 (at -1.27 -2.33) (layer F.SilkS))
    (fp_text value D_Photo (at -1.27 2.33) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(10M2-Pad2)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 58F56500)
    (at 149.805001 96.515)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.804999 7.645) (layer F.SilkS))
    (fp_text value LM324N (at 3.81 17.63) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(10M1-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(10M2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(10M1-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(10M2-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(10M1-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(10M2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(100k1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(100K1-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(100k1-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(100K1-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58F564BE)
    (at 164.02 101.08 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference Power1 (at 2.44 1.56 180) (layer F.SilkS))
    (fp_text value CONN_01X02_MALE (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 2.44 1.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "Chris Daigle\nSpring 2017\nFinal Project" (at 151.94 116.34) (layer F.SilkS))
  (gr_text VTC (at 149.53 116.17) (layer F.SilkS))
  (gr_circle (center 165.57 115.9772) (end 167.67 115.9772) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 141.57 115.9772) (end 143.67 115.9772) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 141.57 96.9772) (end 143.67 96.9772) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 165.57 96.9772) (end 167.67 96.9772) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 141.57 115.9772) (end 138.57 115.9772) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 141.57 96.9772) (end 141.57 93.9772) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 165.57 115.9772) (end 165.57 118.9772) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 165.57 96.9772) (end 168.57 96.9772) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.57 96.9772) (end 168.57 115.9772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.57 96.9772) (end 138.57 115.9772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.57 118.9772) (end 165.57 118.9772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.57 93.9772) (end 165.57 93.9772) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.23 94.6) (xy 162.89 94.66) (xy 162.89 98.68) (xy 164.41 99.12) (xy 168.23 99.22)
        (xy 168.25 113.66) (xy 162.83 113.88) (xy 161.88 118.3) (xy 143.95 117.85) (xy 143.61 114.16)
        (xy 140.93 113.6) (xy 139.92 113.72) (xy 138.97 113.66) (xy 139.09 98.91) (xy 141.21 99.35)
        (xy 143.89 99.3) (xy 143.93 94.59) (xy 144.24 94.61)
      )
    )
  )
  (zone (net 10) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.85 94.59) (xy 167.52 95.2) (xy 168.11 96.24) (xy 168.29 97.15) (xy 168.25 116.48)
        (xy 167.89 117.52) (xy 167.14 118.07) (xy 165.8 118.55) (xy 164.96 118.66) (xy 164.18 118.55)
        (xy 140.9 118.49) (xy 140.06 118.05) (xy 139.09 116.37) (xy 138.97 114.67) (xy 139 113.97)
        (xy 139.03 96.48) (xy 139.31 95.39) (xy 140.51 94.41) (xy 141.18 94.24) (xy 141.379017 94.269853)
        (xy 165.47 94.24)
      )
    )
  )
)
