(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 313)
    (zones 0)
    (modules 37)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VBAT)
  (net 3 VBUS)
  (net 4 5.0V)
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 PI_3V3)
  (net 10 PI_BCM_2_SDA)
  (net 11 PI_BCM_3_SCL)
  (net 12 PI_BCM_4_GPCLK0)
  (net 13 PI_BCM_14_TXD)
  (net 14 PI_BCM_15_RXD)
  (net 15 PI_BCM_17)
  (net 16 PI_BCM_18_PWM0)
  (net 17 PI_BCM_27)
  (net 18 PI_BCM_22)
  (net 19 PI_BCM_23)
  (net 20 "Net-(L1-Pad2)")
  (net 21 "Net-(Q1-Pad2)")
  (net 22 "Net-(R1-Pad2)")
  (net 23 "Net-(R5-Pad2)")
  (net 24 "Net-(R6-Pad2)")
  (net 25 "Net-(R10-Pad1)")
  (net 26 "Net-(R11-Pad1)")
  (net 27 "Net-(R12-Pad1)")
  (net 28 "Net-(R13-Pad2)")
  (net 29 "Net-(R14-Pad2)")
  (net 30 "Net-(R15-Pad1)")
  (net 31 "Net-(S1-Pad3)")
  (net 32 "Net-(S1-Pad4)")
  (net 33 "Net-(S1-Pad5)")
  (net 34 "Net-(S1-Pad6)")
  (net 35 "Net-(U1-Pad2)")
  (net 36 "Net-(U2-Pad6)")
  (net 37 "Net-(J3-PadB2)")
  (net 38 "Net-(J3-PadB3)")
  (net 39 "Net-(J3-PadB5)")
  (net 40 "Net-(J3-PadB8)")
  (net 41 "Net-(J3-PadB10)")
  (net 42 "Net-(J3-PadB11)")
  (net 43 "Net-(J3-PadB6)")
  (net 44 "Net-(J3-PadB7)")
  (net 45 "Net-(J3-PadA11)")
  (net 46 "Net-(J3-PadA10)")
  (net 47 "Net-(J3-PadA8)")
  (net 48 "Net-(J3-PadA7)")
  (net 49 "Net-(J3-PadA6)")
  (net 50 "Net-(J3-PadA5)")
  (net 51 "Net-(J3-PadA3)")
  (net 52 "Net-(J3-PadA2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5.0V)
    (add_net GND)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J3-PadA10)")
    (add_net "Net-(J3-PadA11)")
    (add_net "Net-(J3-PadA2)")
    (add_net "Net-(J3-PadA3)")
    (add_net "Net-(J3-PadA5)")
    (add_net "Net-(J3-PadA6)")
    (add_net "Net-(J3-PadA7)")
    (add_net "Net-(J3-PadA8)")
    (add_net "Net-(J3-PadB10)")
    (add_net "Net-(J3-PadB11)")
    (add_net "Net-(J3-PadB2)")
    (add_net "Net-(J3-PadB3)")
    (add_net "Net-(J3-PadB5)")
    (add_net "Net-(J3-PadB6)")
    (add_net "Net-(J3-PadB7)")
    (add_net "Net-(J3-PadB8)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S1-Pad5)")
    (add_net "Net-(S1-Pad6)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad6)")
    (add_net PI_3V3)
    (add_net PI_BCM_14_TXD)
    (add_net PI_BCM_15_RXD)
    (add_net PI_BCM_17)
    (add_net PI_BCM_18_PWM0)
    (add_net PI_BCM_22)
    (add_net PI_BCM_23)
    (add_net PI_BCM_27)
    (add_net PI_BCM_2_SDA)
    (add_net PI_BCM_3_SCL)
    (add_net PI_BCM_4_GPCLK0)
    (add_net VBAT)
    (add_net VBUS)
  )
  (module digikey-footprints:USB-C_Female_E8124-015-01 (layer F.Cu) (tedit 5D28AD42)
    (at 173.482 74.93 180)
    (descr https://www.digikey.com/product-detail/en/pulse-electronics-network/E8124-015-01/553-3195-2-ND/5800435)
    (attr smd)
    (fp_text reference J3 (at -5.969 4.318) (layer F.SilkS))
    (fp_text value USB_C_Receptacle (at 0 9.29) (layer F.Fab))
    (fp_text user %R (at 0 3.3) (layer F.Fab))
    (pad SH thru_hole oval (at 4.5 4.335 180) (size 0.9 1.9) (drill oval 0.5 1.5) (layers *.Cu *.Mask))
    (pad SH thru_hole oval (at -4.5 4.335 180) (size 0.9 1.9) (drill oval 0.5 1.5) (layers *.Cu *.Mask))
    (pad SH thru_hole oval (at 4.22 1.82 180) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask))
    (pad SH thru_hole oval (at -4.22 1.82 180) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask))
    (pad SH thru_hole oval (at 3.845 -0.98 180) (size 1.15 0.8) (drill oval 0.75 0.4) (layers *.Cu *.Mask))
    (pad SH thru_hole oval (at -3.845 -0.98 180) (size 1.15 0.8) (drill oval 0.75 0.4) (layers *.Cu *.Mask))
    (pad "" smd rect (at 1.25 -0.98 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -1.25 -0.98 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole oval (at 3.6 0.57 180) (size 0.95 0.65) (drill oval 0.95 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.6 0.57 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad B2 thru_hole circle (at 2.4 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 37 "Net-(J3-PadB2)"))
    (pad B3 thru_hole circle (at 1.6 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 38 "Net-(J3-PadB3)"))
    (pad B5 thru_hole circle (at 0.8 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-PadB5)"))
    (pad B8 thru_hole circle (at -0.8 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-PadB8)"))
    (pad B10 thru_hole circle (at -1.6 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-PadB10)"))
    (pad B11 thru_hole circle (at -2.4 1.92 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-PadB11)"))
    (pad B1 thru_hole circle (at 2.8 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B4 thru_hole circle (at 1.2 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 3 VBUS))
    (pad B6 thru_hole circle (at 0.4 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-PadB6)"))
    (pad B7 thru_hole circle (at -0.4 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-PadB7)"))
    (pad B9 thru_hole circle (at -1.2 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 3 VBUS))
    (pad B12 thru_hole circle (at -2.8 1.22 180) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A12 smd rect (at 2.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A11 smd rect (at 2.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J3-PadA11)"))
    (pad A10 smd rect (at 1.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J3-PadA10)"))
    (pad A9 smd rect (at 1.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VBUS))
    (pad A8 smd rect (at 0.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J3-PadA8)"))
    (pad A7 smd rect (at 0.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J3-PadA7)"))
    (pad A6 smd rect (at -0.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J3-PadA6)"))
    (pad A5 smd rect (at -0.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J3-PadA5)"))
    (pad A4 smd rect (at -1.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VBUS))
    (pad A3 smd rect (at -1.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J3-PadA3)"))
    (pad A2 smd rect (at -2.25 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J3-PadA2)"))
    (pad A1 smd rect (at -2.75 0 180) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N16_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5E11FE4E)
    (at 164.6555 95.6945 90)
    (descr "QFN, 16 Pin (http://www.ti.com/lit/ds/symlink/msp430g2001.pdf#page=43), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U1 (at -3.5 0.1845 180) (layer F.SilkS))
    (fp_text value TPS61090 (at 0 3.32 90) (layer F.Fab))
    (fp_text user %R (at 0 0.127 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.9625 -0.975 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V) (zone_connect 2))
    (pad 2 smd roundrect (at -1.9625 -0.325 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U1-Pad2)") (zone_connect 2))
    (pad 3 smd roundrect (at -1.9625 0.325 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(L1-Pad2)") (zone_connect 2))
    (pad 4 smd roundrect (at -1.9625 0.975 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(L1-Pad2)") (zone_connect 2))
    (pad 5 smd roundrect (at -0.975 1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd roundrect (at -0.325 1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 7 smd roundrect (at 0.325 1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd roundrect (at 0.975 1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT) (zone_connect 2))
    (pad 9 smd roundrect (at 1.9625 0.975 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R1-Pad2)") (zone_connect 2))
    (pad 10 smd roundrect (at 1.9625 0.325 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 11 smd roundrect (at 1.9625 -0.325 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R5-Pad2)") (zone_connect 2))
    (pad 12 smd roundrect (at 1.9625 -0.975 90) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PI_BCM_23) (zone_connect 2))
    (pad 13 smd roundrect (at 0.975 -1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 14 smd roundrect (at 0.325 -1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R6-Pad2)") (zone_connect 2))
    (pad 15 smd roundrect (at -0.325 -1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V) (zone_connect 2))
    (pad 16 smd roundrect (at -0.975 -1.9625 90) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V) (zone_connect 2))
    (pad 17 smd rect (at 0 0 90) (size 2.7 2.7) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at -1.1 -1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 0 -1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 1.1 -1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at -1.1 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 1.1 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at -1.1 1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 0 1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 1.1 1.1 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 17 smd rect (at 0 0 90) (size 2.7 2.7) (layers B.Cu)
      (net 1 GND) (zone_connect 2))
    (pad "" smd roundrect (at -0.55 -0.55 90) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 2))
    (pad "" smd roundrect (at -0.55 0.55 90) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.55 -0.55 90) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.55 0.55 90) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N16_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_DPDT_CK_JS202011JCQN (layer F.Cu) (tedit 5E695155)
    (at 161.99358 71.3548 180)
    (descr "Sub-miniature slide switch, vertical, SMT J bend https://dznh3ojzb2azq.cloudfront.net/products/Slide/JS/documents/datasheet.pdf")
    (tags "switch DPDT SMT")
    (attr smd)
    (fp_text reference S1 (at 0 -3.05) (layer F.SilkS))
    (fp_text value JS202011SCQN (at 0 3.15) (layer F.Fab))
    (fp_text user %R (at 0 -3.05) (layer F.Fab))
    (pad 3 smd rect (at 2.5 -1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(S1-Pad3)"))
    (pad 2 smd rect (at 0 -1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.5 -1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 2.5 1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(S1-Pad6)"))
    (pad 5 smd rect (at 0 1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(S1-Pad5)"))
    (pad 4 smd rect (at -2.5 1.2 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(S1-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DPDT_CK_JS202011JCQN.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tinycam:FP11SPA1B1TP00 (layer F.Cu) (tedit 5F409F6E)
    (at 195.453 74.803 270)
    (fp_text reference SW1 (at 0.127 -0.889) (layer F.SilkS))
    (fp_text value SW_SPST (at 0.0254 5.8928 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 2.54 2.54 270) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.54 2.54 270) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 PI_BCM_18_PWM0))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 153.5 97.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H2 (at 0 -0.091) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 153.5 71.5)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0.043 0.001) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 189.865 98.171 270)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J4 (at -0.0635 10.668 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 PI_BCM_3_SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PI_BCM_2_SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 5.0V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x08_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A42B)
    (at 195.58 80.391 180)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J1 (at 2.921 0.127) (layer B.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at -1.27 -20.55) (layer B.Fab))
    (fp_text user %R (at -1.27 -8.89 270) (layer B.Fab))
    (pad 16 thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 PI_BCM_23))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 PI_BCM_22))
    (pad 14 thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 PI_BCM_27))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 PI_BCM_18_PWM0))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 PI_BCM_17))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 PI_BCM_15_RXD))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 PI_BCM_14_TXD))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 PI_BCM_4_GPCLK0))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 PI_BCM_3_SCL))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 5.0V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PI_BCM_2_SDA))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 5.0V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PI_3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 187.833 90.0915 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 2.3645 0 180) (layer F.SilkS))
    (fp_text value 15K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 190.119 85.979 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.54 -0.254 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 190.119 83.82 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -2.54 0.254 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 187.96 80.1855 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 2.3345 0 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 185.801 80.1855 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.3345 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 183.515 90.0915 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.3645 0 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 185.674 90.0915 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.3645 0.127 180) (layer F.SilkS))
    (fp_text value 270K (at 0 1.524 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 155.575 85.0415 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.0485 -2.032 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 159.3365 95.504 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.6185 0) (layer F.SilkS))
    (fp_text value 200K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 159.3365 93.218)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.6185 0) (layer F.SilkS))
    (fp_text value 1.87M (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 162.56 90.2185 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.3345 0 180) (layer F.SilkS))
    (fp_text value 200K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.9245 76.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.517 0) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J3-PadB5)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.9245 78.232)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.517 0.127) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(J3-PadA5)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.846 90.2185 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.3345 0 180) (layer F.SilkS))
    (fp_text value 340K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 167.132 90.2185 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.3345 0 180) (layer F.SilkS))
    (fp_text value 1.87M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at -0.0485 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 159.3365 90.932)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.6185 0) (layer F.SilkS))
    (fp_text value "100 uF" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 159.3065 97.79 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5885 0) (layer F.SilkS))
    (fp_text value "2.2 uF" (at -0.2055 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 160.909 77.0105 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.3645 0 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 158.877 77.0105 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.3645 0 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 181.2925 90.1065 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.3495 0.0635 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 183.642 80.2005 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.3495 0 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 181.9425 75.184 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0.015 -1.651) (layer F.SilkS))
    (fp_text value RED_LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 197.5335 70.104 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 2.906 -0.0635) (layer F.SilkS))
    (fp_text value BLUE_LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 5.0V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 186.04 75.184 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at -0.015 -1.651) (layer F.SilkS))
    (fp_text value ORANGE_LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 190.0705 75.184)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at -0.015 1.651) (layer F.SilkS))
    (fp_text value GREEN_LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0.0485 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:PinHeader_1x2_P2mm_Drill1mm (layer F.Cu) (tedit 5A4C0C10)
    (at 153.797 79.343 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (fp_text reference J2 (at 4.921 1.905 180) (layer F.SilkS))
    (fp_text value B2B-PH-K-S_LF__SN_ (at 1.04 3.58 90) (layer F.Fab))
    (fp_text user %R (at 1.02 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
  )
  (module Inductor_SMD:L_Wuerth_HCI-5040 (layer F.Cu) (tedit 5990349D)
    (at 165.118 84.074)
    (descr "Inductor, Wuerth Elektronik, Wuerth_HCI-5040, 5.5mmx5.2mm")
    (tags "inductor Wuerth hci smd")
    (attr smd)
    (fp_text reference L1 (at 0 -3.6) (layer F.SilkS))
    (fp_text value "6.8 uH" (at 0 4.1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.05 0) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VBAT))
    (pad 2 smd rect (at 2.05 0) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_HCI-5040.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 158.75 85.09)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.794) (layer F.SilkS))
    (fp_text value MMUN2211LT1G (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VBAT) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q1-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 PI_BCM_23) (solder_mask_margin 0.07))
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm (layer F.Cu) (tedit 5DC5F6A3)
    (at 185.039 85.09 90)
    (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=274), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U2 (at 0 -3.937 180) (layer F.SilkS))
    (fp_text value MCP73871-1AA (at 0 3.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.9375 -1 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (pad 2 smd roundrect (at -1.9375 -0.5 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad1)"))
    (pad 3 smd roundrect (at -1.9375 0 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 4 smd roundrect (at -1.9375 0.5 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 5 smd roundrect (at -1.9375 1 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R15-Pad1)"))
    (pad 6 smd roundrect (at -1 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(U2-Pad6)"))
    (pad 7 smd roundrect (at -0.5 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R14-Pad2)"))
    (pad 8 smd roundrect (at 0 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R13-Pad2)"))
    (pad 9 smd roundrect (at 0.5 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 10 smd roundrect (at 1 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 1.9375 1 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 1.9375 0.5 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R12-Pad1)"))
    (pad 13 smd roundrect (at 1.9375 0 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R11-Pad1)"))
    (pad 14 smd roundrect (at 1.9375 -0.5 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (pad 15 smd roundrect (at 1.9375 -1 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (pad 16 smd roundrect (at 1 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (pad 17 smd roundrect (at 0.5 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 18 smd roundrect (at 0 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 19 smd roundrect (at -0.5 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 20 smd roundrect (at -1 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (pad 21 smd rect (at 0 0 90) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd roundrect (at -0.625 -0.625 90) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.247525))
    (pad "" smd roundrect (at -0.625 0.625 90) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.247525))
    (pad "" smd roundrect (at 0.625 -0.625 90) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.247525))
    (pad "" smd roundrect (at 0.625 0.625 90) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.247525))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 189.865 96.012) (layer F.SilkS))
  (gr_text 5V (at 187.325 96.012) (layer F.SilkS))
  (gr_text SCL (at 182.245 96.012) (layer F.SilkS))
  (gr_text SDA (at 184.785 96.012) (layer F.SilkS))
  (gr_line (start 178.5 90.75) (end 178.5 78.5) (layer Edge.Cuts) (width 0.2))
  (gr_text "RPi power mgmt\nboard for use with\n2.8in screen. Based \non Adafruit \nPowerBoost 1000C." (at 168.1861 86.7029) (layer B.SilkS))
  (gr_text github.com/pvphan/tinycam (at 179.959 94.234) (layer F.SilkS))
  (gr_line (start 178 78) (end 169.5 78) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 178 78.5) (end 178.5 78.5) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 169.5 78.5) (end 169.5 78) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 169 78.5) (end 169 90.75) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 178 90.75) (end 178 91.25) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 169.5 90.75) (end 169 90.75) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 169.5 91.25) (end 178 91.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 190.5 74) (end 181.5 74) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 190.5 73) (end 190.5 74) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 181.5 73) (end 180.5 73) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 191.5 70) (end 191.5 73) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 180.5 73) (end 180.5 70) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 192.5 70) (end 192.5 69) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 179.5 70) (end 180.5 70) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 199 69) (end 192.5 69) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 179.5 69) (end 152 69) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 199 70) (end 200 70) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 152 70) (end 152 69) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 200 99) (end 200 70) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151 70) (end 151 99) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 199 99) (end 199 100) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 152 99) (end 151 99) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 152 100) (end 199 100) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 69.85) (xy 180.34 73.406) (xy 181.102 74.168) (xy 191.008 74.168) (xy 191.77 73.406)
        (xy 191.77 69.85) (xy 192.532 69.088) (xy 199.136 69.088) (xy 199.898 69.85) (xy 199.898 99.06)
        (xy 199.39 99.822) (xy 152.146 99.822) (xy 151.13 99.06) (xy 151.13 69.85) (xy 151.892 69.088)
        (xy 179.578 69.088)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.34 69.85) (xy 180.34 73.406) (xy 181.102 74.168) (xy 191.008 74.168) (xy 191.77 73.406)
        (xy 191.77 69.85) (xy 192.532 69.088) (xy 199.136 69.088) (xy 199.898 69.85) (xy 199.898 99.06)
        (xy 199.39 99.822) (xy 152.146 99.822) (xy 151.13 99.06) (xy 151.13 69.85) (xy 151.892 69.088)
        (xy 179.578 69.088)
      )
    )
  )
)
