(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "HEMT Amplifier 300K Filter Box")
    (date "2024-05-09")
    (rev "V4.1")
    (company "SPLENDOR Collaboration")
    (comment 1 "Jadyn Anczarski | 2024")
    (comment 2 "KIPAC at Stanford and SLAC")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 50.810662 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(J2-Pad2)")
  (net 3 "unconnected-(J2-Pad3)")
  (net 4 "unconnected-(J2-Pad6)")
  (net 5 "unconnected-(J2-Pad7)")
  (net 6 "unconnected-(J2-P10-Pad10)")
  (net 7 "unconnected-(J2-P111-Pad11)")
  (net 8 "unconnected-(J2-P14-Pad14)")
  (net 9 "unconnected-(J3-Pad2)")
  (net 10 "unconnected-(J3-Pad11)")
  (net 11 "unconnected-(J3-Pad13)")
  (net 12 "unconnected-(J3-P15-Pad15)")
  (net 13 "unconnected-(J3-P24-Pad24)")
  (net 14 "unconnected-(J5-Pad2)")
  (net 15 "unconnected-(J5-Pad3)")
  (net 16 "unconnected-(J5-Pad6)")
  (net 17 "unconnected-(J5-Pad7)")
  (net 18 "unconnected-(J5-P10-Pad10)")
  (net 19 "unconnected-(J5-P111-Pad11)")
  (net 20 "unconnected-(J5-P14-Pad14)")
  (net 21 "/Vdd1+(2)")
  (net 22 "/Vdd1-(2)")
  (net 23 "/INJ (2)")
  (net 24 "/Vgg1-(2)")
  (net 25 "/Vdd2-(2)")
  (net 26 "/Vgg2-(2)")
  (net 27 "/Vdd1+(1)")
  (net 28 "/Vdd1-(1)")
  (net 29 "/INJ (1)")
  (net 30 "/Vgg1-(1)")
  (net 31 "/Vdd2-(1)")
  (net 32 "/Vgg2-(1)")
  (net 33 "/OUT-(2)")
  (net 34 "/OUT+(2)")
  (net 35 "/DETBIAS-(2)")
  (net 36 "/DETBIAS+(2)")
  (net 37 "/Vgg2+(2)")
  (net 38 "/Vdd2+(2)")
  (net 39 "/OUT-(1)")
  (net 40 "/DETBIAS-(1)")
  (net 41 "/OUT+(1)")
  (net 42 "/DETBIAS+(1)")
  (net 43 "/Vgg2+(1)")
  (net 44 "/Vdd2+(1)")
  (net 45 "/Vdd1+(2) ")
  (net 46 "/Vgg1+(2)")
  (net 47 "/Vdd2(2) ")
  (net 48 "/Vgg2(2) ")
  (net 49 "/Vdd1+(1) ")
  (net 50 "/Vdd2(1) ")
  (net 51 "/Vgg2(1) ")
  (net 52 "/Vgg1+(1)")
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 238.770662 101.6)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 32 "/Vgg2-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 51 "/Vgg2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 230.890662 77.5335)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 22 "/Vdd1-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 45 "/Vdd1+(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 213.370662 114.3)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 30 "/Vgg1-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 29 "/INJ (1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 218.450662 88.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 38 "/Vdd2+(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 47 "/Vdd2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 244.270662 114.0035)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 27 "/Vdd1+(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 49 "/Vdd1+(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 212.950662 77.5335)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 26 "/Vgg2-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 48 "/Vgg2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 237.390662 77.5335)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 22 "/Vdd1-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 45 "/Vdd1+(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 218.870662 114.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 52 "/Vgg1+(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 29 "/INJ (1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 218.450662 77.5335)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 37 "/Vgg2+(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "/Vgg2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 242.890662 77.5335)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 21 "/Vdd1+(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 45 "/Vdd1+(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 212.950662 101.6)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 31 "/Vdd2-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 50 "/Vdd2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 232.270662 101.6)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 32 "/Vgg2-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 51 "/Vgg2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 206.450662 101.6)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 31 "/Vdd2-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 50 "/Vdd2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 206.870662 114.3)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 30 "/Vgg1-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 29 "/INJ (1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 206.450662 88.9)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 25 "/Vdd2-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 47 "/Vdd2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lib:MILL-MAX_830-10-006-10-005000" (layer "F.Cu")
    (at 175.270662 82.475 90)
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -3.075 -2.885 90) (layer "F.SilkS"))
    (fp_text value "BNC_IN_2" (at -2.413 2.286 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -5 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 36 "/DETBIAS+(2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -1 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 35 "/DETBIAS-(2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 1 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 34 "/OUT+(2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 3 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 33 "/OUT-(2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 5 0 90) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 23 "/INJ (2)") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 231.55941 88.9)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 24 "/Vgg1-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 23 "/INJ (2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lib:MILL-MAX_830-10-006-10-005000" (layer "F.Cu")
    (at 175.270662 107.14 -90)
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -3.075 -2.885 90) (layer "F.SilkS"))
    (fp_text value "BNC_IN_1" (at -2.429 2.286 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -5 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 42 "/DETBIAS+(1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -1 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 40 "/DETBIAS-(1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 1 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 41 "/OUT+(1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 3 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 39 "/OUT-(1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 5 0 270) (size 1.218 1.218) (drill 0.71) (layers "*.Cu" "*.Mask")
      (net 29 "/INJ (1)") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 238.770662 114.0035)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 28 "/Vdd1-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 49 "/Vdd1+(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 212.950662 88.9)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 25 "/Vdd2-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 47 "/Vdd2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 232.270662 114.0035)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 28 "/Vdd1-(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 49 "/Vdd1+(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric" (layer "F.Cu")
    (at 206.450662 77.5335)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "470uF" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 26 "/Vgg2-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.05 0) (size 1.4 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 48 "/Vgg2(2) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 218.450662 101.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 44 "/Vdd2+(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 50 "/Vdd2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 238.05941 88.9)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 24 "/Vgg1-(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 23 "/INJ (2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 243.55941 88.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 46 "/Vgg1+(2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "/INJ (2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 244.270662 101.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 43 "/Vgg2+(1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 51 "/Vgg2(1) ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm" (layer "B.Cu")
    (at 86.600662 83.82)
    (descr "15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "15-pin female receptacle socket D-SUB connector (low-density/2 columns)")
    (property "ki_keywords" "female receptacle D-SUB connector")
    (attr through_hole)
    (fp_text reference "J2" (at -9.695 5.89) (layer "B.SilkS"))
    (fp_text value "HARVARD_PS_2" (at -9.695 -8.73) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -9.695 -1.42) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/Vdd1+(2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(J2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(J2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/Vgg1+(2)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/Vdd2+(2)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -13.85 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(J2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -16.62 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(J2-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -19.39 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/Vgg2+(2)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.385 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/Vdd1-(2)") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole circle (at -4.155 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(J2-P10-Pad10)") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole circle (at -6.925 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(J2-P111-Pad11)") (pinfunction "P111") (pintype "passive"))
    (pad "12" thru_hole circle (at -9.695 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Vgg1-(2)") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole circle (at -12.465 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Vdd2-(2)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.235 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(J2-P14-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -18.005 -2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/Vgg2-(2)") (pinfunction "P15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Vertical_P2.77x2.84mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lib:CONN_5747846-4_TYC" (layer "B.Cu")
    (at 265.159931 95 90)
    (tags "5747846-4 ")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "25-pin female receptacle socket D-SUB connector")
    (property "ki_keywords" "female receptacle D-SUB connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 0 270 unlocked) (layer "B.SilkS"))
    (fp_text value "DB25_F_Fridge" (at 0 0 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -16.6116 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 42 "/DETBIAS+(1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -13.843 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -11.0744 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 49 "/Vdd1+(1) ") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.3058 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 29 "/INJ (1)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -5.5372 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 50 "/Vdd2(1) ") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.7686 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 41 "/OUT+(1)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 34 "/OUT+(2)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.7686 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 47 "/Vdd2(2) ") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.5372 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 23 "/INJ (2)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 8.3058 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 45 "/Vdd1+(2) ") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 11.0744 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J3-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 13.843 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 36 "/DETBIAS+(2)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 16.6116 -10.922 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(J3-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.2273 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 40 "/DETBIAS-(1)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -12.4587 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(J3-P15-Pad15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at -9.6901 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 28 "/Vdd1-(1)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at -6.9215 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 51 "/Vgg2(1) ") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at -4.1529 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 31 "/Vdd2-(1)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at -1.3843 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 39 "/OUT-(1)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at 1.3843 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 33 "/OUT-(2)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at 4.1529 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 25 "/Vdd2-(2)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at 6.9215 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 48 "/Vgg2(2) ") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at 9.6901 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 22 "/Vdd1-(2)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at 12.4587 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(J3-P24-Pad24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at 15.2273 -8.0772 90) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 35 "/DETBIAS-(2)") (pinfunction "P25") (pintype "passive"))
    (pad "26" thru_hole circle (at -23.6474 -9.4996 90) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
    (pad "27" thru_hole circle (at 23.6474 -9.4996 90) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm" (layer "B.Cu")
    (at 67.440662 104.14 180)
    (descr "15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm")
    (property "Sheetfile" "hemt_board_filter_v4.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "15-pin female receptacle socket D-SUB connector (low-density/2 columns)")
    (property "ki_keywords" "female receptacle D-SUB connector")
    (attr through_hole)
    (fp_text reference "J5" (at -9.695 5.89) (layer "B.SilkS"))
    (fp_text value "HARVARD_PS_1" (at -9.695 -8.73) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -9.695 -1.42) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/Vdd1+(1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(J5-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(J5-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "/Vgg1+(1)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/Vdd2+(1)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -13.85 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J5-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -16.62 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J5-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -19.39 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/Vgg2+(1)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.385 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/Vdd1-(1)") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole circle (at -4.155 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J5-P10-Pad10)") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole circle (at -6.925 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J5-P111-Pad11)") (pinfunction "P111") (pintype "passive"))
    (pad "12" thru_hole circle (at -9.695 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Vgg1-(1)") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole circle (at -12.465 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/Vdd2-(1)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.235 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J5-P14-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -18.005 -2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/Vgg2-(1)") (pinfunction "P15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Vertical_P2.77x2.84mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 43 65) (end 43 125)
    (layer "Edge.Cuts"))
  (gr_line (start 43 125) (end 259 125)
    (layer "Edge.Cuts"))
  (gr_line (start 259 125) (end 259 65)
    (layer "Edge.Cuts"))
  (gr_line (start 259 65) (end 43 65)
    (layer "Edge.Cuts"))
  (gr_text "KIPAC at STANFORD and SLAC\nSPLENDOR COLLABORATION\nHEMT AMPLIFIER 300K FILTER BOARD V4.1\nJADYN ANCZARSKI, MAY 2024" (at 43.317662 124.841) (layer "F.SilkS"))
  (gr_text "Vgg2" (at 227.571662 103.9495 90) (layer "F.SilkS"))
  (gr_text "CHANNEL 1" (at 160.030662 111.76 90) (layer "F.SilkS"))
  (gr_text "CHANNEL 2" (at 160.030662 86.36 90) (layer "F.SilkS"))
  (gr_text "Vdd1" (at 226.451662 79.6925 90) (layer "F.SilkS"))
  (gr_text "Vgg2" (at 201.757662 79.6925 90) (layer "F.SilkS"))
  (gr_text "Vgg1" (at 202.171662 116.332 90) (layer "F.SilkS"))
  (gr_text "Vdd2" (at 202.051324 103.9915 90) (layer "F.SilkS"))
  (gr_text "Vgg1" (at 226.86641 90.805 90) (layer "F.SilkS"))
  (gr_text "Vdd1" (at 227.952662 116.1625 90) (layer "F.SilkS"))
  (gr_text "Vdd2" (at 202.011662 91.186 90) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 261.630662 60.96)
        (xy 261.630662 129.54)
        (xy 38.110662 129.54)
        (xy 38.110662 60.96)
      )
    )
  )
)
