(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Quad ESL-63 HV Board")
    (date "Aug 1, 2018")
    (rev "A")
    (company "SDS Labs")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x0000030_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(B1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(R3-Pad1)")
  (net 4 "Net-(D1-K)")
  (net 5 "Net-(D3-K)")
  (net 6 "Net-(D5-K)")
  (net 7 "Net-(D7-K)")
  (net 8 "Net-(D2-K)")
  (net 9 "Net-(D1-A)")
  (net 10 "Net-(D4-K)")
  (net 11 "Net-(D6-K)")
  (net 12 "Net-(D8-K)")
  (net 13 "Net-(P1-Pin_1)")
  (net 14 "Net-(P2-Pin_1)")
  (net 15 "Net-(OUT1-Pin_1)")
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 168.275 73.914)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 18.415 3.556) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 149.225 73.914)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at -3.81 4.826) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 130.175 73.914)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 8.255 4.826) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D5-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 111.125 73.914)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 6.985 4.826) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D7-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D5-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 190.754 72.517 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.683 -2.921 -90) (layer "F.SilkS"))
    (fp_text value "82K" (at 8.763 0.254 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(P1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 198.501 85.217 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.302 -2.92 90) (layer "F.SilkS"))
    (fp_text value "220K" (at 3.937 -0.381 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Wire_Pads:SolderWirePad_single_0-8mmDrill" (layer "F.Cu")
    (at 191.516 128.016)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "GND1" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 9.525 9.525) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4" (layer "F.Cu")
    (at 118.237 97.028 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C15" (at -3.048 1.143 180) (layer "F.SilkS"))
    (fp_text value "0.047uF" (at 3.75 3.75 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(OUT1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(B1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 110.871 117.856)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C14" (at 6.604 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D8-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 110.871 109.728)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at 7.5 -4.75) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D8-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 129.667 117.856)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at 7.493 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Wire_Pads:SolderWirePad_single_0-8mmDrill" (layer "F.Cu")
    (at 194.183 96.012)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "P2" (at 0 -2.794) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(P2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Wire_Pads:SolderWirePad_single_0-8mmDrill" (layer "F.Cu")
    (at 187.833 95.885)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "P1" (at 0 -2.794) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(P1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Varistor:RV_Disc_D12mm_W7.9mm_P7.5mm" (layer "F.Cu")
    (at 192.659 101.854 -90)
    (descr "Varistor, diameter 12mm, width 7.9mm, pitch 7.5mm")
    (tags "varistor SIOV")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Voltage dependent resistor")
    (property "ki_keywords" "VDR resistance")
    (attr through_hole)
    (fp_text reference "VR1" (at 3.75 7.15 -90) (layer "F.SilkS"))
    (fp_text value "VR" (at 3.75 -2.75 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.2 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(P1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 4.4 270) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Varistor.3dshapes/RV_Disc_D12mm_W7.9mm_P7.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 110.363 102.362)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 12.827 -2.667) (layer "F.SilkS"))
    (fp_text value "10M" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(B1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D8-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 198.501 88.9 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 1.905 2.921 -90) (layer "F.SilkS"))
    (fp_text value "220K" (at 5.715 -0.254 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(P2-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 198.501 105.029 -90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 6.096 2.921 -90) (layer "F.SilkS"))
    (fp_text value "180K" (at 6.096 -0.254 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(P2-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 128.143 102.362 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D8" (at 6.35 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D8-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D7-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 136.017 89.662 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D7" (at 6.223 2.667 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 143.891 102.362 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D6" (at 6.35 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D5-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 151.511 89.662 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D5" (at 6.35 2.921 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 159.385 102.362 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D4" (at 6.35 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 167.259 89.662 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D3" (at 6.35 2.794 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 175.133 102.362 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 6.35 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 182.753 89.662 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 6.35 3.048 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 129.667 109.728)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C11" (at 7.5 -4.75) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 148.463 117.856)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at 7.5 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 148.463 109.728)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 7.5 -4.75) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D4-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 167.513 117.856)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at 7.747 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 168.275 82.296)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 10.795 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 167.513 109.728)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 7.5 -4.75) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "sdsLogos:sdsLabs-large-fSilk" (layer "F.Cu")
    (at 129.54 83.185)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -7.62) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 -5.08) (layer "F.SilkS") hide)
  )
  (footprint "Wire_Pads:SolderWirePad_single_0-8mmDrill" (layer "F.Cu")
    (at 120.015 89.662)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "OUT1" (at 1.27 3.048) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.81 3.81) (drill 1.524) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(OUT1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Wire_Pads:SolderWirePad_single_0-8mmDrill" (layer "F.Cu")
    (at 188.468 117.729)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "GND2" (at 2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.81 3.81) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D1-A)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "kicad-SDS-footprints:neonBulb" (layer "F.Cu")
    (at 113.411 87.122)
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Neon lamp")
    (property "ki_keywords" "neon lamp")
    (attr through_hole)
    (fp_text reference "B1" (at -2.921 -2.032) (layer "F.SilkS"))
    (fp_text value "neonBulb" (at 0 -0.5) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -2.54 2.54) (size 2.54 2.54) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "Net-(B1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.54 2.54) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 15 "Net-(OUT1-Pin_1)") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (at 149.225 82.296)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*7mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 7mm Capacitor")
    (property "Sheetfile" "esl63_hvMain.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 13.97 4.699) (layer "F.SilkS"))
    (fp_text value "0.01uF" (at 7.5 4.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D3-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W7.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 117.856 128.016)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Symbol:Symbol_HighVoltage_Type2_CopperTop_VerySmall" (layer "B.Cu")
    (at 179.07 128.27 180)
    (descr "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (tags "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at -0.127 5.715) (layer "B.SilkS") hide)
    (fp_text value "Symbol_HighVoltage_Type2_CopperTop_VerySmall" (at -0.381 -4.572) (layer "B.Fab"))
  )
  (gr_line (start 107.696 69.596) (end 201.676 69.596)
    (layer "Edge.Cuts"))
  (gr_circle (center 117.856 128.016) (end 119.38 128.016)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 201.676 69.596) (end 201.676 133.096)
    (layer "Edge.Cuts"))
  (gr_line (start 107.696 133.096) (end 107.696 69.596)
    (layer "Edge.Cuts"))
  (gr_circle (center 191.516 128.016) (end 193.04 128.016)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 201.676 133.096) (end 107.696 133.096)
    (layer "Edge.Cuts"))
  (gr_text "ESL-63 HV Board" (at 136.525 86.36) (layer "F.SilkS"))
)
