(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 9)
    (no_connects 2)
    (area 160.024999 97.924999 168.175001 106.675001)
    (thickness 1.6)
    (drawings 20)
    (tracks 27)
    (zones 0)
    (modules 2)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.03)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /Vbus)
  (net 3 /D-)
  (net 4 /D+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D+)
    (add_net /D-)
    (add_net /GND)
    (add_net /Vbus)
  )
  (module adapter:WM12855-ND (layer F.Cu) (tedit 5AC029C9)
    (at 163.6 102.3 90)
    (fp_text reference U1 (at 0.025 6.2 90) (layer F.SilkS) hide)
    (fp_text value USBC (at 0 -4.6 90) (layer F.Fab) hide)
    (pad B1 smd rect (at -2.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad X smd rect (at -3.425 -1.925 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask))
    (pad A12 smd rect (at -2.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad A11 smd rect (at -2.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A10 smd rect (at -1.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A9 smd rect (at -1.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /Vbus))
    (pad A8 smd rect (at -0.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at -0.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /D-))
    (pad A6 smd rect (at 0.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /D+))
    (pad A5 smd rect (at 0.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A4 smd rect (at 1.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /Vbus))
    (pad A3 smd rect (at 1.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd rect (at 2.25 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask))
    (pad A1 smd rect (at 2.75 -2.5 90) (size 0.38 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad X smd rect (at -3.42 -1.92 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd rect (at -2.25 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B3 smd rect (at -1.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B4 smd rect (at -1.25 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vbus))
    (pad B5 smd rect (at -0.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B8 smd rect (at 0.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B9 smd rect (at 1.25 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vbus))
    (pad B10 smd rect (at 1.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B11 smd rect (at 2.25 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
    (pad B12 smd rect (at 2.75 -2.5 90) (size 0.38 1) (layers B.Cu B.Paste B.Mask))
  )
  (module adapter:PCB_Pad (layer F.Cu) (tedit 5AC02B60)
    (at 163.8 102.3 90)
    (fp_text reference U2 (at 0 5.4 90) (layer F.SilkS) hide)
    (fp_text value USBA_Footprint (at 0 -4.1 90) (layer F.Fab) hide)
    (pad Vbus smd rect (at 3 3 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 /Vbus))
    (pad D+ smd rect (at 1 3 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 /D+))
    (pad D- smd rect (at -1 3 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /D-))
    (pad GND smd rect (at -3 3 90) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (gr_text G (at 164.3 105.3) (layer F.SilkS))
  (gr_text - (at 164.4 103.2) (layer F.SilkS))
  (gr_text "+\n" (at 164.3 101.3) (layer F.SilkS))
  (gr_text V (at 164.3 99.3) (layer F.SilkS))
  (gr_line (start 161.1 106.6) (end 167.8 106.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.9 106.4) (end 160.9 105.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.1 106.4) (end 161.1 106.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.8 98) (end 161.1 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.9 98.2) (end 160.9 98.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.1 98.2) (end 160.9 98.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.6 99.2) (end 160.3 99.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.1 105.2) (end 160.1 99.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.6 105.4) (end 160.3 105.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.3 105.2) (end 160.3 105.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.3 99.4) (end 160.1 99.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.6 98.9) (end 160.9 98.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.6 105.7) (end 160.6 105.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.1 98.3) (end 168.1 106.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.8 98.3) (end 167.8 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.8 106.3) (end 168.1 106.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.03))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.6) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 107.5) (xy 159.5 107.5) (xy 159.5 97.5) (xy 169 97.5) (xy 169 107.5)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.03))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.6) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 107.5) (xy 159.5 107.5) (xy 159.5 97.5) (xy 169 97.5) (xy 169 107.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.03))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.6) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.8 105.4) (xy 160.4 105.4) (xy 160.4 99.2) (xy 161.8 99.2) (xy 161.8 105.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.03))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.6) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168 106.5) (xy 165 106.5) (xy 165 99) (xy 168 99) (xy 168 106.5)
      )
    )
  )
)
