(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 37)
    (no_connects 0)
    (area 19.924999 18.924999 56.075001 55.075001)
    (thickness 1.6)
    (drawings 18)
    (tracks 162)
    (zones 0)
    (modules 24)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 20 19)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RAM)
  (net 3 /video_in)
  (net 4 /vtx_video)
  (net 5 +5V)
  (net 6 /vtx_audio)
  (net 7 +3V3)
  (net 8 /SPI_SLK)
  (net 9 /SPI_MOSI)
  (net 10 /SPI_CS)
  (net 11 /FC_TX1)
  (net 12 /FC_RX1)
  (net 13 /FC_TX2)
  (net 14 /FC_RX2)
  (net 15 /LED_STRIP)
  (net 16 "Net-(J8-Pad3)")
  (net 17 /ant)
  (net 18 /buz+)
  (net 19 /buz-)
  (net 20 +BATT)
  (net 21 "Net-(J4-Pad6)")
  (net 22 "Net-(J7-Pad3)")
  (net 23 "Net-(J11-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /FC_RX1)
    (add_net /FC_RX2)
    (add_net /FC_TX1)
    (add_net /FC_TX2)
    (add_net /LED_STRIP)
    (add_net /RAM)
    (add_net /SPI_CS)
    (add_net /SPI_MOSI)
    (add_net /SPI_SLK)
    (add_net /buz+)
    (add_net /buz-)
    (add_net /video_in)
    (add_net /vtx_audio)
    (add_net /vtx_video)
    (add_net GND)
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad3)")
  )
  (net_class ant ""
    (clearance 0.2)
    (trace_width 1.05)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ant)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5967D47E)
    (at 43.72 23 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RAM))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /vtx_video))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 58B1A329)
    (at 49.21 33.732 270)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 4.114 -0.828 360) (layer F.SilkS))
    (fp_text value Buzzer (at 3.8 7.4 270) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 270) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 270) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 /buz+))
    (pad 2 thru_hole circle (at 7.6 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 /buz-))
    (model Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5967D48B)
    (at 43.72 20.4 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RAM))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /video_in))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5967D447)
    (at 53.25 21.75)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5967D444)
    (at 22.75 21.75)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5967D457)
    (at 53.25 52.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 5967D4BD)
    (at 22.75 52.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connectors_JST:JST_SH_SM06B-SRSS-TB_06x1.00mm_Angled (layer F.Cu) (tedit 5967D498)
    (at 30.5 22.1 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J4 (at -2.5 -4 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 4.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at -0.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /SPI_SLK))
    (pad 4 smd rect (at 0.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /SPI_CS))
    (pad 5 smd rect (at 1.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /SPI_MOSI))
    (pad 6 smd rect (at 2.5 -1.9375 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J4-Pad6)"))
    (pad "" smd rect (at -3.8 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.8 1.9375 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5967D431)
    (at 24 39.68)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /FC_TX1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /FC_RX1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5967D435)
    (at 26.6 39.68)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /FC_TX2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /FC_RX2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module spectre:bitmap (layer F.Cu) (tedit 0)
    (at 52.1 46.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5967D424)
    (at 21.5 27 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J11-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /LED_STRIP))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5967D427)
    (at 21.5 29.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /buz-))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /buz+))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5967D42E)
    (at 21.5 39.66)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +BATT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 5967D4A2)
    (at 53.528 26.366)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J12 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value LED_5V (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 15 /LED_STRIP))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 5967D49F)
    (at 53.528 28.906)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J13 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value LED_DOUT (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 5967D49C)
    (at 53.528 31.446)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J14 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value LED_GND (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5967D486)
    (at 41.24 23)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_FEMALE (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /vtx_audio))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5967D43F)
    (at 37.846 24.892 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at 1.78 0 360) (layer F.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 6 /vtx_audio))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5967D43B)
    (at 41.24 20.4)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J15 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_FEMALE (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /video_in))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module spectre:spd15 (layer F.Cu) (tedit 5967D65D)
    (at 30.26 54.06)
    (fp_text reference U2 (at 2.252 -1.99) (layer F.SilkS) hide)
    (fp_text value SPD15 (at 13 -2) (layer F.Fab))
    (fp_text user +5V (at 13.428 -10.118) (layer F.SilkS))
    (fp_text user Sbus (at 13.428 -12.7) (layer F.SilkS))
    (fp_text user Sport (at 13.174 -15.198) (layer F.SilkS))
    (fp_text user Gnd (at 13.682 -17.78) (layer F.SilkS))
    (pad 1 thru_hole circle (at 16.637 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 16.637 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /FC_TX2))
    (pad 3 thru_hole circle (at 16.637 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /FC_RX2))
    (pad 4 thru_hole rect (at 16.637 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
  )
  (module connect-sm:U.FL-COAX (layer F.Cu) (tedit 0)
    (at 26.3 33.8 180)
    (attr smd)
    (fp_text reference J1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value COAX-JACK (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /ant))
    (pad 2 smd rect (at 0 -1.5 180) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.5 180) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module spectre:Xm+ (layer F.Cu) (tedit 5967D5A9)
    (at 42.25 54.02 90)
    (fp_text reference U3 (at 18.4 -1.25 90) (layer F.SilkS) hide)
    (fp_text value XM+ (at 17.775 -10.55 90) (layer F.Fab))
    (fp_text user GND (at 3.81 -1.651 90) (layer F.SilkS))
    (fp_text user +5V (at 3.81 -3.937 90) (layer F.SilkS))
    (fp_text user Sbus (at 3.81 -6.477 90) (layer F.SilkS))
    (fp_text user Xm/Xm+ (at 10.5 -5 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 1.12 -6.45 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /FC_RX2))
    (pad 2 thru_hole circle (at 1.12 -3.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole circle (at 1.12 -1.37 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module spectre:FX758-2 (layer B.Cu) (tedit 5967DA3D)
    (at 54 48.5 180)
    (fp_text reference U1 (at 2.54 1.27 180) (layer B.SilkS))
    (fp_text value FX758-2 (at 7 17 180) (layer B.SilkS))
    (fp_text user SLK_CH1 (at 17.145 4.445 180) (layer B.SilkS))
    (fp_text user MOSI_CH2 (at 17.145 6.985 180) (layer B.SilkS))
    (fp_text user CS_CH3 (at 17.78 9.525 180) (layer B.SilkS))
    (fp_text user GND (at 19.05 12.065 180) (layer B.SilkS))
    (fp_text user Ant (at 19.05 14.605 180) (layer B.SilkS))
    (fp_text user GND (at 19.05 17.145 180) (layer B.SilkS))
    (fp_text user GND (at 3.175 4.445 180) (layer B.SilkS))
    (fp_text user +5V (at 2.54 6.985 180) (layer B.SilkS))
    (fp_text user GND (at 3.175 9.525 180) (layer B.SilkS))
    (fp_text user "Audio In" (at 4.445 12.065 180) (layer B.SilkS))
    (fp_text user "Video In" (at 4.445 14.605 180) (layer B.SilkS))
    (pad 5 smd rect (at 0 14.66 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /vtx_video))
    (pad 4 smd rect (at 0 12.12 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /vtx_audio))
    (pad 3 smd rect (at 0 9.58 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 7.04 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 1 smd rect (at 0 4.5 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 22 4.5 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /SPI_SLK))
    (pad 10 smd rect (at 22 7.04 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /SPI_MOSI))
    (pad 9 smd rect (at 22 9.58 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 /SPI_CS))
    (pad 8 smd rect (at 22 12.12 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 22 14.66 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 /ant))
    (pad 6 smd rect (at 22 17.2 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (gr_text "Audio in" (at 38.1 23.114) (layer F.SilkS))
  (gr_text "Video In" (at 38.1 20.574) (layer F.SilkS))
  (gr_text LED (at 51.308 26.416) (layer F.SilkS))
  (gr_text GND (at 51.562 31.496) (layer F.SilkS))
  (gr_text +5V (at 51.308 28.956) (layer F.SilkS))
  (gr_text +5V (at 28.956 42.164) (layer F.SilkS))
  (gr_text GND (at 28.956 39.624) (layer F.SilkS))
  (gr_line (start 22 55) (end 53.5 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 21.5) (end 56 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 22 19) (end 53.5 19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20 53) (end 20 21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 22 21) (end 20 21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 22 53) (end 22 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 53.5 21.5) (end 53.5 19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 53.5 52.5) (end 56 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 30.5 (width 0.3) (layer Eco1.User)
    (gr_text "30,500 mm" (at 38 60.1) (layer Eco1.User))
    (feature1 (pts (xy 53.25 52.25) (xy 53.25 61.45)))
    (feature2 (pts (xy 22.75 52.25) (xy 22.75 61.45)))
    (crossbar (pts (xy 22.75 58.75) (xy 53.25 58.75)))
    (arrow1a (pts (xy 53.25 58.75) (xy 52.123496 59.336421)))
    (arrow1b (pts (xy 53.25 58.75) (xy 52.123496 58.163579)))
    (arrow2a (pts (xy 22.75 58.75) (xy 23.876504 59.336421)))
    (arrow2b (pts (xy 22.75 58.75) (xy 23.876504 58.163579)))
  )
  (dimension 36 (width 0.3) (layer Eco1.User)
    (gr_text "36,000 mm" (at 63.1 37 90) (layer Eco1.User))
    (feature1 (pts (xy 56 19) (xy 64.45 19)))
    (feature2 (pts (xy 56 55) (xy 64.45 55)))
    (crossbar (pts (xy 61.75 55) (xy 61.75 19)))
    (arrow1a (pts (xy 61.75 19) (xy 62.336421 20.126504)))
    (arrow1b (pts (xy 61.75 19) (xy 61.163579 20.126504)))
    (arrow2a (pts (xy 61.75 55) (xy 62.336421 53.873496)))
    (arrow2b (pts (xy 61.75 55) (xy 61.163579 53.873496)))
  )
  (dimension 36 (width 0.3) (layer Eco1.User)
    (gr_text "36,000 mm" (at 38 13.65) (layer Eco1.User))
    (feature1 (pts (xy 56 19) (xy 56 12.3)))
    (feature2 (pts (xy 20 19) (xy 20 12.3)))
    (crossbar (pts (xy 20 15) (xy 56 15)))
    (arrow1a (pts (xy 56 15) (xy 54.873496 15.586421)))
    (arrow1b (pts (xy 56 15) (xy 54.873496 14.413579)))
    (arrow2a (pts (xy 20 15) (xy 21.126504 15.586421)))
    (arrow2b (pts (xy 20 15) (xy 21.126504 14.413579)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56 55) (xy 20 55) (xy 20 19) (xy 56 19)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56 55) (xy 20 55) (xy 20 19) (xy 56 19)
      )
    )
  )
)
