(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 39)
    (no_connects 0)
    (area 114.774999 77.724 155.879115 147.053001)
    (thickness 1.6)
    (drawings 23)
    (tracks 182)
    (zones 0)
    (modules 7)
    (nets 34)
  )
  (page A)
  (title_block
    (title "ADV Senor Board")
    (rev 1.0)
    (company "Honeybee Robotics")
    (comment 1 "Elijah Pivo")
    (comment 2 "Project 494")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.1778)
    (user_trace_width 0.4064)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.5588)
    (via_drill 0.3048)
    (via_min_size 0.5588)
    (via_min_drill 0.3048)
    (user_via 0.5588 0.3048)
    (user_via 0.6604 0.4064)
    (user_via 1.27 1.016)
    (uvia_size 0.5588)
    (uvia_drill 0.3048)
    (uvias_allowed no)
    (uvia_min_size 0.5588)
    (uvia_min_drill 0.3048)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0635)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(J2-Pad8)")
  (net 4 "Net-(J2-Pad10)")
  (net 5 "Net-(J5-Pad2)")
  (net 6 +3V3)
  (net 7 /int_tof1)
  (net 8 /en_tof1)
  (net 9 /scl)
  (net 10 /sda)
  (net 11 /int_tof2)
  (net 12 /en_tof2)
  (net 13 /int_tof3)
  (net 14 /en_tof3)
  (net 15 /led-pwm)
  (net 16 "Net-(J2-Pad7)")
  (net 17 "Net-(J2-Pad11)")
  (net 18 "Net-(J2-Pad13)")
  (net 19 "Net-(J2-Pad19)")
  (net 20 "Net-(J2-Pad21)")
  (net 21 "Net-(J2-Pad22)")
  (net 22 "Net-(J2-Pad23)")
  (net 23 "Net-(J2-Pad24)")
  (net 24 "Net-(J2-Pad26)")
  (net 25 "Net-(J2-Pad27)")
  (net 26 "Net-(J2-Pad28)")
  (net 27 "Net-(J2-Pad29)")
  (net 28 "Net-(J2-Pad31)")
  (net 29 "Net-(J2-Pad32)")
  (net 30 "Net-(J2-Pad33)")
  (net 31 "Net-(J2-Pad36)")
  (net 32 "Net-(J2-Pad37)")
  (net 33 "Net-(J2-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.1778)
    (via_dia 0.5588)
    (via_drill 0.3048)
    (uvia_dia 0.5588)
    (uvia_drill 0.3048)
    (add_net +3V3)
    (add_net +5V)
    (add_net /en_tof1)
    (add_net /en_tof2)
    (add_net /en_tof3)
    (add_net /int_tof1)
    (add_net /int_tof2)
    (add_net /int_tof3)
    (add_net /led-pwm)
    (add_net /scl)
    (add_net /sda)
    (add_net GND)
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J5-Pad2)")
  )
  (module adv-sensor-board:Conn_Molex_Micro-Fit_3.0_43650-0201_1x02_P3.00mm_Horizontal (layer F.Cu) (tedit 5AA144EC)
    (at 132.08 127 270)
    (fp_text reference J1 (at -4.1456 -1.6156 270) (layer F.SilkS))
    (fp_text value pwr_conn (at -1.504 7.376 270) (layer F.Fab))
    (fp_text user %R (at -0.996 2.042 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -3 0 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad "" np_thru_hole circle (at -1.5 4.32 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 133.223 106.68 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 4.385 -2.27 180) (layer F.SilkS))
    (fp_text value fan_conn (at 4.385 4.81 180) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B03211B)
    (at 133.223 115.062 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27 180) (layer F.SilkS))
    (fp_text value fan_conn (at 2.54 -3.81 180) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adv-sensor-board:Molex_CLIK-Mate_503175-0310_1x03_P1.50mm_Horizontal (layer F.Cu) (tedit 5AFC8367)
    (at 129.921 93.345 270)
    (fp_text reference J5 (at -0.508 -1.524 270) (layer F.SilkS))
    (fp_text value led-ring_conn (at 1.524 4.572 270) (layer F.Fab))
    (fp_text user %R (at 2.032 3.302 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.55 1.85 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.5 3.7 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J5-Pad2)"))
    (pad 3 thru_hole circle (at 3 0 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad "" np_thru_hole circle (at -1.55 1.85 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module adv-sensor-board:Conn_Molex_CLIK-Mate_503148-1890_2x09_P1.50mm_Horizontal (layer F.Cu) (tedit 5B0305BC)
    (at 144.526 135.128)
    (clearance 0.0254)
    (fp_text reference J6 (at -13.716 -2.286) (layer F.SilkS))
    (fp_text value tof_conn (at -6.4135 1.905) (layer F.Fab))
    (fp_text user %R (at -6.0325 4.191) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -0.75 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.5 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /int_tof1))
    (pad 4 smd rect (at -2.25 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /en_tof1))
    (pad 5 smd rect (at -3 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /scl))
    (pad 6 smd rect (at -3.75 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /sda))
    (pad 7 smd rect (at -4.5 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 8 smd rect (at -5.25 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -6 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /int_tof2))
    (pad 10 smd rect (at -6.75 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /en_tof2))
    (pad 11 smd rect (at -7.5 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /scl))
    (pad 12 smd rect (at -8.25 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /sda))
    (pad 13 smd rect (at -9 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 14 smd rect (at -9.75 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -10.5 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /int_tof3))
    (pad 16 smd rect (at -11.25 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /en_tof3))
    (pad 17 smd rect (at -12 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /scl))
    (pad 18 smd rect (at -12.75 0) (size 0.55 2.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /sda))
    (pad "" smd rect (at 2.23 5.175) (size 1.2 4.65) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -14.98 5.175) (size 1.2 4.65) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-553 (layer F.Cu) (tedit 5B03227A)
    (at 132.461 97.917 270)
    (descr SOT553)
    (tags SOT-553)
    (clearance 0.0254)
    (attr smd)
    (fp_text reference U1 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value SN74AHCT1G125DRLR (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 450) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -0.5 270) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.7 0.5 270) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.7 -0.5 270) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.7 0 270) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /led-pwm))
    (pad 4 smd rect (at 0.7 0.5 270) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer B.Cu) (tedit 59650533)
    (at 149.1234 134.8232)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value rpizerow_conn (at 1.27 -50.59) (layer B.Fab))
    (fp_text user %R (at 1.27 -24.13 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /sda))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /scl))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /led-pwm))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /int_tof2))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /en_tof3))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /int_tof3))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad24)"))
    (pad 25 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad28)"))
    (pad 29 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad32)"))
    (pad 33 thru_hole oval (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /en_tof1))
    (pad 36 thru_hole oval (at 2.54 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad36)"))
    (pad 37 thru_hole oval (at 0 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /int_tof1))
    (pad 39 thru_hole oval (at 0 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /en_tof2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev 1.0\nElijah Pivo\n05/30/18" (at 130.302 82.931) (layer F.Cu))
  (gr_text "ADV Sensor Board" (at 137.16 79.883) (layer F.SilkS))
  (gr_arc (start 127.051 139.369) (end 127.051 143.244) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.301 139.369) (end 153.176 139.369) (angle 89.9) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.301 82.119) (end 149.301 78.244) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 127.051 82.119) (end 123.176 82.119) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.301 78.244) (end 127.051 78.244) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.176 139.369) (end 153.176 82.119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.051 143.244) (end 149.301 143.244) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.176 82.119) (end 123.176 139.369) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.416 143.764) (xy 122.936 143.764) (xy 122.936 77.724) (xy 153.416 77.724)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.416 143.764) (xy 122.936 143.764) (xy 122.936 77.724) (xy 153.416 77.724)
      )
    )
  )
)
