(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 479)
    (no_connects 183)
    (area 12.746667 63.224999 266.653334 141.045001)
    (thickness 1.6)
    (drawings 18)
    (tracks 802)
    (zones 0)
    (modules 174)
    (nets 18)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF7FF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 +12V)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 -24V)
  (net 6 +5V)
  (net 7 GND)
  (net 8 SDA)
  (net 9 SCL)
  (net 10 "Net-(Q1-Pad2)")
  (net 11 ONSET)
  (net 12 HOLD)
  (net 13 LED)
  (net 14 "Net-(D4-Pad2)")
  (net 15 "Net-(D5-Pad2)")
  (net 16 "Net-(D6-Pad2)")
  (net 17 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net HOLD)
    (add_net LED)
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net ONSET)
  )
  (net_class POWER ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -24V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
  )
  (net_class i2c ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net SCL)
    (add_net SDA)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A070047)
    (at 17.78 85.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A070047)
    (at 17.78 132.08)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A070047)
    (at 261.62 132.08)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module Connectors_Samtec:SL-106-X-XX_1x06 (layer F.Cu) (tedit 5A070441)
    (at 257.175 78.74 180)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference P1 (at -2.27 6.35 270) (layer F.SilkS) hide)
    (fp_text value CONN_1x6 (at 2.27 6.35 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 -24V))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-106-X-XX_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A07030C)
    (at 206.375 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference A (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A07031A)
    (at 226.06 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference A# (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A070326)
    (at 245.745 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference B (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702D1)
    (at 107.95 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference E (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702ED)
    (at 167.005 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference G (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702F7)
    (at 186.69 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference G# (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702DA)
    (at 127.635 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference F (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702C8)
    (at 88.265 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference D# (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702E3)
    (at 147.32 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference F# (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702BE)
    (at 68.58 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference D (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A0702A5)
    (at 48.895 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference C# (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 26.67 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5A070297)
    (at 29.21 137.16 90)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference C (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Solenoid (at 2.27 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A070047)
    (at 261.62 86.36)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 225.425 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 220.345 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 233.045 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 227.965 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 222.885 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 220.345 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 226.695 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 226.695 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 233.045 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 220.345 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 221.615 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 231.775 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 223.52 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 85.725 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 93.98 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 83.82 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 82.55 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 95.25 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 88.9 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 88.9 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 82.55 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 85.09 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 90.17 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 95.25 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 82.55 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 87.63 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 67.945 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 62.865 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 75.565 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 70.485 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 65.405 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 62.865 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 69.215 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 69.215 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 75.565 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 62.865 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 64.135 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 74.295 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 66.04 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 105.41 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 113.665 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 103.505 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 102.235 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 114.935 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 108.585 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 108.585 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 102.235 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 104.775 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 109.855 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 114.935 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 102.235 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 107.315 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 127 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 121.92 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 134.62 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 129.54 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 124.46 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 121.92 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 128.27 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 128.27 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 134.62 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 121.92 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 123.19 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 133.35 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 125.095 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 203.835 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 212.09 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 201.93 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 200.66 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 213.36 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 207.01 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 207.01 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 200.66 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 203.2 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 208.28 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 213.36 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 200.66 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 205.74 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 186.055 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 180.975 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 193.675 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 188.595 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 183.515 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 180.975 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 187.325 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 187.325 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 193.675 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 180.975 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 182.245 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 192.405 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 184.15 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 144.78 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 153.035 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 142.875 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 141.605 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 154.305 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 147.955 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 147.955 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 141.605 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 144.145 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 149.225 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 154.305 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 141.605 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 146.685 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 46.355 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 54.61 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 44.45 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 43.18 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 55.88 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 49.53 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 49.53 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 43.18 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 45.72 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 50.8 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 55.88 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 43.18 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 48.26 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 166.37 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 161.29 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 173.99 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 168.91 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 163.83 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 161.29 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 167.64 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 167.64 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 173.99 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 161.29 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 162.56 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 172.72 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 164.465 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-106-X-XX_1x06 (layer F.Cu) (tedit 5A070450)
    (at 23.495 78.74 180)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference P1 (at -2.27 6.35 270) (layer F.SilkS) hide)
    (fp_text value CONN_1x6 (at 2.27 6.35 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 -24V))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-106-X-XX_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 245.11 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 240.03 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 252.73 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 247.65 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 242.57 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 240.03 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 246.38 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 246.38 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 252.73 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 240.03 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 241.3 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 251.46 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A36C)
    (at 243.205 132.08)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D1 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value BYV23-200 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048631)
    (at 34.925 119.38 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A04A34D)
    (at 24.765 101.6 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 0 270) (layer F.SilkS))
    (fp_text value SF52 (at 7.62 3.66 270) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P12.70mm_Horizontal (layer F.Cu) (tedit 5A04A349)
    (at 23.495 123.19)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 6.35 0) (layer F.SilkS))
    (fp_text value Z10V (at 6.35 2.06) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A048660)
    (at 36.195 102.87 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.27 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A352)
    (at 29.845 101.6 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRL640 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5A04A356)
    (at 29.845 113.03 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value IRF610 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5A048613)
    (at 23.495 127)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 4k7 (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -24V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 26.035 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 31.115 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value HOLD (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 36.195 95.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value ONSET (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A05CB9D)
    (at 23.495 83.82 270)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A05CBA0)
    (at 28.575 90.17 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.175 6.35 90) (layer F.SilkS))
    (fp_text value ATTINY85-20MU (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 HOLD))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 LED))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ONSET))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 13.97 63.5) (end 14.605 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 13.97 140.97) (end 13.97 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 265.43 140.97) (end 13.97 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 265.43 63.5) (end 265.43 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 13.97 63.5) (end 265.43 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "+12V\n" (at 17.78 66.04) (layer F.SilkS))
  (gr_text -24V (at 17.78 68.58) (layer F.SilkS))
  (gr_text SDA (at 17.145 71.12) (layer F.SilkS))
  (gr_text SCL (at 17.145 73.66) (layer F.SilkS))
  (gr_text +5V (at 17.145 76.2) (layer F.SilkS))
  (gr_text GND (at 17.145 78.74) (layer F.SilkS))
  (gr_text GND (at 262.255 78.74) (layer F.SilkS))
  (gr_text +5V (at 262.255 76.2) (layer F.SilkS))
  (gr_text SCL (at 262.255 73.66) (layer F.SilkS))
  (gr_text SDA (at 262.255 71.12) (layer F.SilkS))
  (gr_text SDA (at 241.3 71.12) (layer F.Paste))
  (gr_text -24V (at 262.255 68.58) (layer F.SilkS))
  (gr_text "+12V\n" (at 262.255 66.04) (layer F.SilkS))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 265.43 140.97) (xy 13.97 140.97) (xy 13.97 63.5) (xy 265.43 63.5)
      )
    )
  )
)
