<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="34.29" y2="0" width="0" layer="20"/>
<wire x1="34.29" y1="0" x2="34.29" y2="35.56" width="0" layer="20"/>
<wire x1="34.29" y1="35.56" x2="0" y2="35.56" width="0" layer="20"/>
<wire x1="0" y1="35.56" x2="0" y2="0" width="0" layer="20"/>
<hole x="30.48" y="31.75" drill="3.175"/>
<hole x="30.48" y="6.985" drill="3.175"/>
<hole x="3.81" y="31.75" drill="3.175"/>
<hole x="5.715" y="2.38125" drill="1.2954"/>
<hole x="16.51" y="2.38125" drill="1.2954"/>
<hole x="1.9685" y="6.08965" drill="0.9906"/>
<hole x="9.4615" y="6.08965" drill="0.9906"/>
<hole x="12.7635" y="6.08965" drill="0.9906"/>
<hole x="20.2565" y="6.08965" drill="0.9906"/>
<text>Inty Composite Mod 1.0</text>
<text>21 JUN 2018</text>
<text>VID</text>
<text>AUD</text>
<hole x="5.08" y="12.7" drill="3.175"/>
<text>VCC</text>
<text>VIDEO</text>
<text>AUDIO</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switchcraft">
<packages>
<package name="PJRAN1X1U">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="51k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.4" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.4" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.4" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.4" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="switchcraft" package="PJRAN1X1U" value="VID">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="switchcraft" package="PJRAN1X1U" value="AUD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R4" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="T1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="P$1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="T2" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="1"/>
<contactref element="R6" pad="P$1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="T1" pad="3"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="T2" pad="1"/>
<contactref element="R8" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="T2" pad="3"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="JP1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R4" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="JP1" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="VID_IN">
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="AUD_IN">
<contactref element="JP1" pad="3"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VID_OUT">
<contactref element="J1" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="AUD_OUT">
<contactref element="J2" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
