(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 40)
    (no_connects 0)
    (area 160.3 100.714266 195.200001 131.200001)
    (thickness 1.6002)
    (drawings 22)
    (tracks 74)
    (zones 0)
    (modules 13)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "SSD1306 SPI Breakout v1.0")
    (date 2017-02-08)
    (rev A)
    (company "Rene van der Meer / rene@golemparts.com / @GolemParts")
    (comment 2 https://creativecommons.org/licenses/by-sa/4.0/.)
    (comment 3 "License. To view a copy of this license, visit")
    (comment 4 "This work is licensed under the Creative Commons Attribution-ShareAlike 4.0 International")
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.0254)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6858 0.6858)
    (pad_drill 0.3302)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 /MOSI)
  (net 10 /SCK)
  (net 11 /OLED_CS)
  (net 12 /OLED_DC)
  (net 13 /OLED_RST)
  (net 14 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /MOSI)
    (add_net /OLED_CS)
    (add_net /OLED_DC)
    (add_net /OLED_RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(R1-Pad1)")
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 589FBBD2)
    (at 177.35 125.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.4 0.25) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 589F6A75)
    (at 180.9 113.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 589FBB44)
    (at 180.9 121.15)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D21F)
    (at 173.2 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C1 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 1µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D213)
    (at 185.8 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C2 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 2.2µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D223)
    (at 171.1 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C3 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 1µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D228)
    (at 169 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C4 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 1µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D20D)
    (at 166.9 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C5 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 1µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D218)
    (at 187.9 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference C6 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 4.7µF (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D209)
    (at 183.7 118.5 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R1 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 390k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:0805_HandSoldering (layer Bottom) (tedit 58A1D200)
    (at 173.2 111.35 90)
    (descr "SMD 0805, hand soldering")
    (tags 0805)
    (attr smd)
    (fp_text reference R2 (at 2.8 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 11 /OLED_CS))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:Pin_Header_Straight_1x07_Pitch2.54mm (layer Top) (tedit 58A1D1FB)
    (at 177.75 105.7 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P1 (at 0 -10.414 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 10.16 90) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /OLED_CS))
    (pad 4 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /OLED_RST))
    (pad 5 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /OLED_DC))
    (pad 6 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCK))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /MOSI))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Golemparts:FPC30_0.7 (layer Bottom) (tedit 58A1DD26)
    (at 177.75 123.55)
    (tags "FPC FFC flat flex cable flexible printed circuit 30 0.7 mm")
    (fp_text reference U1 (at 0.35 -3.81) (layer B.SilkS) hide)
    (fp_text value ER-OLED013-1 (at 0.35 5.08) (layer B.Fab))
    (pad 1 smd rect (at -10.15 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -9.45 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 3 smd rect (at -8.75 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 4 smd rect (at -8.05 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -7.35 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 6 smd rect (at -6.65 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -5.95 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask))
    (pad 8 smd rect (at -5.25 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -4.55 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -3.85 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -3.15 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -2.45 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -1.75 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 11 /OLED_CS))
    (pad 14 smd rect (at -1.05 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 13 /OLED_RST))
    (pad 15 smd rect (at -0.35 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 12 /OLED_DC))
    (pad 16 smd rect (at 0.35 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 1.05 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 1.75 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 10 /SCK))
    (pad 19 smd rect (at 2.45 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 9 /MOSI))
    (pad 20 smd rect (at 3.15 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask))
    (pad 21 smd rect (at 3.85 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.55 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 5.25 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.95 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 6.65 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 7.35 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 27 smd rect (at 8.05 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 28 smd rect (at 8.75 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 29 smd rect (at 9.45 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 30 smd rect (at 10.15 0) (size 0.4 2.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
  )
  (gr_text 30 (at 189 123.5 270) (layer B.SilkS))
  (gr_text 1 (at 166.5 123.5 270) (layer B.SilkS))
  (gr_text "SSD1306 SPI Breakout v1.0 A\nRene van der Meer @GolemParts\nCC BY-SA 4.0\n " (at 192.1 130.4 270) (layer B.SilkS))
  (gr_text "3.3 V\n3.3 V" (at 164.45 105.8) (layer B.SilkS))
  (gr_text "Power:\nLogic:" (at 168.2 105.8) (layer B.SilkS))
  (gr_arc (start 192.5 106.2) (end 195 106.2) (angle -90) (layer Edge.Cuts) (width 0.00254))
  (gr_arc (start 163 106.2) (end 160.5 106.2) (angle 90) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 195 106.2) (end 195 131) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 163 103.7) (end 192.5 103.7) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 160.5 131) (end 160.5 106.2) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 160.5 131) (end 195 131) (layer Edge.Cuts) (width 0.00254))
  (gr_text RST (at 177.75 107.45) (layer F.SilkS))
  (gr_text DC (at 180.29 107.45) (layer F.SilkS))
  (gr_text CS (at 175.21 107.45) (layer F.SilkS))
  (gr_text SCK (at 182.83 107.45) (layer F.SilkS))
  (gr_text MOSI (at 185.37 107.45) (layer F.SilkS))
  (gr_text 3.3V (at 172.67 107.45) (layer F.SilkS))
  (gr_text GND (at 170.13 107.45) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 103.6) (xy 160.3 131.2) (xy 195.2 131.2) (xy 195.2 103.6)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 103.6) (xy 160.3 131.2) (xy 195.2 131.2) (xy 195.2 103.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.6148 106.2482) (xy 194.4497 105.41) (xy 193.9925 104.7242) (xy 193.3067 104.2543) (xy 192.4558 104.0892)
        (xy 192.4558 104.013) (xy 194.6656 104.013) (xy 194.6656 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8836 106.2482) (xy 161.0487 105.41) (xy 161.5059 104.7242) (xy 162.1917 104.2543) (xy 163.0426 104.0892)
        (xy 163.0426 104.013) (xy 160.8328 104.013) (xy 160.8328 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.0426 104.0892) (xy 163.0426 104.013) (xy 192.4558 104.013) (xy 192.4558 104.0892)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8836 106.2482) (xy 160.8836 130.5052) (xy 160.8963 130.5433) (xy 160.9217 130.5814) (xy 160.9598 130.6068)
        (xy 160.9979 130.6068) (xy 160.9979 130.6576) (xy 160.8328 130.6576) (xy 160.8328 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.6148 106.2482) (xy 194.6148 130.5052) (xy 194.6021 130.5433) (xy 194.5767 130.5814) (xy 194.5386 130.6068)
        (xy 194.5005 130.6068) (xy 194.5005 130.6576) (xy 194.6656 130.6576) (xy 194.6656 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.5005 130.6068) (xy 194.5005 130.6576) (xy 160.9979 130.6576) (xy 160.9979 130.6068)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.6148 106.2482) (xy 194.6148 130.5052) (xy 194.6021 130.5433) (xy 194.5767 130.5814) (xy 194.5386 130.6068)
        (xy 194.5005 130.6068) (xy 194.5005 130.6576) (xy 194.6656 130.6576) (xy 194.6656 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8836 106.2482) (xy 160.8836 130.5052) (xy 160.8963 130.5433) (xy 160.9217 130.5814) (xy 160.9598 130.6068)
        (xy 160.9979 130.6068) (xy 160.9979 130.6576) (xy 160.8328 130.6576) (xy 160.8328 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.5005 130.6576) (xy 194.5005 130.6068) (xy 160.9979 130.6068) (xy 160.9979 130.6576)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8836 106.2482) (xy 161.0487 105.41) (xy 161.5059 104.7242) (xy 162.1917 104.2543) (xy 163.0426 104.0892)
        (xy 163.0426 104.013) (xy 160.8328 104.013) (xy 160.8328 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.6148 106.2482) (xy 194.4497 105.41) (xy 193.9925 104.7242) (xy 193.3067 104.2543) (xy 192.4558 104.0892)
        (xy 192.4558 104.013) (xy 194.6656 104.013) (xy 194.6656 106.2482)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.0426 104.013) (xy 163.0426 104.0892) (xy 192.4558 104.0892) (xy 192.4558 104.013)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.5 105.8) (xy 185.05 105.8) (xy 185.05 105.85) (xy 173.5 105.85)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.361348 122.05) (xy 172.9 122.05) (xy 172.9 122.1) (xy 171.361348 122.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.461348 122.05) (xy 179.35 122.05) (xy 179.35 122.1) (xy 173.461348 122.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.5 122.2) (xy 188 122.3) (xy 188 124.7) (xy 167.5 124.7)
      )
    )
  )
)
