(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 0)
    (no_connects 6)
    (area 72.459287 84.742 159.488 166.403001)
    (thickness 1.6)
    (drawings 31)
    (tracks 41)
    (zones 0)
    (modules 13)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 36.195 94.742)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 "Net-(P1-Pad8)")
  (net 9 "Net-(P1-Pad9)")
  (net 10 "Net-(P1-Pad10)")
  (net_class Default "Esta es la clase de red por defecto."
    (clearance 0.254)
    (trace_width 0.635)
    (via_dia 0.508)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 588DD6BF)
    (at 99.545 132.08)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.25 -2) (layer F.SilkS))
    (fp_text value btn2 (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad9)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad9)"))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 588DD760)
    (at 125.095 144.272)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 588DD764)
    (at 98.425 144.272)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0.127 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 588DD758)
    (at 125.095 101.092)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588DD709)
    (at 109.728 100.838)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference Shoulder (at 1.27 -2.413) (layer F.SilkS))
    (fp_text value Shoulder (at 0.635 -2.286) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 588DD6C2)
    (at 107.442 123.952)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value btn1 (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad10)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad10)"))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 588DD6C8)
    (at 114.935 132.08)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.25 -2) (layer F.SilkS))
    (fp_text value btn3 (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 588DD6CD)
    (at 107.442 140.242)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 3.25 -2) (layer F.SilkS))
    (fp_text value btn4 (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ALPS_SKQUAAA010 (layer F.Cu) (tedit 588DD724)
    (at 105.905 105.012)
    (fp_text reference Joystick (at 5.347 5.351) (layer F.SilkS))
    (fp_text value joystick (at 5.474 3.573) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 6 thru_hole circle (at 10.3 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 10.3 6.5) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 6.5) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 2 thru_hole circle (at 0 3.7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 5 thru_hole circle (at 10.3 3.7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x05 (layer F.Cu) (tedit 588DD737)
    (at 124.333 113.792 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference Header (at -2.413 1.27 360) (layer F.SilkS))
    (fp_text value "" (at 4.445 -2.032 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad10)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x05.wrl
      (at (xyz 0.2 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 588DD754)
    (at 98.425 101.092)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 98.895 109.342 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module footprints:ludus (layer B.Cu) (tedit 0)
    (at 100.895 119.942 180)
    (fp_text reference G*** (at 8.4 -0.7 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 8.5 1.4 180) (layer B.SilkS) hide)
  )
  (gr_text "Ludus Button Pad v1.0" (at 96.395 119.942 90) (layer F.SilkS))
  (dimension 4.1 (width 0.3) (layer Dwgs.User)
    (gr_text "4.100 mm" (at 78.245 98.992 90) (layer Dwgs.User))
    (feature1 (pts (xy 98.395 96.942) (xy 76.895 96.942)))
    (feature2 (pts (xy 98.395 101.042) (xy 76.895 101.042)))
    (crossbar (pts (xy 79.595 101.042) (xy 79.595 96.942)))
    (arrow1a (pts (xy 79.595 96.942) (xy 80.181421 98.068504)))
    (arrow1b (pts (xy 79.595 96.942) (xy 79.008579 98.068504)))
    (arrow2a (pts (xy 79.595 101.042) (xy 80.181421 99.915496)))
    (arrow2b (pts (xy 79.595 101.042) (xy 79.008579 99.915496)))
  )
  (dimension 3.9 (width 0.3) (layer Dwgs.User)
    (gr_text "3.900 mm" (at 96.445 86.092) (layer Dwgs.User))
    (feature1 (pts (xy 94.495 101.042) (xy 94.495 84.742)))
    (feature2 (pts (xy 98.395 101.042) (xy 98.395 84.742)))
    (crossbar (pts (xy 98.395 87.442) (xy 94.495 87.442)))
    (arrow1a (pts (xy 94.495 87.442) (xy 95.621504 86.855579)))
    (arrow1b (pts (xy 94.495 87.442) (xy 95.621504 88.028421)))
    (arrow2a (pts (xy 98.395 87.442) (xy 97.268496 86.855579)))
    (arrow2b (pts (xy 98.395 87.442) (xy 97.268496 88.028421)))
  )
  (dimension 7.7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.700 mm" (at 114.445 152.692) (layer Dwgs.User))
    (feature1 (pts (xy 118.295 134.342) (xy 118.295 154.042)))
    (feature2 (pts (xy 110.595 134.342) (xy 110.595 154.042)))
    (crossbar (pts (xy 110.595 151.342) (xy 118.295 151.342)))
    (arrow1a (pts (xy 118.295 151.342) (xy 117.168496 151.928421)))
    (arrow1b (pts (xy 118.295 151.342) (xy 117.168496 150.755579)))
    (arrow2a (pts (xy 110.595 151.342) (xy 111.721504 151.928421)))
    (arrow2b (pts (xy 110.595 151.342) (xy 111.721504 150.755579)))
  )
  (dimension 25.654 (width 0.3) (layer Dwgs.User)
    (gr_text "25.654 mm" (at 152.988 121.539 90) (layer Dwgs.User))
    (feature1 (pts (xy 110.617 108.712) (xy 154.338 108.712)))
    (feature2 (pts (xy 110.617 134.366) (xy 154.338 134.366)))
    (crossbar (pts (xy 151.638 134.366) (xy 151.638 108.712)))
    (arrow1a (pts (xy 151.638 108.712) (xy 152.224421 109.838504)))
    (arrow1b (pts (xy 151.638 108.712) (xy 151.051579 109.838504)))
    (arrow2a (pts (xy 151.638 134.366) (xy 152.224421 133.239496)))
    (arrow2b (pts (xy 151.638 134.366) (xy 151.051579 133.239496)))
  )
  (dimension 11.938 (width 0.3) (layer Dwgs.User)
    (gr_text "11.938 mm" (at 145.622 128.397 90) (layer Dwgs.User))
    (feature1 (pts (xy 110.617 122.428) (xy 146.972 122.428)))
    (feature2 (pts (xy 110.617 134.366) (xy 146.972 134.366)))
    (crossbar (pts (xy 144.272 134.366) (xy 144.272 122.428)))
    (arrow1a (pts (xy 144.272 122.428) (xy 144.858421 123.554504)))
    (arrow1b (pts (xy 144.272 122.428) (xy 143.685579 123.554504)))
    (arrow2a (pts (xy 144.272 134.366) (xy 144.858421 133.239496)))
    (arrow2b (pts (xy 144.272 134.366) (xy 143.685579 133.239496)))
  )
  (dimension 50.927 (width 0.3) (layer Dwgs.User)
    (gr_text "50.927 mm" (at 85.01 122.4915 90) (layer Dwgs.User))
    (feature1 (pts (xy 97.79 97.028) (xy 83.66 97.028)))
    (feature2 (pts (xy 97.79 147.955) (xy 83.66 147.955)))
    (crossbar (pts (xy 86.36 147.955) (xy 86.36 97.028)))
    (arrow1a (pts (xy 86.36 97.028) (xy 86.946421 98.154504)))
    (arrow1b (pts (xy 86.36 97.028) (xy 85.773579 98.154504)))
    (arrow2a (pts (xy 86.36 147.955) (xy 86.946421 146.828496)))
    (arrow2b (pts (xy 86.36 147.955) (xy 85.773579 146.828496)))
  )
  (dimension 33.909 (width 0.3) (layer Dwgs.User)
    (gr_text "33.909 mm" (at 111.5695 165.053) (layer Dwgs.User))
    (feature1 (pts (xy 94.615 144.272) (xy 94.615 166.403)))
    (feature2 (pts (xy 128.524 144.272) (xy 128.524 166.403)))
    (crossbar (pts (xy 128.524 163.703) (xy 94.615 163.703)))
    (arrow1a (pts (xy 94.615 163.703) (xy 95.741504 163.116579)))
    (arrow1b (pts (xy 94.615 163.703) (xy 95.741504 164.289421)))
    (arrow2a (pts (xy 128.524 163.703) (xy 127.397496 163.116579)))
    (arrow2b (pts (xy 128.524 163.703) (xy 127.397496 164.289421)))
  )
  (dimension 11.684 (width 0.3) (layer Dwgs.User)
    (gr_text "11.684 mm" (at 132.033 102.87 90) (layer Dwgs.User))
    (feature1 (pts (xy 111.379 97.028) (xy 133.383 97.028)))
    (feature2 (pts (xy 111.379 108.712) (xy 133.383 108.712)))
    (crossbar (pts (xy 130.683 108.712) (xy 130.683 97.028)))
    (arrow1a (pts (xy 130.683 97.028) (xy 131.269421 98.154504)))
    (arrow1b (pts (xy 130.683 97.028) (xy 130.096579 98.154504)))
    (arrow2a (pts (xy 130.683 108.712) (xy 131.269421 107.585496)))
    (arrow2b (pts (xy 130.683 108.712) (xy 130.096579 107.585496)))
  )
  (dimension 8.382 (width 0.3) (layer Dwgs.User)
    (gr_text "8.382 mm" (at 138.129 138.557 270) (layer Dwgs.User))
    (feature1 (pts (xy 118.237 142.748) (xy 139.479 142.748)))
    (feature2 (pts (xy 118.237 134.366) (xy 139.479 134.366)))
    (crossbar (pts (xy 136.779 134.366) (xy 136.779 142.748)))
    (arrow1a (pts (xy 136.779 142.748) (xy 136.192579 141.621496)))
    (arrow1b (pts (xy 136.779 142.748) (xy 137.365421 141.621496)))
    (arrow2a (pts (xy 136.779 134.366) (xy 136.192579 135.492504)))
    (arrow2b (pts (xy 136.779 134.366) (xy 137.365421 135.492504)))
  )
  (dimension 8.128 (width 0.3) (layer Dwgs.User)
    (gr_text "8.128 mm" (at 132.795 130.302 270) (layer Dwgs.User))
    (feature1 (pts (xy 110.617 134.366) (xy 134.145 134.366)))
    (feature2 (pts (xy 110.617 126.238) (xy 134.145 126.238)))
    (crossbar (pts (xy 131.445 126.238) (xy 131.445 134.366)))
    (arrow1a (pts (xy 131.445 134.366) (xy 130.858579 133.239496)))
    (arrow1b (pts (xy 131.445 134.366) (xy 132.031421 133.239496)))
    (arrow2a (pts (xy 131.445 126.238) (xy 130.858579 127.364504)))
    (arrow2b (pts (xy 131.445 126.238) (xy 132.031421 127.364504)))
  )
  (dimension 7.874 (width 0.3) (layer Dwgs.User)
    (gr_text "7.874 mm" (at 106.68 152.734) (layer Dwgs.User))
    (feature1 (pts (xy 110.617 134.366) (xy 110.617 154.084)))
    (feature2 (pts (xy 102.743 134.366) (xy 102.743 154.084)))
    (crossbar (pts (xy 102.743 151.384) (xy 110.617 151.384)))
    (arrow1a (pts (xy 110.617 151.384) (xy 109.490496 151.970421)))
    (arrow1b (pts (xy 110.617 151.384) (xy 109.490496 150.797579)))
    (arrow2a (pts (xy 102.743 151.384) (xy 103.869504 151.970421)))
    (arrow2b (pts (xy 102.743 151.384) (xy 103.869504 150.797579)))
  )
  (dimension 15.494 (width 0.3) (layer Dwgs.User)
    (gr_text "15.494 mm" (at 110.49 160.862) (layer Dwgs.User))
    (feature1 (pts (xy 118.237 134.366) (xy 118.237 162.212)))
    (feature2 (pts (xy 102.743 134.366) (xy 102.743 162.212)))
    (crossbar (pts (xy 102.743 159.512) (xy 118.237 159.512)))
    (arrow1a (pts (xy 118.237 159.512) (xy 117.110496 160.098421)))
    (arrow1b (pts (xy 118.237 159.512) (xy 117.110496 158.925579)))
    (arrow2a (pts (xy 102.743 159.512) (xy 103.869504 160.098421)))
    (arrow2b (pts (xy 102.743 159.512) (xy 103.869504 158.925579)))
  )
  (dimension 43.18 (width 0.3) (layer Dwgs.User)
    (gr_text "43.180 mm" (at 90.725 122.682 90) (layer Dwgs.User))
    (feature1 (pts (xy 98.425 101.092) (xy 89.375 101.092)))
    (feature2 (pts (xy 98.425 144.272) (xy 89.375 144.272)))
    (crossbar (pts (xy 92.075 144.272) (xy 92.075 101.092)))
    (arrow1a (pts (xy 92.075 101.092) (xy 92.661421 102.218504)))
    (arrow1b (pts (xy 92.075 101.092) (xy 91.488579 102.218504)))
    (arrow2a (pts (xy 92.075 144.272) (xy 92.661421 143.145496)))
    (arrow2b (pts (xy 92.075 144.272) (xy 91.488579 143.145496)))
  )
  (dimension 26.67 (width 0.3) (layer Dwgs.User)
    (gr_text "26.670 mm" (at 111.76 93.392) (layer Dwgs.User))
    (feature1 (pts (xy 125.095 101.092) (xy 125.095 92.042)))
    (feature2 (pts (xy 98.425 101.092) (xy 98.425 92.042)))
    (crossbar (pts (xy 98.425 94.742) (xy 125.095 94.742)))
    (arrow1a (pts (xy 125.095 94.742) (xy 123.968496 95.328421)))
    (arrow1b (pts (xy 125.095 94.742) (xy 123.968496 94.155579)))
    (arrow2a (pts (xy 98.425 94.742) (xy 99.551504 95.328421)))
    (arrow2b (pts (xy 98.425 94.742) (xy 99.551504 94.155579)))
  )
  (gr_line (start 97.506 96.928) (end 125.506 96.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.506 99.928) (end 128.506 144.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.506 147.928) (end 97.506 147.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 94.506 144.928) (end 94.506 99.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 125.506 99.928) (end 125.506 96.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 125.506 144.928) (end 128.506 144.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 97.506 144.928) (end 97.506 147.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 97.506 99.928) (end 94.506 99.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 97.506 96.928) (end 125.506 96.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.506 99.928) (end 128.506 144.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.506 147.928) (end 97.506 147.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 94.506 144.928) (end 94.506 99.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 125.506 99.928) (end 125.506 96.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 125.506 144.928) (end 128.506 144.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 97.506 144.928) (end 97.506 147.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 97.506 99.928) (end 94.506 99.928) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 94.996) (xy 135.509 94.996) (xy 135.509 153.035) (xy 91.059 153.035) (xy 89.789 117.602)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.233 93.218) (xy 142.113 93.218) (xy 142.24 160.909) (xy 84.709 158.242)
      )
    )
  )
)
