(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "MounT_K85_Feather")
    (date "2022-10-23")
    (rev "005")
    (company "Brian K. White - b.kenyon.w@gmail.com")
    (comment 2 "github.com/bkw777/MounT")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (grid_origin 147.32 96.52)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_${TITLE}_${REVISION}")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/En")
  (net 3 "+3V3")
  (net 4 "/DTR_TTL")
  (net 5 "/DSR_TTL")
  (net 6 "/TX_TTL")
  (net 7 "/RX_TTL")
  (net 8 "/DTR_232")
  (net 9 "/CTS_232")
  (net 10 "/RTS_232")
  (net 11 "/RX_232")
  (net 12 "/TX_232")
  (net 13 "unconnected-(J1-Pad1)")
  (net 14 "unconnected-(J1-Pad3)")
  (net 15 "unconnected-(J1-Pad5)")
  (net 16 "unconnected-(J1-Pad6)")
  (net 17 "unconnected-(J1-Pad7)")
  (net 18 "unconnected-(J1-Pad8)")
  (net 19 "unconnected-(J1-Pad9)")
  (net 20 "unconnected-(J1-Pad10)")
  (net 21 "unconnected-(J1-Pad11)")
  (net 22 "unconnected-(J1-Pad12)")
  (net 23 "unconnected-(J1-Pad13)")
  (net 24 "unconnected-(J1-Pad17)")
  (net 25 "unconnected-(J1-Pad18)")
  (net 26 "unconnected-(J1-Pad21)")
  (net 27 "unconnected-(J1-Pad22)")
  (net 28 "unconnected-(J1-Pad23)")
  (net 29 "unconnected-(J1-Pad24)")
  (net 30 "unconnected-(J1-Pad25)")
  (net 31 "unconnected-(J1-Pad26)")
  (net 32 "unconnected-(J1-Pad28)")
  (net 33 "/DSR_DCD_232")
  (net 34 "unconnected-(J2-Pad9)")
  (net 35 "unconnected-(J2-Pad10)")
  (net 36 "unconnected-(J2-Pad11)")
  (net 37 "unconnected-(J2-Pad12)")
  (net 38 "unconnected-(J2-Pad13)")
  (net 39 "unconnected-(J2-Pad14)")
  (net 40 "unconnected-(J2-Pad15)")
  (net 41 "unconnected-(J2-Pad16)")
  (net 42 "unconnected-(J2-Pad17)")
  (net 43 "unconnected-(J2-Pad18)")
  (net 44 "unconnected-(J2-Pad19)")
  (net 45 "unconnected-(J2-Pad21)")
  (net 46 "/RI_232")
  (net 47 "unconnected-(J2-Pad23)")
  (net 48 "unconnected-(J2-Pad24)")
  (net 49 "unconnected-(J2-Pad25)")
  (net 50 "Net-(C2-Pad1)")
  (net 51 "Net-(C2-Pad2)")
  (net 52 "Net-(C3-Pad1)")
  (net 53 "Net-(C3-Pad2)")
  (net 54 "Net-(C4-Pad1)")
  (net 55 "Net-(C5-Pad1)")
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 151.13 88.519 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0.0254 0 270 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 147.32 88.519 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0.0254 0 270 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:Adafruit_Feather_stagger_6mil" (layer "F.Cu")
    (tedit 60436A52)
    (at 147.32 96.52 180)
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "J1" (at -5.842 0) (layer "F.SilkS") hide)
    (fp_text value "Adafruit_Feather" (at 0 -2) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 22.86 8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -22.86 -8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -22.86 8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 22.86 -8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at -19.05 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad1)") (pinfunction "~{RST}") (pintype "input+no_connect"))
    (pad "2" thru_hole circle locked (at -16.51 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 3 "+3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "3" thru_hole circle locked (at -13.97 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad3)") (pinfunction "ARef") (pintype "input+no_connect"))
    (pad "4" thru_hole circle locked (at -11.43 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at -8.89 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J1-Pad5)") (pinfunction "A0") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole circle locked (at -6.35 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J1-Pad6)") (pinfunction "A1") (pintype "bidirectional+no_connect"))
    (pad "7" thru_hole circle locked (at -3.81 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-Pad7)") (pinfunction "A2") (pintype "bidirectional+no_connect"))
    (pad "8" thru_hole circle locked (at -1.27 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J1-Pad8)") (pinfunction "A3") (pintype "bidirectional+no_connect"))
    (pad "9" thru_hole circle locked (at 1.27 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-Pad9)") (pinfunction "A4") (pintype "bidirectional+no_connect"))
    (pad "10" thru_hole circle locked (at 3.81 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J1-Pad10)") (pinfunction "A5") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole circle locked (at 6.35 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad11)") (pinfunction "SCK") (pintype "bidirectional+no_connect"))
    (pad "12" thru_hole circle locked (at 8.89 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad12)") (pinfunction "MOSI") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole circle locked (at 11.43 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad13)") (pinfunction "MISO") (pintype "bidirectional+no_connect"))
    (pad "14" thru_hole circle locked (at 13.97 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 "/RX_TTL") (pinfunction "RX/0") (pintype "bidirectional"))
    (pad "15" thru_hole circle locked (at 16.51 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 6 "/TX_TTL") (pinfunction "TX/1") (pintype "bidirectional"))
    (pad "16" thru_hole circle locked (at 19.05 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "17" thru_hole circle locked (at 19.05 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-Pad17)") (pinfunction "SDA/2") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole circle locked (at 16.51 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad18)") (pinfunction "SCL/3") (pintype "bidirectional+no_connect"))
    (pad "19" thru_hole circle locked (at 13.97 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 "/DTR_TTL") (pinfunction "~5") (pintype "bidirectional"))
    (pad "20" thru_hole circle locked (at 11.43 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 5 "/DSR_TTL") (pinfunction "6") (pintype "bidirectional"))
    (pad "21" thru_hole circle locked (at 8.89 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J1-Pad21)") (pinfunction "~9") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole circle locked (at 6.35 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J1-Pad22)") (pinfunction "~10") (pintype "bidirectional+no_connect"))
    (pad "23" thru_hole circle locked (at 3.81 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J1-Pad23)") (pinfunction "~11") (pintype "bidirectional+no_connect"))
    (pad "24" thru_hole circle locked (at 1.27 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J1-Pad24)") (pinfunction "12") (pintype "bidirectional+no_connect"))
    (pad "25" thru_hole circle locked (at -1.27 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J1-Pad25)") (pinfunction "13") (pintype "bidirectional+no_connect"))
    (pad "26" thru_hole circle locked (at -3.81 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 "unconnected-(J1-Pad26)") (pinfunction "USB") (pintype "power_in+no_connect"))
    (pad "27" thru_hole circle locked (at -6.35 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 "/En") (pinfunction "En") (pintype "input"))
    (pad "28" thru_hole circle locked (at -8.89 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J1-Pad28)") (pinfunction "BAT") (pintype "power_in+no_connect"))
  )
  (footprint "0_LOCAL:SOIC-16_W3.90mm" (layer "F.Cu")
    (tedit 6157DC02)
    (at 147.32 93.218 180)
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -0.762) (layer "F.SilkS") hide)
    (fp_text value "MAX3232" (at 0 0) (layer "F.SilkS"))
    (fp_text user "REF**" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.445 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(C2-Pad1)") (pinfunction "C1+") (pintype "passive"))
    (pad "2" smd roundrect locked (at -3.175 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(C4-Pad1)") (pinfunction "VS+") (pintype "power_out"))
    (pad "3" smd roundrect locked (at -1.905 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(C2-Pad2)") (pinfunction "C1-") (pintype "passive"))
    (pad "4" smd roundrect locked (at -0.635 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(C3-Pad1)") (pinfunction "C2+") (pintype "passive"))
    (pad "5" smd roundrect locked (at 0.635 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C3-Pad2)") (pinfunction "C2-") (pintype "passive"))
    (pad "6" smd roundrect locked (at 1.905 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(C5-Pad1)") (pinfunction "VS-") (pintype "power_out"))
    (pad "7" smd roundrect locked (at 3.175 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/DSR_DCD_232") (pinfunction "T2OUT") (pintype "output"))
    (pad "8" smd roundrect locked (at 4.445 2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/DTR_232") (pinfunction "R2IN") (pintype "input"))
    (pad "9" smd roundrect locked (at 4.445 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DSR_TTL") (pinfunction "R2OUT") (pintype "output"))
    (pad "10" smd roundrect locked (at 3.175 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DTR_TTL") (pinfunction "T2IN") (pintype "input"))
    (pad "11" smd roundrect locked (at 1.905 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/TX_TTL") (pinfunction "T1IN") (pintype "input"))
    (pad "12" smd roundrect locked (at 0.635 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/RX_TTL") (pinfunction "R1OUT") (pintype "output"))
    (pad "13" smd roundrect locked (at -0.635 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/TX_232") (pinfunction "R1IN") (pintype "input"))
    (pad "14" smd roundrect locked (at -1.905 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/RX_232") (pinfunction "T1OUT") (pintype "output"))
    (pad "15" smd roundrect locked (at -3.175 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" smd roundrect locked (at -4.445 -2.7 180) (size 0.6 1.27) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 143.51 88.519 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.0254 0 270 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 153.67 94.869 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -0.0508 0) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 153.67 91.186 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -0.0508 -0.0254) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:EG1215" (layer "F.Cu")
    (tedit 6053B3E1)
    (at 171.02 96.52 90)
    (property "Field4" "CUI Inc.")
    (property "Field5" "3.96 mm")
    (property "Field6" "Manufacturer Recommendations")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 0.684 270 unlocked) (layer "F.SilkS"))
    (fp_text value "CUS-12TB" (at -0.15 -4.55 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.5 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "1" smd roundrect (at -2.25 -1.75 90) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "/En") (pintype "passive"))
    (pad "2" smd roundrect (at 0.75 -1.75 90) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "Common") (pintype "passive"))
    (pad "3" smd roundrect (at 2.25 -1.75 90) (size 0.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pintype "passive"))
    (pad "S" smd roundrect (at 3.65 1.05 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "Shell") (pintype "passive"))
    (pad "S" smd roundrect (at -3.65 -1.05 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "Shell") (pintype "passive"))
    (pad "S" smd roundrect (at 3.65 -1.05 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "Shell") (pintype "passive"))
    (pad "S" smd roundrect (at -3.65 1.05 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "Shell") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/CUS-12TB.stp"
      (offset (xyz 0 0 1.37))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "0_LOCAL:PinHeader_1x02_P2.54mm_Horizontal" (layer "B.Cu")
    (tedit 6157B0B5)
    (at 127.508 91.694)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at 4.385 2.27) (layer "B.SilkS") hide)
    (fp_text value "Jumper_2_Bridged" (at 4.385 -4.81) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -1.27 -90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 "/CTS_232") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -2.54) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 "/RTS_232") (pinfunction "B") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/Jumper.stp"
      (offset (xyz 4.1 -3.77 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (footprint "0_LOCAL:DSUB-25_Male_Vertical_P2.77x2.84mm" (layer "B.Cu")
    (tedit 5F491F41)
    (at 163.94 97.79 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (property "Sheetfile" "File: MounT_K85_Feather.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.4605 -1.2827 180) (layer "B.SilkS") hide)
    (fp_text value "DB25_Male" (at 16.62 -8.73 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 16.62 -1.42 180) (layer "B.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 12 "/TX_232") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 11 "/RX_232") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 10 "/RTS_232") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 9 "/CTS_232") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 13.85 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 33 "/DSR_DCD_232") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 16.62 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 19.39 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 33 "/DSR_DCD_232") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 22.16 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J2-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle locked (at 24.93 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J2-Pad10)") (pinfunction "10") (pintype "passive+no_connect"))
    (pad "11" thru_hole circle locked (at 27.7 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J2-Pad11)") (pinfunction "11") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle locked (at 30.47 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J2-Pad12)") (pinfunction "12") (pintype "passive+no_connect"))
    (pad "13" thru_hole circle locked (at 33.24 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J2-Pad13)") (pinfunction "13") (pintype "passive+no_connect"))
    (pad "14" thru_hole circle locked (at 1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 39 "unconnected-(J2-Pad14)") (pinfunction "P14") (pintype "passive+no_connect"))
    (pad "15" thru_hole circle locked (at 4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 40 "unconnected-(J2-Pad15)") (pinfunction "P15") (pintype "passive+no_connect"))
    (pad "16" thru_hole circle locked (at 6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 41 "unconnected-(J2-Pad16)") (pinfunction "P16") (pintype "passive+no_connect"))
    (pad "17" thru_hole circle locked (at 9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J2-Pad17)") (pinfunction "P17") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle locked (at 12.465 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J2-Pad18)") (pinfunction "P18") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle locked (at 15.235 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J2-Pad19)") (pinfunction "P19") (pintype "passive+no_connect"))
    (pad "20" thru_hole circle locked (at 18.005 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 8 "/DTR_232") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle locked (at 20.775 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J2-Pad21)") (pinfunction "P21") (pintype "passive+no_connect"))
    (pad "22" thru_hole circle locked (at 23.545 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 46 "/RI_232") (pinfunction "P22") (pintype "passive+no_connect"))
    (pad "23" thru_hole circle locked (at 26.315 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J2-Pad23)") (pinfunction "P23") (pintype "passive+no_connect"))
    (pad "24" thru_hole circle locked (at 29.085 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J2-Pad24)") (pinfunction "P24") (pintype "passive+no_connect"))
    (pad "25" thru_hole circle locked (at 31.855 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 49 "unconnected-(J2-Pad25)") (pinfunction "P25") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_25_PP_Z_cut.step"
      (offset (xyz 16.625 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 124.46 107.95) (end 170.18 107.95) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 172.72 105.41) (end 172.72 87.63) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 170.18 85.09) (end 124.46 85.09) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 121.92 87.63) (end 121.92 105.41) (layer "Edge.Cuts") (width 0.0254))
  (gr_arc (start 170.18 85.09) (mid 171.976051 85.833949) (end 172.72 87.63) (layer "Edge.Cuts") (width 0.0254))
  (gr_arc (start 124.46 107.95) (mid 122.663949 107.206051) (end 121.92 105.41) (layer "Edge.Cuts") (width 0.0254))
  (gr_arc (start 121.92 87.63) (mid 122.663949 85.833949) (end 124.46 85.09) (layer "Edge.Cuts") (width 0.0254))
  (gr_arc (start 172.72 105.41) (mid 171.976051 107.206051) (end 170.18 107.95) (layer "Edge.Cuts") (width 0.0254))
  (gr_text "ON" (at 171.82 93.22 90) (layer "B.SilkS"))
  (gr_text "Feather MounT" (at 154.305 90.17) (layer "B.SilkS"))
  (gr_text "CTS" (at 125.095 91.694) (layer "B.SilkS"))
  (gr_text "OFF" (at 171.82 100.22 90) (layer "B.SilkS"))
  (gr_text "DB25M this side" (at 147.32 96.139) (layer "B.SilkS"))
  (gr_text "RTS" (at 125.095 89.789) (layer "B.SilkS"))
  (gr_text "${COMMENT2} ${TITLE} ${REVISION}" (at 147.32 104.775) (layer "B.SilkS"))
  (gr_text "Adafruit Feather to {dblquote}Model T{dblquote} RS-232" (at 154.305 92.075) (layer "B.SilkS"))
  (gr_text "ON" (at 171.82 92.32 90) (layer "F.SilkS"))
  (gr_text "Adafruit Feather\nthis side" (at 133.858 94.869) (layer "F.SilkS"))
  (gr_text "GND" (at 158.75 87.884 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 128.905 87.884 -90) (layer "F.SilkS"))
  (gr_text "DIP rows friction fit, solder or sockets optional" (at 151.765 104.775) (layer "F.SilkS"))
  (gr_text "RTS" (at 155.575 98.6282 -90) (layer "F.SilkS"))
  (gr_text "flush-cut & reflow db25 pins to protect lipo cell" (at 152.4 102.235) (layer "F.SilkS"))
  (gr_text "TX" (at 161.1122 98.6282 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 163.9062 98.6282 -90) (layer "F.SilkS"))
  (gr_text "DCD" (at 144.5006 98.6282 -90) (layer "F.SilkS"))
  (gr_text "RX" (at 158.3436 98.6282 -90) (layer "F.SilkS"))
  (gr_text "RX_TTL" (at 133.35 87.884 -90) (layer "F.SilkS"))
  (gr_text "DSR" (at 150.0378 98.6282 -90) (layer "F.SilkS"))
  (gr_text "OFF" (at 171.82 100.62 90) (layer "F.SilkS"))
  (gr_text "C1-C5: 0.1uf" (at 155.7274 92.075 -90) (layer "F.SilkS"))
  (gr_text "TX_TTL" (at 130.81 87.884 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 163.83 87.884 -90) (layer "F.SilkS"))
  (gr_text "RI" (at 140.335 99.7966 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 147.2692 98.6282 -90) (layer "F.SilkS"))
  (gr_text "DTR" (at 145.8976 99.7966 -90) (layer "F.SilkS"))
  (gr_text "DSR_TTL" (at 135.89 105.156 -90) (layer "F.SilkS"))
  (gr_text "DTR_TTL" (at 133.35 105.156 -90) (layer "F.SilkS"))
  (gr_text "CTS" (at 152.8064 98.6282 -90) (layer "F.SilkS"))
  (gr_text "Use ENIG finish so the friction-fit DIP row contacts are gold plated." (at 147.32 83.52) (layer "Dwgs.User"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 121.92 85.09)
        (xy 172.72 85.09)
        (xy 172.72 107.95)
        (xy 121.92 107.95)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 121.92 85.09)
        (xy 172.72 85.09)
        (xy 172.72 107.95)
        (xy 121.92 107.95)
      )
    )
  )
)
