<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3V</text>
<text>R</text>
<text>3</text>
<text>4</text>
<text>G</text>
<wire x1="12.550096875" y1="38.735" x2="1.419903125" y2="38.735" width="0.2032" layer="20"/>
<wire x1="1.419903125" y1="38.735" x2="0" y2="37.315096875" width="0.2032" layer="20" curve="90"/>
<wire x1="0" y1="37.315096875" x2="0" y2="1.419903125" width="0.2032" layer="20"/>
<wire x1="0" y1="1.419903125" x2="1.419903125" y2="0" width="0.2032" layer="20" curve="90"/>
<wire x1="1.419903125" y1="0" x2="12.550096875" y2="0" width="0.2032" layer="20"/>
<wire x1="12.550096875" y1="0" x2="13.97" y2="1.419903125" width="0.2032" layer="20" curve="90"/>
<wire x1="13.97" y1="1.419903125" x2="13.97" y2="37.315096875" width="0.2032" layer="20"/>
<wire x1="13.97" y1="37.315096875" x2="12.550096875" y2="38.735" width="0.2032" layer="20" curve="90"/>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="C603">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="SOIC127P798X216-8N">
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOT95P255X145-3N">
</package>
</packages>
</library>
<library name="lion">
<packages>
<package name="CONN_USB_MICRO-B">
<description>Modified to put part of the silkscreen that 
extends off the edge of the PCB to layer
49, reference.
USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CN1" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="SOIC127P798X216-8N" value="ATTINY85-20SU">
<attribute name="MPN" value="ATTINY85-20SU"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="58M3797"/>
<attribute name="OC_FARNELL" value="1455164"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="U2" library="Microchip_By_element14_Batch_1" package="SOT95P255X145-3N" value="MCP1702T-3302E/CB">
<attribute name="MPN" value="MCP1702T-3302E/CB"/>
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="OC_NEWARK" value="84R5179"/>
<attribute name="OC_FARNELL" value="1331490"/>
<attribute name="SUPPLIER" value="Microchip"/>
</element>
<element name="USB1" library="lion" package="CONN_USB_MICRO-B" value="CON-USB-F-MICRO-B"/>
<element name="C2" library="dp_devices" package="C603" value="10uF"/>
<element name="C4" library="dp_devices" package="C603" value="0.1uF"/>
<element name="C1" library="dp_devices" package="C603" value="10uF"/>
<element name="JP1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="USB1" pad="P5"/>
<contactref element="CN1" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="CN1" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="USB1" pad="P1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U1" pad="6"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PB2">
<contactref element="U1" pad="7"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PB3">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PB0">
<contactref element="U1" pad="5"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
