(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin -7.62 -256.54)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "1")
  (net 2 "2")
  (net 3 "3")
  (net 4 "4")
  (net 5 "5")
  (net 6 "14")
  (net 7 "15")
  (net 8 "16")
  (net 9 "17")
  (net 10 "a")
  (net 11 "c")
  (net 12 "13")
  (net 13 "12")
  (net 14 "11")
  (net 15 "10")
  (net 16 "9")
  (net 17 "8")
  (net 18 "7")
  (net 19 "6")
  (net 20 "18")
  (net 21 "19")
  (net 22 "20")
  (net 23 "21")
  (net 24 "22")
  (net 25 "23")
  (net 26 "24")
  (net 27 "25")
  (net 28 "b")
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 77.216 78.232 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rbias" (at -5.588 0.254) (layer "F.SilkS"))
    (fp_text value "R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 7.011 -18.949 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 28 "b"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "1"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:SOT-23-Handsolder" (layer "F.Cu")
    (tedit 619D1D91)
    (at 81.534 73.824 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (attr smd)
    (fp_text reference "Qr" (at 0 -2.794 -180) (layer "F.SilkS"))
    (fp_text value "Q_NJFET_GDS" (at -19.812 -45.593 -270) (layer "F.Fab"))
    (fp_text user "S" (at 1.868 -2.286 -180) (layer "F.SilkS"))
    (fp_text user "G" (at -2.069 -2.286 -180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 -0.95 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3"))
    (pad "2" smd rect locked (at -1.35 0.95 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "2"))
    (pad "3" smd rect locked (at 1.36 0 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "a"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 72.898 74.422 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "REF**" (at 3.302 9.906 90) (layer "F.SilkS") hide)
    (fp_text value "R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 4.953 10.033 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0.084 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "15"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "c"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 108.839 54.991 180)
    (attr through_hole)
    (fp_text reference "J5" (at 0 3.175) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 180) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (solder_mask_margin 1.27))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.534 80.0715 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "J1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R_1206_3216Metric" (at -32.766 -52.07 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 10 "a"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 11 "c"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 108.839 93.091)
    (attr through_hole)
    (fp_text reference "J4" (at 0 3.175) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (solder_mask_margin 1.27))
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 70.739 54.991 -90)
    (attr through_hole)
    (fp_text reference "J5" (at 0 3.175 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 270) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (solder_mask_margin 1.27))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB22C)
    (at 92.202 80.518 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Cc1" (at -0.127 2.413 180) (layer "F.SilkS"))
    (fp_text value "C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (at 9.652 12.446 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "b"))
    (pad "2" smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "c"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:mdm25_footprint" (layer "F.Cu")
    (tedit 0)
    (at 88.9 66.04 180)
    (descr "380-025-213L001-1")
    (tags "Connector")
    (attr through_hole)
    (fp_text reference "D1" (at 0.420856 2.383599) (layer "F.SilkS"))
    (fp_text value "MDM 25 Female" (at 0 -0.338) (layer "F.SilkS") hide)
    (fp_text user "13" (at -8.255 -2.54) (layer "F.SilkS"))
    (fp_text user "25" (at -8.89 2.54) (layer "F.SilkS"))
    (fp_text user "14" (at 8.255 2.54) (layer "F.SilkS"))
    (fp_text user "1" (at 8.255 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.338) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "1"))
    (pad "2" thru_hole circle (at 6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 2 "2"))
    (pad "3" thru_hole circle (at 5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 3 "3"))
    (pad "4" thru_hole circle (at 3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 4 "4"))
    (pad "5" thru_hole circle (at 2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 5 "5"))
    (pad "6" thru_hole circle (at 1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 19 "6"))
    (pad "7" thru_hole circle (at 0 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 18 "7"))
    (pad "8" thru_hole circle (at -1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 17 "8"))
    (pad "9" thru_hole circle (at -2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 16 "9"))
    (pad "10" thru_hole circle (at -3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 15 "10"))
    (pad "11" thru_hole circle (at -5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 14 "11"))
    (pad "12" thru_hole circle (at -6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 13 "12"))
    (pad "13" thru_hole circle (at -7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 12 "13"))
    (pad "14" thru_hole circle (at 6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 6 "14"))
    (pad "15" thru_hole circle (at 5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 7 "15"))
    (pad "16" thru_hole circle (at 4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 8 "16"))
    (pad "17" thru_hole circle (at 3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 9 "17"))
    (pad "18" thru_hole circle (at 1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 20 "18"))
    (pad "19" thru_hole circle (at 0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 21 "19"))
    (pad "20" thru_hole circle (at -0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 22 "20"))
    (pad "21" thru_hole circle (at -1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 23 "21"))
    (pad "22" thru_hole circle (at -3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 24 "22"))
    (pad "23" thru_hole circle (at -4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 25 "23"))
    (pad "24" thru_hole circle (at -5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 26 "24"))
    (pad "25" thru_hole circle (at -6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 27 "25"))
    (pad "MH1" thru_hole circle (at -12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (pad "MH2" thru_hole circle (at 12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (model "380-025-213L001.stp"
      (offset (xyz 7.62 0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.814 78.232 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfb" (at -5.588 0.211) (layer "F.SilkS"))
    (fp_text value "R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at -3.81 -9.949 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "c"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "15"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:SOT-23-Handsolder" (layer "F.Cu")
    (tedit 619D1D91)
    (at 93.152 76.12 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (attr smd)
    (fp_text reference "Q1" (at -0.254 -3.175 180) (layer "F.SilkS"))
    (fp_text value "Q_NJFET_GDS" (at -0.508 16.637 90) (layer "F.Fab"))
    (fp_text user "G" (at -1.985 -2.982 180) (layer "F.SilkS"))
    (fp_text user "D" (at -1.985 2.733 180) (layer "F.SilkS"))
    (fp_text user "S" (at 1.19 -2.982 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 -0.95 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "c"))
    (pad "2" smd rect locked (at -1.35 0.95 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "5"))
    (pad "3" smd rect locked (at 1.36 0 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "4"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 92.202 84.2275 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Detector" (at 0 4.318 180) (layer "F.SilkS"))
    (fp_text value "C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at -2.032 17.018 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "14"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "b"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 70.739 93.091)
    (attr through_hole)
    (fp_text reference "J5" (at 0 3.175) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (solder_mask_margin 1.27))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 77.216 82.042 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "REF**" (at -0.508 -13.716 90) (layer "F.SilkS") hide)
    (fp_text value "R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (at 1.778 -15.748 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "b"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "1"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 64.262 48.514) (end 115.189 99.441) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "D" (at 79.375 71.755) (layer "F.SilkS"))
  (gr_text "ZJS 2023-01-10 KURINSKY GROUP\n" (at 113.284 76.2 90) (layer "F.SilkS"))
  (gr_text "SPLENDOR SPLIT-STAGE AMP. BASE (V0.1)" (at 86.36 97.536) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.316 91.186)
        (xy 115.316 99.568)
        (xy 64.516 99.568)
        (xy 64.262 98.298)
        (xy 64.262 91.186)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.316 48.514)
        (xy 115.316 58.42)
        (xy 64.516 58.42)
        (xy 64.262 53.848)
        (xy 64.262 48.514)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.057 73.58)
        (xy 95.057 78.66)
        (xy 91.247 78.66)
        (xy 91.247 73.58)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.629 76.364)
        (xy 79.629 71.284)
        (xy 83.439 71.284)
        (xy 83.439 76.364)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.808 99.568)
        (xy 107.442 99.568)
        (xy 107.442 48.768)
        (xy 108.712 48.514)
        (xy 114.808 48.514)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.516 48.514)
        (xy 70.866 48.514)
        (xy 70.866 99.314)
        (xy 70.612 99.568)
        (xy 64.516 99.568)
      )
    )
  )
)
