(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 4)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 9)
    (tracks 13)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.9 8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BZ1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(IC1-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad6)")
  (net 6 "Net-(IC1-Pad3)")
  (net 7 "Net-(IC1-Pad7)")
  (net 8 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net VCC)
  )
  (module connectors:usb-PCB (layer F.Cu) (tedit 58C18398)
    (at 68.58 91.44 270)
    (attr virtual)
    (fp_text reference J2 (at 6.48 -7.85 270) (layer F.SilkS) hide)
    (fp_text value USB_A_PLUG (at 6.64 -10.13 270) (layer F.SilkS) hide)
    (pad 1 connect rect (at 10.16 -4.9 270) (size 1.9 8) (layers F.Cu F.Mask)
      (net 8 VCC))
    (pad 4 connect rect (at 2.54 -4.9 270) (size 1.9 8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 connect rect (at 5.05 -5.15 270) (size 2 7.5) (layers F.Cu F.Mask))
    (pad 2 connect rect (at 7.65 -5.15 270) (size 2 7.5) (layers F.Cu F.Mask))
  )
  (module Buzzers_Beepers:BUZZER (layer F.Cu) (tedit 0)
    (at 104.14 97.79 270)
    (fp_text reference BZ1 (at 0.24892 -1.75006 270) (layer F.SilkS))
    (fp_text value Buzzer (at 0 1.50114 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(BZ1-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 586281B4)
    (at 92.71 93.98 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference IC1 (at 3.81 -2.39 270) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 3.81 10.01 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BZ1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 68.58 91.694) (end 68.58 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.772 91.694) (end 68.58 91.694) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.772 90.678) (end 80.772 91.694) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.68 90.678) (end 80.772 90.678) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.68 104.902) (end 106.68 90.678) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.772 104.902) (end 106.68 104.902) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.772 103.886) (end 80.772 104.902) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 103.886) (end 80.772 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 91.694) (end 68.58 103.886) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 104.902) (xy 80.772 104.902) (xy 80.772 90.678) (xy 106.68 90.678)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.772 90.678) (xy 106.68 90.678) (xy 106.68 104.902) (xy 80.772 104.902)
      )
    )
  )
)
