(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (comment 1 "Rigid Board Specs")
    (comment 3 "Track Space - 5 mil, Track Width - 12 mil")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 68.22 101.26)
    (grid_origin 118.2 80.36)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VDD")
  (net 2 "Net-(J1-Pin_2)")
  (net 3 "Net-(J1-Pin_18)")
  (net 4 "Net-(J1-Pin_10)")
  (net 5 "Net-(J1-Pin_22)")
  (net 6 "Net-(J2-Pin_17)")
  (net 7 "Net-(J2-Pin_18)")
  (net 8 "/Twin1-")
  (net 9 "/Twin1+")
  (net 10 "/Twin2-")
  (net 11 "/Twin2+")
  (net 12 "/Twin3-")
  (net 13 "/Twin3+")
  (net 14 "GNDD")
  (net 15 "/Twin4-")
  (net 16 "/Twin4+")
  (net 17 "/Twin5-")
  (net 18 "/Twin5+")
  (net 19 "/Twin6-")
  (net 20 "/Twin6+")
  (net 21 "/Twin7-")
  (net 22 "/Twin7+")
  (net 23 "/Twin8-")
  (net 24 "/Twin8+")
  (net 25 "/Twin9-")
  (net 26 "Net-(J2-Pin_12)")
  (net 27 "/Twin9+")
  (net 28 "Net-(J2-Pin_22)")
  (net 29 "GNDA")
  (net 30 "VDDA")
  (footprint "MountingHole:Fuzz Button Mounting Pad" locked (layer "F.Cu")
    (at 120.74 37.815)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Mounting Hole" (at 1.85 -6.58) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at -0.28 8.09) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3.9 3.714) (size 4 4) (drill 2.9464) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:Fuzz Button Mounting Pad" locked (layer "F.Cu")
    (at 133.16 81.296)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Mounting Hole" (at 1.85 -6.58) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at -0.28 8.09) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -16.32 5.953) (size 4 4) (drill 2.9464) (layers "*.Cu" "*.Mask"))
  )
  (footprint "FuzzButtonFootprint:FuzzButtonPAD" (layer "B.Cu")
    (at 118.11 49.784 180)
    (property "Sheetfile" "Board1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x25, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at -3.302 6.858 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Pad_B" (at -4.445 4.064 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.31 unlocked) (layer "B.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd circle (at 0 -1.27 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd circle (at 0 -2.54 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/Twin6-") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd circle (at 0 -3.81 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/Twin6+") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd circle (at 0 -5.08 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd circle (at 0 -6.35 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/Twin7-") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd circle (at 0 -7.62 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/Twin7+") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd circle (at 0 -8.89 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd circle (at 0 -10.16 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/Twin8-") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd circle (at 0 -11.43 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/Twin8+") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd circle (at 0 -12.7 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd circle (at 0 -13.97 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "Net-(J2-Pin_12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd circle (at 0 -15.24 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd circle (at 0 -16.51 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/Twin9-") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd circle (at 0 -17.78 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/Twin9+") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd circle (at 0 -19.05 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd circle (at 0 -20.32 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "Net-(J2-Pin_17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd circle (at 0 -21.59 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "Net-(J2-Pin_18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd circle (at 0 -22.86 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd circle (at 0 -24.13 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDA") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd circle (at 0 -25.4 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDA") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd circle (at 0 -26.67 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "Net-(J2-Pin_22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd circle (at 0 -27.94 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDA") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd circle (at 0 -29.21 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDA") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd circle (at 0 -30.48 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDA") (pinfunction "Pin_25") (pintype "passive"))
  )
  (footprint "CONN_DD50S564TLF_AMP:CONN_DD50S564TLF_AMP" (layer "B.Cu")
    (at 70.866 44.289007 -90)
    (tags "DD50S564TLF ")
    (property "Sheetfile" "Board1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "DD50S564TLF")
    (attr through_hole)
    (fp_text reference "J3" (at 22.14 3.43 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "DD50S564TLF" (at 29.2 3.24 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "*" (at -2.540001 0 90 unlocked) (layer "B.SilkS") hide)
    (fp_text user "*" (at -2.540001 0 90) (layer "B.SilkS") hide)
    (fp_text user "*" (at -2.540001 0 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "*" (at -2.540001 0 90) (layer "B.Fab") hide)
    (pad "" np_thru_hole circle (at -8.475007 -2.539969 270) (size 3.0988 3.0988) (drill 3.0988) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 52.635005 -2.539969 270) (size 3.0988 3.0988) (drill 3.0988) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 2.76 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 19 "/Twin6-") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 5.519999 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 8.279999 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 21 "/Twin7-") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 11.039998 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 13.799998 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 23 "/Twin8-") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 16.559997 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 19.319997 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 25 "/Twin9-") (pinfunction "8") (pintype "unspecified"))
    (pad "9" thru_hole circle (at 22.079996 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "9") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 24.839996 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_17)") (pinfunction "10") (pintype "unspecified"))
    (pad "11" thru_hole circle (at 27.599996 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pin_18)") (pinfunction "11") (pintype "unspecified"))
    (pad "12" thru_hole circle (at 30.359995 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "12") (pintype "unspecified"))
    (pad "13" thru_hole circle (at 33.119995 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 29 "GNDA") (pinfunction "13") (pintype "unspecified"))
    (pad "14" thru_hole circle (at 35.879994 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(J2-Pin_22)") (pinfunction "14") (pintype "unspecified"))
    (pad "15" thru_hole circle (at 38.639994 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 30 "VDDA") (pinfunction "15") (pintype "unspecified"))
    (pad "16" thru_hole circle (at 41.399993 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 30 "VDDA") (pinfunction "16") (pintype "unspecified"))
    (pad "17" thru_hole circle (at 44.159993 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 30 "VDDA") (pinfunction "17") (pintype "unspecified"))
    (pad "18" thru_hole circle (at 1.38 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "18") (pintype "unspecified"))
    (pad "19" thru_hole circle (at 4.139999 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 20 "/Twin6+") (pinfunction "19") (pintype "unspecified"))
    (pad "20" thru_hole circle (at 6.899999 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "20") (pintype "unspecified"))
    (pad "21" thru_hole circle (at 9.659998 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 22 "/Twin7+") (pinfunction "21") (pintype "unspecified"))
    (pad "22" thru_hole circle (at 12.419998 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "22") (pintype "unspecified"))
    (pad "23" thru_hole circle (at 15.179998 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 24 "/Twin8+") (pinfunction "23") (pintype "unspecified"))
    (pad "24" thru_hole circle (at 17.939997 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J2-Pin_12)") (pinfunction "24") (pintype "unspecified"))
    (pad "25" thru_hole circle (at 20.699997 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 27 "/Twin9+") (pinfunction "25") (pintype "unspecified"))
    (pad "26" thru_hole circle (at 23.459996 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "26") (pintype "unspecified"))
    (pad "27" thru_hole circle (at 26.219996 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 12 "/Twin3-") (pinfunction "27") (pintype "unspecified"))
    (pad "28" thru_hole circle (at 28.979995 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "28") (pintype "unspecified"))
    (pad "29" thru_hole circle (at 31.739995 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 15 "/Twin4-") (pinfunction "29") (pintype "unspecified"))
    (pad "30" thru_hole circle (at 34.499994 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_18)") (pinfunction "30") (pintype "unspecified"))
    (pad "31" thru_hole circle (at 37.259994 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 29 "GNDA") (pinfunction "31") (pintype "unspecified"))
    (pad "32" thru_hole circle (at 40.019994 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 17 "/Twin5-") (pinfunction "32") (pintype "unspecified"))
    (pad "33" thru_hole circle (at 42.779993 -2.53997 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 30 "VDDA") (pinfunction "33") (pintype "unspecified"))
    (pad "34" thru_hole circle (at 0 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "34") (pintype "unspecified"))
    (pad "35" thru_hole circle (at 2.76 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 8 "/Twin1-") (pinfunction "35") (pintype "unspecified"))
    (pad "36" thru_hole circle (at 5.519999 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 9 "/Twin1+") (pinfunction "36") (pintype "unspecified"))
    (pad "37" thru_hole circle (at 8.279999 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "37") (pintype "unspecified"))
    (pad "38" thru_hole circle (at 11.039998 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "38") (pintype "unspecified"))
    (pad "39" thru_hole circle (at 13.799998 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 10 "/Twin2-") (pinfunction "39") (pintype "unspecified"))
    (pad "40" thru_hole circle (at 16.559997 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 11 "/Twin2+") (pinfunction "40") (pintype "unspecified"))
    (pad "41" thru_hole circle (at 19.319997 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "41") (pintype "unspecified"))
    (pad "42" thru_hole circle (at 22.079996 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "42") (pintype "unspecified"))
    (pad "43" thru_hole circle (at 24.839996 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_10)") (pinfunction "43") (pintype "unspecified"))
    (pad "44" thru_hole circle (at 27.599996 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 13 "/Twin3+") (pinfunction "44") (pintype "unspecified"))
    (pad "45" thru_hole circle (at 30.359995 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "45") (pintype "unspecified"))
    (pad "46" thru_hole circle (at 33.119995 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 16 "/Twin4+") (pinfunction "46") (pintype "unspecified"))
    (pad "47" thru_hole circle (at 35.879994 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 14 "GNDD") (pinfunction "47") (pintype "unspecified"))
    (pad "48" thru_hole circle (at 38.639994 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_22)") (pinfunction "48") (pintype "unspecified"))
    (pad "49" thru_hole circle (at 41.399993 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 18 "/Twin5+") (pinfunction "49") (pintype "unspecified"))
    (pad "50" thru_hole circle (at 44.159993 -5.079972 270) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 30 "VDDA") (pinfunction "50") (pintype "unspecified"))
  )
  (footprint "FuzzButtonFootprint:FuzzButtonPAD" (layer "B.Cu")
    (at 115.57 49.149 180)
    (property "Sheetfile" "Board1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x25, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J1" (at 3.556 5.461 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Pad_A" (at 3.81 4.191 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.31 unlocked) (layer "B.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd circle (at 0 -1.27 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd circle (at 0 -2.54 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd circle (at 0 -3.81 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/Twin1-") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd circle (at 0 -5.08 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/Twin1+") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd circle (at 0 -6.35 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd circle (at 0 -7.62 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/Twin2-") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd circle (at 0 -8.89 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/Twin2+") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd circle (at 0 -10.16 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd circle (at 0 -11.43 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd circle (at 0 -12.7 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd circle (at 0 -13.97 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "/Twin3-") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd circle (at 0 -15.24 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/Twin3+") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd circle (at 0 -16.51 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd circle (at 0 -17.78 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/Twin4-") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd circle (at 0 -19.05 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/Twin4+") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd circle (at 0 -20.32 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd circle (at 0 -21.59 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(J1-Pin_18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd circle (at 0 -22.86 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "GNDD") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd circle (at 0 -24.13 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDA") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd circle (at 0 -25.4 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "/Twin5-") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd circle (at 0 -26.67 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(J1-Pin_22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd circle (at 0 -27.94 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "/Twin5+") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd circle (at 0 -29.21 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDA") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd circle (at 0 -30.48 180) (size 0.75 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "VDDA") (pinfunction "Pin_25") (pintype "passive"))
  )
  (gr_line (start 125.27 90.52) (end 78.195 90.52)
    (layer "Edge.Cuts"))
  (gr_line (start 125.3 38) (end 125.27 90.52)
    (layer "Edge.Cuts"))
  (gr_line (start 125.3 38) (end 78.21 37.97)
    (layer "Edge.Cuts"))
  (gr_line (start 78.195 90.52) (end 78.195 100.045)
    (layer "Edge.Cuts"))
  (gr_line (start 78.21 32.51) (end 78.21 37.97)
    (layer "Edge.Cuts"))
  (gr_line (start 68.43 32.51) (end 68.46 100.04)
    (layer "Edge.Cuts"))
  (gr_line (start 78.21 32.51) (end 68.43 32.51)
    (layer "Edge.Cuts"))
  (gr_line (start 78.195 100.045) (end 68.46 100.04)
    (layer "Edge.Cuts"))
  (zone (net 29) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 14) (net_name "GNDD") (layer "In1.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 29) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (priority 9)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 29) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 29) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 29) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 53.26 31.26)
        (xy 125.26 31.26)
        (xy 125.26 101.26)
        (xy 53.26 101.26)
      )
    )
  )
  (zone (net 14) (net_name "GNDD") (layer "In2.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 125.26 101.26)
        (xy 53.26 101.26)
        (xy 53.26 31.26)
      )
    )
  )
  (zone (net 14) (net_name "GNDD") (layer "In2.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
  (zone (net 14) (net_name "GNDD") (layer "In2.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 125.26 101.26)
        (xy 53.26 101.26)
        (xy 53.26 31.26)
      )
    )
  )
  (zone (net 14) (net_name "GNDD") (layer "In2.Cu") (hatch edge 0.5)
    (priority 8)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.26 31.26)
        (xy 53.26 31.26)
        (xy 53.26 101.26)
        (xy 125.26 101.26)
      )
    )
  )
)
