(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 138.924999 80.924999 148.575001 92.575001)
    (thickness 1.6)
    (drawings 5)
    (tracks 68)
    (zones 0)
    (modules 38)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.11)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 0.8001)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 86.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 82.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 145.6 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.85 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 84.6)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 85.35)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 83.85)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 141.85 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 142.6 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 144.1 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module TO_SOT_Packages_SMD:SOT-669_LFPAK (layer F.Cu) (tedit 590BA898)
    (at 143.75 85.25 90)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT-669 Power-SO8")
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference "" (at -0.27 -3.48 90) (layer F.SilkS))
    (fp_text value "" (at -0.27 3.52 90) (layer F.Fab))
    (fp_text user %R (at -0.04 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.16 -1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.69 -1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.01 -1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0.16 1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.69 1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.01 1.15 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.01 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.69 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 2.86 -1.88) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 2.86 1.88) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 2.86 -0.6) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.86 -0.64) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.86 -1.91) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 3 smd rect (at -2.86 0.64) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.61 0) (size 4.7 1.55) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.41 0) (size 4.2 3.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at -2.86 1.91) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.86 0.6) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0.16 0 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz -0.01 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Pads:SolderWirePad_3x_0-8mmDrill (layer F.Cu) (tedit 590BAA2B)
    (at 143.75 91)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.175 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 3.175 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 590BA919)
    (at 143.35 83.1)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (gr_line (start 148.5 92.5) (end 139 92.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.5 81) (end 148.5 92.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 81) (end 148.5 81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 92.5) (end 139 81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "lfpak\n" (at 143.6 87.9) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 148.5 92.5) (xy 139 92.5) (xy 139 81) (xy 148.5 81)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.11))
    (min_thickness 0.11)
    (fill yes (arc_segments 16) (thermal_gap 0.11) (thermal_bridge_width 0.123))
    (polygon
      (pts
        (xy 148.5 92.5) (xy 139 92.5) (xy 139 81) (xy 148.5 81)
      )
    )
  )
)
