(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 94)
    (no_connects 0)
    (area 25.900001 36.3 158.1 110.9242)
    (thickness 1.6)
    (drawings 28)
    (tracks 407)
    (zones 0)
    (modules 37)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /ETH_NETPWR)
  (net 4 /ETH_TX+)
  (net 5 /ETH_TX-)
  (net 6 /ETH_RX+)
  (net 7 /ETH_RX-)
  (net 8 /ETH_L1)
  (net 9 /Omega_RX)
  (net 10 /Omega_TX)
  (net 11 /ETH_PWR+)
  (net 12 /ETH_PWR-)
  (net 13 +24V)
  (net 14 /SBB_DATA2+)
  (net 15 /SBB_DATA2-)
  (net 16 /SBB_DATA1+)
  (net 17 /SBB_DATA1-)
  (net 18 /SBB_DATA3+)
  (net 19 /SBB_DATA3-)
  (net 20 /RS485_TXEN0)
  (net 21 /RS485_TXEN2)
  (net 22 /UART_RX2)
  (net 23 /UART_TX2)
  (net 24 /UART_RX1)
  (net 25 /UART_TX1)
  (net 26 /RS485_TXEN1)
  (net 27 /RS485_RXEN0)
  (net 28 "Net-(C1-Pad1)")
  (net 29 "Net-(C2-Pad1)")
  (net 30 "Net-(J1-Pad9)")
  (net 31 "Net-(J1-Pad11)")
  (net 32 /ETH_L2)
  (net 33 /G18)
  (net 34 /G19)
  (net 35 /I2C_SCL)
  (net 36 /I2C_SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ETH_L1)
    (add_net /ETH_L2)
    (add_net /ETH_NETPWR)
    (add_net /ETH_RX+)
    (add_net /ETH_RX-)
    (add_net /ETH_TX+)
    (add_net /ETH_TX-)
    (add_net /G18)
    (add_net /G19)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /RS485_RXEN0)
    (add_net /RS485_TXEN0)
    (add_net /RS485_TXEN1)
    (add_net /RS485_TXEN2)
    (add_net /SBB_DATA1+)
    (add_net /SBB_DATA1-)
    (add_net /SBB_DATA2+)
    (add_net /SBB_DATA2-)
    (add_net /SBB_DATA3+)
    (add_net /SBB_DATA3-)
    (add_net /UART_RX1)
    (add_net /UART_RX2)
    (add_net /UART_TX1)
    (add_net /UART_TX2)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 1.2)
    (uvia_drill 0.6)
    (add_net +24V)
    (add_net +3V3)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net GND)
  )
  (module plan44:plan44-HLJ-6115ANL (layer F.Cu) (tedit 581B6BD3)
    (at 70.5 67)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J1 (at -1.27 -4.318 180) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.90754 2.9591 180) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 4 /ETH_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 5 /ETH_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 /ETH_NETPWR))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 /ETH_NETPWR))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 /ETH_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 30 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 /ETH_L1))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 32 /ETH_L2))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module plan44:plan44-STELVIO-4P-508 (layer F.Cu) (tedit 58C31135)
    (at 103.75 98 180)
    (attr virtual)
    (fp_text reference J3 (at -4.5 0 270) (layer F.SilkS))
    (fp_text value SBB (at 7.62 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /SBB_DATA1+))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 17 /SBB_DATA1-))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 18 /SBB_DATA3+))
    (pad 4 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 19 /SBB_DATA3-))
  )
  (module plan44:plan44-ONION-2MM-2X16 (layer F.Cu) (tedit 581313E0)
    (at 105.5 74 90)
    (descr "FOOTPRINT FÜR ONION OMEGA")
    (tags "FOOTPRINT FÜR ONION OMEGA")
    (attr virtual)
    (fp_text reference U1 (at 0 -19.812 90) (layer F.SilkS))
    (fp_text value ONION-OMEGA2 (at 0.20828 18.96364 90) (layer F.SilkS))
    (pad B1 thru_hole rect (at 12.39774 -13.99794 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad B2 thru_hole circle (at 12.39774 -11.99896 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +3V3))
    (pad B3 thru_hole circle (at 12.39774 -9.99998 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B4 thru_hole circle (at 12.39774 -7.99846 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B5 thru_hole circle (at 12.39774 -5.99948 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /Omega_RX))
    (pad B6 thru_hole circle (at 12.39774 -3.99796 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /Omega_TX))
    (pad B7 thru_hole circle (at 12.39774 -1.99898 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B8 thru_hole circle (at 12.39774 0 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 3 /ETH_NETPWR))
    (pad B9 thru_hole circle (at 12.39774 1.99898 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 5 /ETH_TX-))
    (pad B10 thru_hole circle (at 12.39774 3.99796 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 4 /ETH_TX+))
    (pad B11 thru_hole circle (at 12.39774 5.99948 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 /ETH_RX-))
    (pad B12 thru_hole circle (at 12.39774 7.99846 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_RX+))
    (pad B13 thru_hole circle (at 12.39774 9.99998 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 33 /G18))
    (pad B14 thru_hole circle (at 12.39774 11.99896 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 34 /G19))
    (pad B15 thru_hole circle (at 12.39774 13.99794 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 35 /I2C_SCL))
    (pad B16 thru_hole circle (at 12.39774 15.99946 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 36 /I2C_SDA))
    (pad A1 thru_hole rect (at -11.99896 -13.99794 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad A2 thru_hole circle (at -11.99896 -11.99896 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 20 /RS485_TXEN0))
    (pad A3 thru_hole circle (at -11.99896 -9.99998 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /RS485_RXEN0))
    (pad A4 thru_hole circle (at -11.99896 -7.99846 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 21 /RS485_TXEN2))
    (pad A5 thru_hole circle (at -11.99896 -5.99948 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 22 /UART_RX2))
    (pad A6 thru_hole circle (at -11.99896 -3.99796 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 23 /UART_TX2))
    (pad A7 thru_hole circle (at -11.99896 -1.99898 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A8 thru_hole circle (at -11.99896 0 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 /UART_RX1))
    (pad A9 thru_hole circle (at -11.99896 1.99898 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /UART_TX1))
    (pad A10 thru_hole circle (at -11.99896 3.99796 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A11 thru_hole circle (at -11.99896 5.99948 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A12 thru_hole circle (at -11.99896 7.99846 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A13 thru_hole circle (at -11.99896 9.99998 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 /ETH_L1))
    (pad A14 thru_hole circle (at -11.99896 11.99896 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 32 /ETH_L2))
    (pad A15 thru_hole circle (at -11.99896 13.99794 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 26 /RS485_TXEN1))
    (pad A16 thru_hole circle (at -11.99896 15.99946 90) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
  )
  (module plan44:plan44-STELVIO-4P-508 (layer F.Cu) (tedit 58C3112D)
    (at 77 98 180)
    (attr virtual)
    (fp_text reference J2 (at 19.5 -0.75 450) (layer F.SilkS))
    (fp_text value SBB (at 7.62 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 13 +24V))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 14 /SBB_DATA2+))
    (pad 4 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 15 /SBB_DATA2-))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 90.25 92 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ADM3485E (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 /SBB_DATA1-))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 /SBB_DATA1+))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 /UART_TX1))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 /RS485_TXEN1))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 /UART_RX1))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 57FE2A1A)
    (at 55 69.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 57FE2A14)
    (at 120 69.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 58C2E12E)
    (at 55 94.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 58C2E100)
    (at 120 94.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 80.25 92 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ADM3485E (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 /SBB_DATA2-))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 /SBB_DATA2+))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 /UART_TX2))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 /RS485_TXEN2))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 /UART_RX2))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 100.5 92 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value ADM3485E (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 /SBB_DATA3-))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 /SBB_DATA3+))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 /Omega_TX))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 /RS485_TXEN0))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 /RS485_RXEN0))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 /Omega_RX))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E14F)
    (at 73.5 84.75 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E117)
    (at 69 84.75 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E110)
    (at 85.25 62.25 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E15B)
    (at 116.5 102)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.5 0) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E0CF)
    (at 50 98.25 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +24V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E10A)
    (at 49.75 101.75)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C8 (at 2.5 0) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 58C2E142)
    (at 62 81 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C9 (at 4.5 -3.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C2E155)
    (at 113.5 102 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C10 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:plan44-Recom-R78Cxx (layer F.Cu) (tedit 581323FC)
    (at 55.5 82.75 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U2 (at -0.4 5.6 270) (layer F.SilkS))
    (fp_text value Recom_R78Cxx (at 2.4 -3.2 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 +24V))
    (pad 3 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C30AB2)
    (at 78 82.25 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /ETH_NETPWR))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 58C3115C)
    (at 62 92 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C7 (at -2 3.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +24V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C31114)
    (at 73.75 93.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58C31118)
    (at 82.75 102.25 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C12 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58C31143)
    (at 125.25 101.75 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at 2.75 3 270) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.09 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 58C3110A)
    (at 53.5 74.75)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P2 (at -2.5 2.75 90) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.93) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 +24V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ETH_PWR-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C311A0)
    (at 74.5 80.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /ETH_TX+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C31199)
    (at 72.25 80.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /ETH_TX-))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C31192)
    (at 70 80.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /ETH_RX+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C31189)
    (at 67.75 80.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /ETH_RX-))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C312E1)
    (at 55 62 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.25 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad9)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C312D7)
    (at 55 64.75 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.25 0 450) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad11)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 97.75 68.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 /RS485_TXEN1))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 97.75 80 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /RS485_TXEN2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 93.5 68.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /RS485_RXEN0))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 93.5 80 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /RS485_TXEN0))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 111.25 91.5)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P3 (at 1.27 -2.39) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /I2C_SCL))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /G19))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /I2C_SDA))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /G18))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "splitflapcontroller v1\n© 2017 plan44.ch" (at 49.75 68.5 90) (layer F.SilkS))
  (gr_line (start 127.5 60) (end 47.5 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.5 104.5) (end 127.5 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47.5 104.5) (end 127.5 104.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47.5 60) (end 47.5 104.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 94 (width 0.3) (layer Dwgs.User)
    (gr_text "94.000 mm" (at 87.5 37.65) (layer Dwgs.User))
    (feature1 (pts (xy 134.5 67.5) (xy 134.5 36.3)))
    (feature2 (pts (xy 40.5 67.5) (xy 40.5 36.3)))
    (crossbar (pts (xy 40.5 39) (xy 134.5 39)))
    (arrow1a (pts (xy 134.5 39) (xy 133.373496 39.586421)))
    (arrow1b (pts (xy 134.5 39) (xy 133.373496 38.413579)))
    (arrow2a (pts (xy 40.5 39) (xy 41.626504 39.586421)))
    (arrow2b (pts (xy 40.5 39) (xy 41.626504 38.413579)))
  )
  (dimension 44.5 (width 0.3) (layer Dwgs.User)
    (gr_text "44.500 mm" (at 32.4 82.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 47.5 104.5) (xy 31.05 104.5)))
    (feature2 (pts (xy 47.5 60) (xy 31.05 60)))
    (crossbar (pts (xy 33.75 60) (xy 33.75 104.5)))
    (arrow1a (pts (xy 33.75 104.5) (xy 33.163579 103.373496)))
    (arrow1b (pts (xy 33.75 104.5) (xy 34.336421 103.373496)))
    (arrow2a (pts (xy 33.75 60) (xy 33.163579 61.126504)))
    (arrow2b (pts (xy 33.75 60) (xy 34.336421 61.126504)))
  )
  (dimension 80 (width 0.3) (layer Dwgs.User)
    (gr_text "80.000 mm" (at 87.5 44.15) (layer Dwgs.User))
    (feature1 (pts (xy 127.5 60) (xy 127.5 42.8)))
    (feature2 (pts (xy 47.5 60) (xy 47.5 42.8)))
    (crossbar (pts (xy 47.5 45.5) (xy 127.5 45.5)))
    (arrow1a (pts (xy 127.5 45.5) (xy 126.373496 46.086421)))
    (arrow1b (pts (xy 127.5 45.5) (xy 126.373496 44.913579)))
    (arrow2a (pts (xy 47.5 45.5) (xy 48.626504 46.086421)))
    (arrow2b (pts (xy 47.5 45.5) (xy 48.626504 44.913579)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 87.5 49.65) (layer Dwgs.User))
    (feature1 (pts (xy 55 69.75) (xy 55 48.3)))
    (feature2 (pts (xy 120 69.75) (xy 120 48.3)))
    (crossbar (pts (xy 120 51) (xy 55 51)))
    (arrow1a (pts (xy 55 51) (xy 56.126504 50.413579)))
    (arrow1b (pts (xy 55 51) (xy 56.126504 51.586421)))
    (arrow2a (pts (xy 120 51) (xy 118.873496 50.413579)))
    (arrow2b (pts (xy 120 51) (xy 118.873496 51.586421)))
  )
  (dimension 25 (width 0.3) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 151.6 82.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 120 94.75) (xy 152.95 94.75)))
    (feature2 (pts (xy 120 69.75) (xy 152.95 69.75)))
    (crossbar (pts (xy 150.25 69.75) (xy 150.25 94.75)))
    (arrow1a (pts (xy 150.25 94.75) (xy 149.663579 93.623496)))
    (arrow1b (pts (xy 150.25 94.75) (xy 150.836421 93.623496)))
    (arrow2a (pts (xy 150.25 69.75) (xy 149.663579 70.876504)))
    (arrow2b (pts (xy 150.25 69.75) (xy 150.836421 70.876504)))
  )
  (zone (net 1) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 104) (xy 48 104) (xy 48 60.5) (xy 127 60.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48 60.5) (xy 127 60.5) (xy 127 104) (xy 48 104)
      )
    )
  )
)
