(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+24V")
  (net 2 "24VCOM")
  (net 3 "NORLMT In")
  (net 4 "NORLMT Out")
  (net 5 "REVLMT In")
  (net 6 "REVLMT Out")
  (net 7 "Net-(R1-Pad1)")
  (net 8 "Net-(R2-Pad1)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 127 88.646)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 10.16 0) (layer "F.SilkS"))
    (fp_text value "7.78k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 101.6 76.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-4_W7.62mm" (layer "F.Cu")
    (at 127 102.87)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 10.15 0.005) (layer "F.SilkS"))
    (fp_text value "CPC1301G" (at 3.81 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(R2-Pad1)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "REVLMT In") (pintype "input"))
    (pad "3" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "REVLMT Out") (pintype "input"))
    (pad "4" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+24V") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 101.6 119.38)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 190.5 76.2)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 127 99.06)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 10.16 0) (layer "F.SilkS"))
    (fp_text value "7.78k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 190.5 119.38)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-4_W7.62mm" (layer "F.Cu")
    (at 127 92.451)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 10.15 0.005) (layer "F.SilkS"))
    (fp_text value "CPC1301G" (at 3.81 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(R1-Pad1)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "NORLMT In") (pintype "input"))
    (pad "3" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "NORLMT Out") (pintype "input"))
    (pad "4" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+24V") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:PHOENIX_1990041" (layer "F.Cu")
    (at 99.52 88.69 -90)
    (property "MANUFACTURER" "PHOENIX")
    (property "Sheetfile" "NORLMT REVLMT inverter board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.06 -11.478 -180) (layer "F.SilkS"))
    (fp_text value "1990041" (at 9.525 1.115 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 2.75 -9.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+24V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 5.25 -4.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "24VCOM") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.75 -9.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "NORLMT In") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 10.25 -4.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "NORLMT Out") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 12.75 -9.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "REVLMT In") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 15.25 -4.7 270) (size 1.508 1.508) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "REVLMT Out") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.102))
    (model ":STIERS_3DMODEL_DIR:1990041.step"
      (offset (xyz 8.25 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_arc (start 195.58 119.38) (mid 194.092102 122.972102) (end 190.5 124.46)
    (layer "Edge.Cuts"))
  (gr_line (start 101.6 124.46) (end 190.5 124.46)
    (layer "Edge.Cuts"))
  (gr_arc (start 96.52 76.2) (mid 98.007898 72.607898) (end 101.6 71.12)
    (layer "Edge.Cuts"))
  (gr_line (start 190.5 71.12) (end 101.6 71.12)
    (layer "Edge.Cuts"))
  (gr_line (start 96.52 76.2) (end 96.52 119.38)
    (layer "Edge.Cuts"))
  (gr_arc (start 190.5 71.12) (mid 194.092102 72.607898) (end 195.58 76.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.6 124.46) (mid 98.007898 122.972102) (end 96.52 119.38)
    (layer "Edge.Cuts"))
  (gr_line (start 195.58 119.38) (end 195.58 76.2)
    (layer "Edge.Cuts"))
  (gr_text "+24V" (at 112.268 91.44) (layer "F.SilkS"))
  (gr_text "NORLMT REVLMT inverter board, v1\n10 June 2024, E. Stiers" (at 190.5 97.79 -90) (layer "F.SilkS"))
  (gr_text "REVLMT In" (at 112.268 101.346) (layer "F.SilkS"))
  (gr_text "NORLMT Out" (at 112.268 99.06) (layer "F.SilkS"))
  (gr_text "REVLMT Out" (at 112.268 103.886) (layer "F.SilkS"))
  (gr_text "NORLMT In" (at 112.268 96.52) (layer "F.SilkS"))
  (gr_text "+24V COM" (at 112.268 93.98) (layer "F.SilkS"))
  (zone (net 2) (net_name "24VCOM") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 91.44 66.04)
        (xy 91.44 127)
        (xy 198.12 127)
        (xy 198.12 66.04)
      )
    )
  )
)
