(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 117)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 4)
    (tracks 424)
    (zones 0)
    (modules 43)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.25)
    (user_via 1 0.5)
    (user_via 2 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.8006 4.8006)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 B3)
  (net 2 B2)
  (net 3 B1)
  (net 4 GND)
  (net 5 B4)
  (net 6 VIN)
  (net 7 VCC)
  (net 8 "Net-(CON1-Pad3)")
  (net 9 BD1)
  (net 10 BVL1)
  (net 11 BD2)
  (net 12 BVL2)
  (net 13 BD3)
  (net 14 BVL3)
  (net 15 BD4)
  (net 16 BVL4)
  (net 17 SW1)
  (net 18 CPL0)
  (net 19 CPL1)
  (net 20 CPL2)
  (net 21 "Net-(U1-Pad13)")
  (net 22 "Net-(U1-Pad18)")
  (net 23 "Net-(U1-Pad19)")
  (net 24 "Net-(U1-Pad20)")
  (net 25 "Net-(C5-Pad2)")
  (net 26 "Net-(CON1-Pad1)")
  (net 27 REF)
  (net 28 SDA)
  (net 29 SCL)
  (net 30 "Net-(R10-Pad1)")
  (net 31 "Net-(U1-Pad3)")
  (net 32 BVL)
  (net 33 VDD)
  (net 34 SW2)
  (net 35 SW3)
  (net 36 SW4)
  (net 37 SW5)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net BD1)
    (add_net BD2)
    (add_net BD3)
    (add_net BD4)
    (add_net BVL)
    (add_net BVL1)
    (add_net BVL2)
    (add_net BVL3)
    (add_net BVL4)
    (add_net CPL0)
    (add_net CPL1)
    (add_net CPL2)
    (add_net GND)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad3)")
    (add_net REF)
    (add_net SCL)
    (add_net SDA)
    (add_net SW1)
    (add_net SW2)
    (add_net SW3)
    (add_net SW4)
    (add_net SW5)
    (add_net VCC)
    (add_net VDD)
    (add_net VIN)
  )
  (module 18650:BK-18650-PC8 (layer B.Cu) (tedit 588FA0CD)
    (at 150.368 92.456 180)
    (fp_text reference B1 (at -0.889 -35.052 180) (layer B.SilkS))
    (fp_text value 4x18650 (at 0 41 180) (layer B.Fab))
    (pad 6 thru_hole circle (at -36.45 -9.7 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 1 B3))
    (pad 4 thru_hole circle (at -36.45 9.7 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 2 B2))
    (pad 2 thru_hole circle (at -36.45 29 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 3 B1))
    (pad 1 thru_hole circle (at 36.45 29 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 3 thru_hole circle (at 36.45 9.7 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 5 thru_hole circle (at 36.45 -9.7 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 7 thru_hole circle (at 36.45 -29 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 8 thru_hole circle (at -36.45 -29 180) (size 3 3) (drill 1.6) (layers *.Cu *.Mask B.SilkS)
      (net 5 B4))
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L16_P5 (layer F.Cu) (tedit 0)
    (at 143.764 59.563)
    (descr "Radial Electrolytic Capacitor 10mm x Length 16mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.3) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L16_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L16_P5 (layer F.Cu) (tedit 0)
    (at 161.798 59.563 180)
    (descr "Radial Electrolytic Capacitor 10mm x Length 16mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 2.5 -6.3 180) (layer F.SilkS))
    (fp_text value CP1 (at 2.5 6.3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 VIN))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L16_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 541A9C03)
    (at 151.384 46.863 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 2.3 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VIN))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 541A9C03)
    (at 143.764 46.863 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 2.3 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 541A9C03)
    (at 118.364 46.863 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 2.3 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 110.617 55.118 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 SW1))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 110.744 63.627 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 SW2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 110.49 72.136 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 SW3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 110.49 80.772 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 SW4))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 130.81 56.769)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 110.49 89.408 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 SW5))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:JACK_ALIM (layer B.Cu) (tedit 588F88D9)
    (at 185.293 44.704 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "CONN JACK")
    (fp_text reference CON1 (at 0.254 5.588 180) (layer B.SilkS))
    (fp_text value BARREL_JACK (at -5.08 -5.588 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 0 180) (size 4.8006 4.8006) (drill 3) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 1 thru_hole rect (at 6.096 0 180) (size 4.8006 4.8006) (drill 3) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(CON1-Pad1)"))
    (pad 3 thru_hole circle (at 2.286 -5.08 180) (size 4.8006 4.8006) (drill 3) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(CON1-Pad3)"))
    (model Connect.3dshapes/JACK_ALIM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA-SMB_Universal_Handsoldering (layer B.Cu) (tedit 552FF496)
    (at 167.894 38.608)
    (descr "Diode, Universal, SMA, SMB, Handsoldering,")
    (tags "Diode Universal SMA SMB Handsoldering ")
    (attr smd)
    (fp_text reference D1 (at 0 3.81) (layer B.SilkS))
    (fp_text value D (at 0 -3.81) (layer B.Fab))
    (fp_text user K (at -3.3 -1.7) (layer B.SilkS))
    (fp_text user A (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 1 smd trapezoid (at -2.90068 0) (size 3.60172 1.69926) (rect_delta 0.59944 0 ) (layers B.Cu B.Paste B.Mask)
      (net 6 VIN))
    (pad 2 smd trapezoid (at 2.90068 0 180) (size 3.60172 1.69926) (rect_delta 0.59944 0 ) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(CON1-Pad1)"))
    (model Diodes_SMD.3dshapes/SMA-SMB_Universal_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_TO-92:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 169.037 47.244 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference D2 (at 0 -4 90) (layer F.SilkS))
    (fp_text value LM385 (at 0 3 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 REF))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 1 thru_hole oval (at 0 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 98.679 49.276)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 SCL))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 122.936 79.502 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 BD1))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 BVL1))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 122.936 94.234 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 11 BD2))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 BVL2))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 122.809 108.966 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 BD3))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 BVL3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 122.809 123.825 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 BD4))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 BVL4))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 119.38 76.2 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 BD1))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm (layer F.Cu) (tedit 53FEE67B)
    (at 157.48 79.502 180)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R2 (at 0 -8.89 180) (layer F.SilkS))
    (fp_text value 1R8 (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 B1))
    (pad 2 thru_hole circle (at 30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 BVL1))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 119.507 90.932 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 BD2))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm (layer F.Cu) (tedit 53FEE67B)
    (at 157.48 94.234 180)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R4 (at 0 -8.89 180) (layer F.SilkS))
    (fp_text value 1R8 (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 B2))
    (pad 2 thru_hole circle (at 30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 BVL2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 119.38 105.664 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 BD3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm (layer F.Cu) (tedit 53FEE67B)
    (at 157.48 108.966 180)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R6 (at 0 -8.89 180) (layer F.SilkS))
    (fp_text value 1R8 (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 B3))
    (pad 2 thru_hole circle (at 30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 BVL3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 119.38 120.396 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 BD4))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm (layer F.Cu) (tedit 588FA0CE)
    (at 157.48 123.825 180)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference R8 (at -2.413 -2.54 180) (layer F.SilkS))
    (fp_text value 1R8 (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 B4))
    (pad 2 thru_hole circle (at 30.48 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 BVL4))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L50mm-W14mm-H13mm-p60mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 164.592 47.879 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 47K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 REF))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 133.096 60.071)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 47K (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 588FA0BB)
    (at 98.171 55.118 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 0.381 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 SW1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 588FA0BF)
    (at 98.171 63.627 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -0.254 0.508 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 SW2))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 588FA0C2)
    (at 98.298 72.39 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0 0.762 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 SW3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 588FA0C5)
    (at 98.298 80.772 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -0.127 0.762 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 SW4))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 588FA0C8)
    (at 98.298 89.408 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 0 0.762 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 SW5))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 104.394 55.753 180)
    (fp_text reference SW1 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 SW1))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 SW1))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 104.394 64.135 180)
    (fp_text reference SW2 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 SW2))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 SW2))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 104.394 72.644 180)
    (fp_text reference SW3 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 SW3))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 SW3))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 104.394 81.28 180)
    (fp_text reference SW4 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 SW4))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 SW4))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 104.394 89.916 180)
    (fp_text reference SW5 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 SW5))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 SW5))
  )
  (module Sockets_DIP:DIP-32__600 (layer F.Cu) (tedit 588F9AFF)
    (at 134.874 43.942)
    (descr "32 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U1 (at -13.97 -3.81) (layer F.SilkS))
    (fp_text value CH340_NANO (at 8.89 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 CPL2))
    (pad 2 thru_hole circle (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C5-Pad2)"))
    (pad 3 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 B4))
    (pad 5 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 B3))
    (pad 6 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 B2))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 B1))
    (pad 8 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 9 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 SCL))
    (pad 10 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 BVL))
    (pad 11 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 REF))
    (pad 12 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (pad 13 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 15 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 VIN))
    (pad 18 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 22 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 SW5))
    (pad 23 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 SW4))
    (pad 24 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 SW3))
    (pad 25 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 SW2))
    (pad 26 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 SW1))
    (pad 27 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 BD4))
    (pad 28 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 BD3))
    (pad 29 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 BD2))
    (pad 30 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 BD1))
    (pad 31 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 CPL0))
    (pad 32 thru_hole circle (at -19.05 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 CPL1))
    (model Sockets_DIP.3dshapes/DIP-32__600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 133.223 66.421 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6 270) (layer F.SilkS))
    (fp_text value 4051 (at 0 6 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 BVL))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R10-Pad1)"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 CPL2))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 CPL1))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 CPL0))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 BVL1))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 BVL2))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 BVL3))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 BVL4))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 VDD))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 98.679 46.228)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 SCL))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_line (start 96.901 131.953) (end 189.357 131.953) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.901 35.179) (end 96.901 131.953) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.357 35.179) (end 96.901 35.179) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.357 131.953) (end 189.357 35.179) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.155 35.433) (xy 189.103 35.56) (xy 189.103 131.699) (xy 97.282 131.699) (xy 97.155 35.433)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.155 35.433) (xy 189.103 35.56) (xy 189.103 131.699) (xy 97.282 131.699) (xy 97.155 35.433)
      )
    )
  )
)
