<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="53.34" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="53.34" y1="2.54" x2="53.34" y2="9.525" width="0" layer="20"/>
<wire x1="53.34" y1="9.525" x2="50.8" y2="12.065" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="12.065" x2="2.54" y2="12.065" width="0" layer="20"/>
<wire x1="2.54" y1="12.065" x2="0" y2="9.525" width="0" layer="20" curve="90"/>
<wire x1="0" y1="9.525" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>SHORT
ENABLE</text>
<text>ADJUST
0.8-4.5V</text>
<text>+</text>
<text>+</text>
<text>5V</text>
<text>MCP1824-ADJ</text>
<text>2017 E. Petersen</text>
<text>USB</text>
<text>300mA</text>
</plain>
<libraries>
<library name="C3-Murata">
<packages>
<package name="21-0805">
<description>&lt;b&gt;Murata *21 Size 0805 Land Pattern&lt;/b&gt;&lt;p&gt;
&lt;a href="http://www.murata.com/products/catalog/pdf/c02e.pdf"&gt;Murata Chip Capacitor Catalog, p130, table 2&lt;/a&gt;</description>
</package>
<package name="31-1206">
<description>&lt;b&gt;Murata *31 Size 1206 Land Pattern&lt;/b&gt;&lt;p&gt;
&lt;a href="http://www.murata.com/products/catalog/pdf/c02e.pdf"&gt;Murata Chip Capacitor Catalog, p154, table 2&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="C3-Comchip">
<description>&lt;b&gt;Comchip Products&lt;/b&gt;</description>
<packages>
<package name="DO-214AA">
<description>&lt;b&gt;DO-214AA&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="C3-Littelfuse">
<packages>
<package name="1206">
<description>&lt;b&gt;1206 SMD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="C3-Connector">
<description>&lt;b&gt;Multi-contact Connectors&lt;/b&gt;
&lt;p&gt;Select the number of contacts and then chose the connector type. f you don't see a package for the type of connector you want, add a new package.
&lt;p&gt;Choose either &lt;i&gt;MXX&lt;/i&gt; for male pin type connectors or &lt;i&gt;FXX&lt;/i&gt; for female socket type connectors.
&lt;p&gt;To select a specific part number for your bill of materials set the VALUE of the component.
&lt;p&gt;For an arbitrary number of individual floating pins/sockets choose the &lt;i&gt;M&lt;/i&gt; or &lt;i&gt;F&lt;/i&gt; connectors devices. You can add up to 100 individual contacts per device. Use INVOKE to add more later.</description>
<packages>
<package name="1X02">
</package>
<package name="USB-MICROB">
<description>&lt;b&gt;Amphenol 10118194 USB 2.0 Micro B Connector&lt;/b&gt;
&lt;p&gt;&lt;a href="http://portal.fciconnect.com/Comergent//fci/drawing/10118194.pdf"&gt;Datasheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="C3-General">
<description>Erik's Custom Parts</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
<package name="TP5000K-040">
<description>&lt;b&gt;Keystone 5000 Series THM Mini Testpoints 0.040 dia. Hole Size&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="C3-Panasonic">
<packages>
<package name="R0603">
<description>0603 (1608) Chip Resistor Package (Panasonic)&lt;p&gt;
&lt;a href="http://industrial.panasonic.com/www-data/pdf/AOA0000/AOA0000PE32.pdf"&gt;Datasheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="C3-Microchip">
<packages>
<package name="SOT95P270X145-5N">
<description>&lt;b&gt;SOT3-5&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="C3-Vishay">
<packages>
<package name="T93YA">
<description>T93YA comp 3296W</description>
</package>
</packages>
</library>
<library name="C3-LED">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="C3-Murata" package="21-0805" value="1uF, 50V, 0R">
<attribute name="CAP" value="1.0E-6"/>
<attribute name="ESR" value="0.0"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="MANUFACTURER_NAME" value="MuRata"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM21BR71H105KA12L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="MuRata"/>
</element>
<element name="C9" library="C3-Murata" package="31-1206" value="4.7uF, 50V, 0R">
<attribute name="CAP" value="4.7E-6"/>
<attribute name="ESR" value="0.0"/>
<attribute name="IRMS" value="0.0"/>
<attribute name="MANUFACTURER_NAME" value="MuRata"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM31CR71H475KA12L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VDC" value="50.0"/>
<attribute name="VENDOR" value="MuRata"/>
</element>
<element name="D1" library="C3-Comchip" package="DO-214AA" value="CZRB5338B-HF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VZ" value="5.1"/>
<attribute name="ZMAX" value="1.5"/>
</element>
<element name="F1" library="C3-Littelfuse" package="1206" value="1.8A">
<attribute name="I-HOLD" value="1A"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="1.8A"/>
</element>
<element name="J1" library="C3-Connector" package="1X02" value="M02PTH">
<attribute name="VALUE"/>
</element>
<element name="J2" library="C3-Connector" package="1X02" value="M02PTH">
<attribute name="VALUE"/>
</element>
<element name="J3" library="C3-Connector" package="1X02" value="M02PTH">
<attribute name="VALUE"/>
</element>
<element name="J4" library="C3-Connector" package="USB-MICROB" value="10118194-0001LF">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="C3-General" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="R5" library="C3-Vishay" package="T93YA" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="C3-Panasonic" package="R0603" value="100K 5%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="C3-Panasonic" package="R0603" value="10K 5%">
<attribute name="NAME"/>
<attribute name="VALUE" value="10K 5%"/>
</element>
<element name="R8" library="C3-Panasonic" package="R0603" value="100K 5%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="C3-Microchip" package="SOT95P270X145-5N" value="MCP1824T-ADJE/OT">
<attribute name="MPN" value="MCP1824T-ADJE/OT"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1578393"/>
<attribute name="OC_NEWARK" value="40M0692"/>
<attribute name="PACKAGE" value="SOT-5"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="VALUE"/>
</element>
<element name="VADJ" library="C3-General" package="TP5000K-040" value="TP-5000K-040">
<attribute name="COLOR" value="RED"/>
<attribute name="NAME"/>
</element>
<element name="TP1" library="C3-General" package="TP5000K-040" value="TP-5001K-040">
<attribute name="COLOR" value="BLACK"/>
<attribute name="NAME"/>
</element>
<element name="LED1" library="C3-LED" package="CHIPLED_0603" value="LCQ971-KN-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="C3-LED" package="CHIPLED_0603" value="LCQ971-KN-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="C3-Panasonic" package="R0603" value="270R 5%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="C3-Panasonic" package="R0603" value="270R 5%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C9" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R8" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="7"/>
<contactref element="J4" pad="8"/>
<contactref element="J4" pad="9"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="TP1" pad="PP"/>
</signal>
<signal name="SHDN">
<contactref element="U4" pad="3"/>
<contactref element="R8" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="ADJ2">
<contactref element="R7" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="ADJ">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="U4" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VUSB">
<contactref element="J4" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="R6" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="C10" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="VADJ" pad="PP"/>
</signal>
<signal name="LED2">
<contactref element="R3" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="LED1">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
