(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~61~ubuntu18.04.1)
  (general
    (links 61)
    (no_connects 0)
    (area 115.674999 82.424999 177.325001 106.425001)
    (thickness 1.6)
    (drawings 23)
    (tracks 254)
    (zones 0)
    (modules 30)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 /Sync)
  (net 6 /Blue)
  (net 7 /Green)
  (net 8 /Red)
  (net 9 /Blue_raw)
  (net 10 /Green_raw)
  (net 11 /Red_raw)
  (net 12 "Net-(C4-Pad1)")
  (net 13 /Video_raw)
  (net 14 "Net-(C6-Pad1)")
  (net 15 GNDA)
  (net 16 "Net-(C7-Pad1)")
  (net 17 "Net-(C10-Pad1)")
  (net 18 "Net-(C11-Pad1)")
  (net 19 /AudioLeftAmp)
  (net 20 /AudioRightAmp)
  (net 21 +5V)
  (net 22 "Net-(C8-Pad1)")
  (net 23 "Net-(C9-Pad1)")
  (net 24 "Net-(R11-Pad2)")
  (net 25 "Net-(R10-Pad1)")
  (net 26 /AudioRight)
  (net 27 /AudioLeft)
  (net 28 /Video)
  (net 29 "Net-(R2-Pad2)")
  (net 30 "Net-(C12-Pad1)")
  (net 31 "Net-(C13-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /AudioLeft)
    (add_net /AudioLeftAmp)
    (add_net /AudioRight)
    (add_net /AudioRightAmp)
    (add_net /Blue)
    (add_net /Blue_raw)
    (add_net /Green)
    (add_net /Green_raw)
    (add_net /Red)
    (add_net /Red_raw)
    (add_net /Sync)
    (add_net /Video)
    (add_net /Video_raw)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B9198B0)
    (at 156.05 93.4 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 2.425 1.3 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GNDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 5B92CFE1)
    (at 164.825 95.35 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -3.85 -3.325 360) (layer F.SilkS))
    (fp_text value THS7374 (at 0 3.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -1.95 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.95 -1.3 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.95 -0.65 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -2.95 0 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -2.95 0.65 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (pad 6 smd rect (at -2.95 1.3 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (pad 7 smd rect (at -2.95 1.95 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.95 1.95 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.95 1.3 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 10 smd rect (at 2.95 0.65 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 11 smd rect (at 2.95 0 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 /Video))
    (pad 12 smd rect (at 2.95 -0.65 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 /Blue))
    (pad 13 smd rect (at 2.95 -1.3 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /Green))
    (pad 14 smd rect (at 2.95 -1.95 180) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /Red))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pcengine-expansion:PCEngineExpansion (layer F.Cu) (tedit 5B93C949)
    (at 146.5 86.5)
    (fp_text reference U1 (at 26.7 4.6) (layer F.SilkS))
    (fp_text value PCEngineExpansion (at 0 -8) (layer F.Fab))
    (pad A1 thru_hole circle (at -27.9 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /AudioLeft))
    (pad A2 thru_hole circle (at -25.36 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad A3 thru_hole circle (at -22.82 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A4 thru_hole circle (at -20.28 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A5 thru_hole circle (at -17.74 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A6 thru_hole circle (at -15.2 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A7 thru_hole circle (at -12.66 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A8 thru_hole circle (at -10.12 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A9 thru_hole circle (at -7.58 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A10 thru_hole circle (at -5.04 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A11 thru_hole circle (at -2.5 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A12 thru_hole circle (at 0.04 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A13 thru_hole circle (at 2.58 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A14 thru_hole circle (at 5.12 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A15 thru_hole circle (at 7.66 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A16 thru_hole circle (at 10.2 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A17 thru_hole circle (at 12.74 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A18 thru_hole circle (at 15.28 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A19 thru_hole circle (at 17.82 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A20 thru_hole circle (at 20.36 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad A21 thru_hole circle (at 22.9 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GNDA))
    (pad A22 thru_hole circle (at 25.44 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /Video_raw))
    (pad A23 thru_hole circle (at 27.98 -2.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /Red_raw))
    (pad B1 thru_hole circle (at -27.9 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B2 thru_hole circle (at -25.36 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B3 thru_hole circle (at -22.82 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B4 thru_hole circle (at -20.28 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B5 thru_hole circle (at -17.74 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B6 thru_hole circle (at -15.2 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B7 thru_hole circle (at -12.66 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B8 thru_hole circle (at -10.12 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B9 thru_hole circle (at -7.58 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B10 thru_hole circle (at -5.04 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B11 thru_hole circle (at -2.5 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B12 thru_hole circle (at 0.04 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B13 thru_hole circle (at 2.58 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B14 thru_hole circle (at 5.12 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B15 thru_hole circle (at 7.66 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B16 thru_hole circle (at 10.2 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B17 thru_hole circle (at 12.74 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B18 thru_hole circle (at 15.28 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B19 thru_hole circle (at 17.82 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B20 thru_hole circle (at 20.36 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B21 thru_hole circle (at 22.9 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B22 thru_hole circle (at 25.44 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad B23 thru_hole circle (at 27.98 0.14) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /Green_raw))
    (pad C1 thru_hole circle (at -27.9 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /AudioRight))
    (pad C2 thru_hole circle (at -25.36 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 GNDA))
    (pad C3 thru_hole circle (at -22.82 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C4 thru_hole circle (at -20.28 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C5 thru_hole circle (at -17.74 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C6 thru_hole circle (at -15.2 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C7 thru_hole circle (at -12.66 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C8 thru_hole circle (at -10.12 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C9 thru_hole circle (at -7.58 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C10 thru_hole circle (at -5.04 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C11 thru_hole circle (at -2.5 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C12 thru_hole circle (at 0.04 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C13 thru_hole circle (at 2.58 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C14 thru_hole circle (at 5.12 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C15 thru_hole circle (at 7.66 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C16 thru_hole circle (at 10.2 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C17 thru_hole circle (at 12.74 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C18 thru_hole circle (at 15.28 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C19 thru_hole circle (at 17.82 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C20 thru_hole circle (at 20.36 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad C21 thru_hole circle (at 22.9 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad C22 thru_hole circle (at 25.44 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(R2-Pad2)"))
    (pad C23 thru_hole circle (at 27.98 2.68) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /Blue_raw))
    (model /home/martin/Documents/SSQ-123-02-T-T-RA.wrl
      (at (xyz 0.001 0.155 0.15))
      (scale (xyz 0.394 0.394 0.394))
      (rotate (xyz 180 0 180))
    )
  )
  (module mini-din:MINI-DIN-9PIN (layer F.Cu) (tedit 5B92D60C)
    (at 153.7 97.075 180)
    (fp_text reference U3 (at -7.35 -3.75 270) (layer F.SilkS))
    (fp_text value Mini-DIN-9-Pin (at 0 -10.1 180) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /Sync))
    (pad 8 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /AudioLeftAmp))
    (pad 4 thru_hole circle (at -2 0 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 /Video))
    (pad 9 thru_hole circle (at 4 0 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /AudioRightAmp))
    (pad 7 thru_hole circle (at -4 0 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /Red))
    (pad 2 thru_hole circle (at 0.7 -2.5 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad 1 thru_hole circle (at -1.3 -2.5 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /Blue))
    (pad 3 thru_hole circle (at -4 -2.5 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /Green))
    (pad 6 thru_hole circle (at 4 -2.5 180) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at 0 -6.3 180) (size 2.8 2.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 15 GNDA))
    (model /home/martin/Downloads/MD-90S.wrl
      (at (xyz 0 0.43 0.25))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 270 0 -90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B918334)
    (at 172.2 98.7)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.05 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Red_raw))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B918330)
    (at 172.2 96.7)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.05 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Green_raw))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B918341)
    (at 172.2 94.7)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.025 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /Blue_raw))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B91904D)
    (at 151.675 93.875)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.15 -0.025) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B91834B)
    (at 172.2 92.7)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.025 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /Video_raw))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B943B5F)
    (at 133.7 93.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.85 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B917C41)
    (at 125.9 93.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -2.8 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B943AFB)
    (at 136.925 102.85 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -2.825 0.025 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5BB3A487)
    (at 117.275 103.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -4 -2.6 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917E1F)
    (at 131.5 93.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.9 0.375 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917E0B)
    (at 135.9 93.2 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.525 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917C8F)
    (at 123.7 93.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.875 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917C8A)
    (at 128.1 93.2 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.9 0.05 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917D7C)
    (at 132.925 97.45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.925 0 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917C73)
    (at 126.6 97.45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -2.85 0 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B917D71)
    (at 134.825 102.95 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 2.925 0 180) (layer F.SilkS))
    (fp_text value 2K7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BB3A859)
    (at 119.4 103.525 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 2.825 1.05 180) (layer F.SilkS))
    (fp_text value 2K7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B943AF1)
    (at 132.7 102.95 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.95 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BB3A84F)
    (at 121.525 103.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 1.45 1.425 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5B91840C)
    (at 127.15 102.05 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -3.25 180) (layer F.SilkS))
    (fp_text value TS922A (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R11-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C9-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C13-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5BB13653)
    (at 164.85 99.15)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.975 0.9) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5BB3A3B4)
    (at 120.875 97.45 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C8 (at -2 0.95 180) (layer F.SilkS))
    (fp_text value 10nF/Poly (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /AudioLeft))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5BB3A3AD)
    (at 117.6 97.45 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 7.075 -0.975 180) (layer F.SilkS))
    (fp_text value 10nF/Poly (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /AudioRight))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.3 (layer F.Cu) (tedit 5B940EB7)
    (at 142.3 96.075)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C12 (at -3.325 -2.1 90) (layer F.SilkS))
    (fp_text value 10uF/Poly (at 0 -3.92) (layer F.Fab))
    (fp_text user + (at -1.37 -0.08) (layer F.Fab))
    (fp_text user + (at -3.38 2.34) (layer F.SilkS))
    (fp_text user %R (at 0 3.92) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /AudioLeftAmp))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.3 (layer F.Cu) (tedit 5B940EAD)
    (at 142.3 102.675)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C13 (at -3.325 -2.075 90) (layer F.SilkS))
    (fp_text value 10uF/Poly (at 0 -3.92) (layer F.Fab))
    (fp_text user + (at -1.37 -0.08) (layer F.Fab))
    (fp_text user + (at -3.38 2.34) (layer F.SilkS))
    (fp_text user %R (at 0 3.92) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /AudioRightAmp))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B92D051)
    (at 165.675 91.275)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.1 0) (layer F.SilkS))
    (fp_text value 75R/Zero (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /Sync))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 177.25 99.85) (end 177.25 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.25 101.85) (end 177.25 106.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.25 99.85) (end 177.25 99.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.25 101.85) (end 174.25 99.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.25 101.85) (end 174.25 101.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.75 106.35) (end 115.75 100.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.75 99.05) (end 115.75 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.75 100.55) (end 115.75 100.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.75 99.05) (end 118.75 100.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.75 99.05) (end 118.75 99.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Attention!\nSCART Cable should contain 75 Ohm\nand 220uF capacitors on video lines!" (at 133.875 99.95) (layer B.SilkS))
  (gr_text "2018, Martin Hejnfelt\n(martin@hejnfelt.com)" (at 168.375 103.9) (layer B.SilkS))
  (gr_text "PCEngine\nRGB Add-on" (at 168.75 103.3) (layer F.SilkS))
  (gr_text "JP OFF=BYPASS\nJP ON=FILTER" (at 150.225 91.825) (layer F.SilkS))
  (gr_line (start 117.5 82.5) (end 175.5 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.25 106.35) (end 115.75 106.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.5 82.5) (end 115.75 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 82.5) (end 177.25 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 15) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.15 106.25) (xy 115.85 106.25) (xy 115.85 100.65) (xy 118.875 100.65) (xy 118.875 98.95)
        (xy 115.85 98.95) (xy 115.85 82.6) (xy 177.15 82.6) (xy 177.15 99.725) (xy 174.1 99.725)
        (xy 174.1 101.95) (xy 177.15 101.95)
      )
    )
  )
  (zone (net 15) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.15 106.25) (xy 115.85 106.25) (xy 115.85 100.65) (xy 118.875 100.65) (xy 118.875 98.95)
        (xy 115.85 98.95) (xy 115.85 82.6) (xy 177.15 82.6) (xy 177.15 99.725) (xy 174.1 99.725)
        (xy 174.1 101.95) (xy 177.15 101.95)
      )
    )
  )
)
