(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 254)
    (no_connects 0)
    (area 44.504 30.828 319.124001 202.833)
    (thickness 1.6)
    (drawings 280)
    (tracks 7997)
    (zones 0)
    (modules 21)
    (nets 56)
  )
  (page A3)
  (title_block
    (title "TOFE to apertus AXIOM Adapter")
    (company "TimVideos.us HDMI2USB Project")
    (comment 1 http://tofe.io)
    (comment 2 "License : CC BY-SA")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.381)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 0.6096 0.254)
    (uvia_size 0.2032)
    (uvia_drill 0.1524)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.65024 0.65024)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 166.624 169.418)
    (grid_origin 166.624 169.418)
    (visible_elements 7FFFCE79)
    (pcbplotparams
      (layerselection 0x01020_80000007)
      (usegerberextensions true)
      (gerberprecision 5)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 /PRSTN)
  (net 2 /RESET)
  (net 3 /VCC12V)
  (net 4 /VCC3V3)
  (net 5 GND)
  (net 6 /SMCLK)
  (net 7 /SMDAT)
  (net 8 /S_IO5)
  (net 9 /N_IO4)
  (net 10 /S_IO7)
  (net 11 /S_IO6)
  (net 12 /N_IO7)
  (net 13 /N_IO6)
  (net 14 /S_IO0)
  (net 15 /N_IO0)
  (net 16 /S_IO4)
  (net 17 /S_IO3)
  (net 18 /S_IO2)
  (net 19 /S_IO1)
  (net 20 /S_SDA)
  (net 21 /S_SCL)
  (net 22 /N_IO3)
  (net 23 /N_IO2)
  (net 24 /N_IO1)
  (net 25 /N_SDA)
  (net 26 /N_SCL)
  (net 27 /N_IO5)
  (net 28 "Net-(CN1-Pad2)")
  (net 29 "Net-(TOFE1-PadA33)")
  (net 30 /N_LVDS_3_P)
  (net 31 /N_LVDS_3_N)
  (net 32 /N_LVDS_4_P)
  (net 33 /N_LVDS_4_N)
  (net 34 /N_LVDS_5_N)
  (net 35 /N_LVDS_5_P)
  (net 36 /N_LVDS_2_N)
  (net 37 /N_LVDS_1_P)
  (net 38 /N_LVDS_0_N)
  (net 39 /N_LVDS_0_P)
  (net 40 /N_LVDS_1_N)
  (net 41 /N_LVDS_2_P)
  (net 42 /S_LVDS_0_P)
  (net 43 /S_LVDS_0_N)
  (net 44 /S_LVDS_1_P)
  (net 45 /S_LVDS_1_N)
  (net 46 /S_LVDS_2_P)
  (net 47 /S_LVDS_2_N)
  (net 48 /S_LVDS_3_P)
  (net 49 /S_LVDS_3_N)
  (net 50 /S_LVDS_4_P)
  (net 51 /S_LVDS_4_N)
  (net 52 /S_LVDS_5_P)
  (net 53 /S_LVDS_5_N)
  (net 54 "Net-(CS1-Pad2)")
  (net 55 /VCC5V0)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.2032)
    (uvia_drill 0.1524)
    (add_net /N_SCL)
    (add_net /N_SDA)
    (add_net /PRSTN)
    (add_net /RESET)
    (add_net /SMCLK)
    (add_net /SMDAT)
    (add_net /S_SCL)
    (add_net /S_SDA)
    (add_net /VCC5V0)
    (add_net "Net-(CN1-Pad2)")
    (add_net "Net-(CS1-Pad2)")
    (add_net "Net-(TOFE1-PadA33)")
  )
  (net_class IO_NORTH_LM0.254 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.2032)
    (uvia_drill 0.1524)
    (add_net /N_IO0)
    (add_net /N_IO1)
    (add_net /N_IO2)
    (add_net /N_IO3)
    (add_net /N_IO4)
    (add_net /N_IO5)
    (add_net /N_IO6)
    (add_net /N_IO7)
  )
  (net_class IO_SOUTH_LM0.254 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.2032)
    (uvia_drill 0.1524)
    (add_net /S_IO0)
    (add_net /S_IO1)
    (add_net /S_IO2)
    (add_net /S_IO3)
    (add_net /S_IO4)
    (add_net /S_IO5)
    (add_net /S_IO6)
    (add_net /S_IO7)
  )
  (net_class LVDS_DP0.0635/0.254 ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.2032)
    (uvia_drill 0.1524)
    (add_net /N_LVDS_0_N)
    (add_net /N_LVDS_0_P)
    (add_net /N_LVDS_1_N)
    (add_net /N_LVDS_1_P)
    (add_net /N_LVDS_2_N)
    (add_net /N_LVDS_2_P)
    (add_net /N_LVDS_3_N)
    (add_net /N_LVDS_3_P)
    (add_net /N_LVDS_4_N)
    (add_net /N_LVDS_4_P)
    (add_net /N_LVDS_5_N)
    (add_net /N_LVDS_5_P)
    (add_net /S_LVDS_0_N)
    (add_net /S_LVDS_0_P)
    (add_net /S_LVDS_1_N)
    (add_net /S_LVDS_1_P)
    (add_net /S_LVDS_2_N)
    (add_net /S_LVDS_2_P)
    (add_net /S_LVDS_3_N)
    (add_net /S_LVDS_3_P)
    (add_net /S_LVDS_4_N)
    (add_net /S_LVDS_4_P)
    (add_net /S_LVDS_5_N)
    (add_net /S_LVDS_5_P)
  )
  (net_class PWR ""
    (clearance 0.1524)
    (trace_width 0.4572)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.2032)
    (uvia_drill 0.1524)
    (add_net /VCC12V)
    (add_net /VCC3V3)
    (add_net GND)
  )
  (module w_conn_pc:pci-x_conn-x1 (layer B.Cu) (tedit 57027946)
    (at 217.52454 166.95)
    (descr "PCI-X 1x card edge connector, FCI P/N 10018783-10x00x")
    (fp_text reference SOUTH1 (at 0 5.99948) (layer B.SilkS))
    (fp_text value AXIOM-PCIE (at -0.10054 -6.168) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.14884 0) (size 2.4003 2.4003) (drill 2.4003) (layers *.Cu B.SilkS))
    (pad "" np_thru_hole circle (at 11.30046 0) (size 2.4003 2.4003) (drill 2.4003) (layers *.Cu B.SilkS))
    (pad A12 thru_hole circle (at 3.50012 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A13 thru_hole circle (at 4.50088 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 48 /S_LVDS_3_P))
    (pad A14 thru_hole circle (at 5.4991 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 49 /S_LVDS_3_N))
    (pad A15 thru_hole circle (at 6.49986 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A16 thru_hole circle (at 7.50062 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 50 /S_LVDS_4_P))
    (pad A17 thru_hole circle (at 8.49884 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 51 /S_LVDS_4_N))
    (pad A18 thru_hole circle (at 9.4996 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B13 thru_hole circle (at 4.50088 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B15 thru_hole circle (at 6.49986 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B17 thru_hole circle (at 8.49884 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 53 /S_LVDS_5_N))
    (pad B12 thru_hole circle (at 3.50012 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 55 /VCC5V0))
    (pad B14 thru_hole circle (at 5.4991 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B16 thru_hole circle (at 7.50062 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 52 /S_LVDS_5_P))
    (pad B18 thru_hole circle (at 9.4996 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A11 thru_hole circle (at 0.50038 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 54 "Net-(CS1-Pad2)"))
    (pad A9 thru_hole circle (at -1.50114 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 47 /S_LVDS_2_N))
    (pad A7 thru_hole circle (at -3.50012 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A5 thru_hole circle (at -5.4991 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 44 /S_LVDS_1_P))
    (pad A3 thru_hole circle (at -7.50062 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 43 /S_LVDS_0_N))
    (pad A1 thru_hole circle (at -9.4996 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A2 thru_hole circle (at -8.49884 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 42 /S_LVDS_0_P))
    (pad A4 thru_hole circle (at -6.49986 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A6 thru_hole circle (at -4.50088 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 45 /S_LVDS_1_N))
    (pad A8 thru_hole circle (at -2.49936 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 46 /S_LVDS_2_P))
    (pad A10 thru_hole circle (at -0.50038 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B1 thru_hole circle (at -9.4996 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 20 /S_SDA))
    (pad B2 thru_hole circle (at -8.49884 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 21 /S_SCL))
    (pad B3 thru_hole circle (at -7.50062 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B4 thru_hole circle (at -6.49986 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 14 /S_IO0))
    (pad B5 thru_hole circle (at -5.4991 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 /S_IO1))
    (pad B6 thru_hole circle (at -4.50088 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 /S_IO2))
    (pad B7 thru_hole circle (at -3.50012 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 17 /S_IO3))
    (pad B8 thru_hole circle (at -2.49936 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 16 /S_IO4))
    (pad B9 thru_hole circle (at -1.50114 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 8 /S_IO5))
    (pad B10 thru_hole circle (at -0.50038 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 11 /S_IO6))
    (pad B11 thru_hole circle (at 0.50038 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 10 /S_IO7))
    (model walter/conn_pc/pci-x_conn-x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pc:pci-x_conn-x1 (layer B.Cu) (tedit 5702793D)
    (at 188.94954 166.95)
    (descr "PCI-X 1x card edge connector, FCI P/N 10018783-10x00x")
    (fp_text reference NORTH1 (at 0 5.99948) (layer B.SilkS))
    (fp_text value AXIOM-PCIE (at -0.10054 -6.168) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 2.14884 0) (size 2.4003 2.4003) (drill 2.4003) (layers *.Cu B.SilkS))
    (pad "" np_thru_hole circle (at 11.30046 0) (size 2.4003 2.4003) (drill 2.4003) (layers *.Cu B.SilkS))
    (pad A12 thru_hole circle (at 3.50012 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A13 thru_hole circle (at 4.50088 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 30 /N_LVDS_3_P))
    (pad A14 thru_hole circle (at 5.4991 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 31 /N_LVDS_3_N))
    (pad A15 thru_hole circle (at 6.49986 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A16 thru_hole circle (at 7.50062 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 32 /N_LVDS_4_P))
    (pad A17 thru_hole circle (at 8.49884 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 33 /N_LVDS_4_N))
    (pad A18 thru_hole circle (at 9.4996 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B13 thru_hole circle (at 4.50088 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B15 thru_hole circle (at 6.49986 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B17 thru_hole circle (at 8.49884 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 34 /N_LVDS_5_N))
    (pad B12 thru_hole circle (at 3.50012 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 55 /VCC5V0))
    (pad B14 thru_hole circle (at 5.4991 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B16 thru_hole circle (at 7.50062 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 35 /N_LVDS_5_P))
    (pad B18 thru_hole circle (at 9.4996 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A11 thru_hole circle (at 0.50038 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 28 "Net-(CN1-Pad2)"))
    (pad A9 thru_hole circle (at -1.50114 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 36 /N_LVDS_2_N))
    (pad A7 thru_hole circle (at -3.50012 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A5 thru_hole circle (at -5.4991 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 37 /N_LVDS_1_P))
    (pad A3 thru_hole circle (at -7.50062 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 38 /N_LVDS_0_N))
    (pad A1 thru_hole circle (at -9.4996 1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A2 thru_hole circle (at -8.49884 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 39 /N_LVDS_0_P))
    (pad A4 thru_hole circle (at -6.49986 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad A6 thru_hole circle (at -4.50088 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 40 /N_LVDS_1_N))
    (pad A8 thru_hole circle (at -2.49936 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 41 /N_LVDS_2_P))
    (pad A10 thru_hole circle (at -0.50038 3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad B1 thru_hole circle (at -9.4996 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 25 /N_SDA))
    (pad B2 thru_hole circle (at -8.49884 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 26 /N_SCL))
    (pad B3 thru_hole circle (at -7.50062 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 /VCC3V3))
    (pad B4 thru_hole circle (at -6.49986 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 15 /N_IO0))
    (pad B5 thru_hole circle (at -5.4991 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 24 /N_IO1))
    (pad B6 thru_hole circle (at -4.50088 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 23 /N_IO2))
    (pad B7 thru_hole circle (at -3.50012 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 22 /N_IO3))
    (pad B8 thru_hole circle (at -2.49936 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 9 /N_IO4))
    (pad B9 thru_hole circle (at -1.50114 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 27 /N_IO5))
    (pad B10 thru_hole circle (at -0.50038 -3.2512) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 /N_IO6))
    (pad B11 thru_hole circle (at 0.50038 -1.24968) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 /N_IO7))
    (model walter/conn_pc/pci-x_conn-x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 56FCFD06)
    (at 180.330313 176.19529 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.064 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56FCFEB7)
    (at 177.028313 178.48129)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.254 1.524 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SMDAT))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57027961)
    (at 197.358 158.496 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference CN1 (at -0.127 -1.905 180) (layer F.SilkS))
    (fp_text value C (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(CN1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56FCFEBF)
    (at 177.028313 173.27429)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.27 -1.524 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SMCLK))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57027968)
    (at 191.643 158.496)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RN1 (at 0 1.651) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(CN1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 56FCFEE9)
    (at 177.028313 175.891467)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -2.276313 -0.885467 90) (layer F.SilkS))
    (fp_text value 24AA01/24LC01B (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /SMCLK))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /SMDAT))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57027D1D)
    (at 224.663 158.496 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference CS1 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value C (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(CS1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57027D0B)
    (at 218.948 158.496)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RS1 (at 0.127 1.651) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCC3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(CS1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57028867)
    (at 184.404 158.369 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CI2CN1 (at -1.143 -4.445 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 2.286 3.683 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VCC3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /N_SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /N_SDA))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57028874)
    (at 214.249 158.369 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CI2CS1 (at -1.143 11.557 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 2.286 3.683 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VCC3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /S_SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /S_SDA))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 577C2E50)
    (at 165.608 178.816 180)
    (attr smd)
    (fp_text reference CV1 (at -0.127 -1.778 180) (layer F.SilkS))
    (fp_text value CP1 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC12V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5702808D)
    (at 165.608 176.276 180)
    (attr smd)
    (fp_text reference CV2 (at -3.556 -0.127 270) (layer F.SilkS))
    (fp_text value CP1 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC12V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 57028090)
    (at 165.608 173.736 180)
    (attr smd)
    (fp_text reference CV3 (at -4.318 0.127 180) (layer F.SilkS))
    (fp_text value CP1 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC12V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 570280B3)
    (at 175.387 166.37 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference CV4 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value C (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /VCC5V0))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57028200)
    (at 169.164 160.02)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference CV5 (at 4.572 0) (layer F.SilkS))
    (fp_text value C (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /VCC5V0))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 169.164 157.734)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference CV6 (at 4.572 0) (layer F.SilkS))
    (fp_text value C (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /VCC5V0))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 57028211)
    (at 170.942 166.878 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U2 (at 6.35 -2.286 360) (layer F.SilkS))
    (fp_text value LM317T (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 55 /VCC5V0))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VCC12V))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 57028219)
    (at 166.624 166.878 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U3 (at 6.223 -2.413 180) (layer F.SilkS))
    (fp_text value LM7805CT (at 0.127 -3.683 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 55 /VCC5V0))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VCC12V))
  )
  (module TOFE_8X_Pins:TOFE_8X_Pins locked (layer F.Cu) (tedit 5749066E)
    (at 174 188.15)
    (fp_text reference TOFE1 (at 0.98044 0.9271) (layer F.SilkS))
    (fp_text value TOFE-8X (at 19.175 -10.75) (layer F.SilkS) hide)
    (pad B1 connect rect (at 0.69922 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B2 connect rect (at 1.69998 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B3 connect rect (at 2.6982 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B4 connect rect (at 3.69896 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B5 connect rect (at 4.69972 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 6 /SMCLK))
    (pad B6 connect rect (at 5.69794 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 7 /SMDAT))
    (pad B7 connect rect (at 6.6987 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B8 connect rect (at 7.69946 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 4 /VCC3V3))
    (pad B9 connect rect (at 8.69768 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 8 /S_IO5))
    (pad B10 connect rect (at 9.69844 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 4 /VCC3V3))
    (pad B11 connect rect (at 10.6992 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 27 /N_IO5))
    (pad B12 connect rect (at 13.69894 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 9 /N_IO4))
    (pad B13 connect rect (at 14.6997 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B14 connect rect (at 15.69792 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 39 /N_LVDS_0_P))
    (pad B15 connect rect (at 16.69868 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 38 /N_LVDS_0_N))
    (pad B16 connect rect (at 17.69944 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B17 connect rect (at 18.69766 -3.70126) (size 0.65024 3.59918) (layers F.Cu F.Mask)
      (net 1 /PRSTN))
    (pad B18 connect rect (at 19.69842 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B19 connect rect (at 20.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 37 /N_LVDS_1_P))
    (pad B20 connect rect (at 21.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 40 /N_LVDS_1_N))
    (pad B21 connect rect (at 22.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B22 connect rect (at 23.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B23 connect rect (at 24.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 41 /N_LVDS_2_P))
    (pad B24 connect rect (at 25.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 36 /N_LVDS_2_N))
    (pad B25 connect rect (at 26.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B26 connect rect (at 27.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B27 connect rect (at 28.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 30 /N_LVDS_3_P))
    (pad B28 connect rect (at 29.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 31 /N_LVDS_3_N))
    (pad B29 connect rect (at 30.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B30 connect rect (at 31.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 22 /N_IO3))
    (pad B31 connect rect (at 32.69882 -3.70088) (size 0.65024 3.59918) (layers F.Cu F.Mask)
      (net 1 /PRSTN))
    (pad B32 connect rect (at 33.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B33 connect rect (at 34.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 32 /N_LVDS_4_P))
    (pad B34 connect rect (at 35.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 33 /N_LVDS_4_N))
    (pad B35 connect rect (at 36.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B36 connect rect (at 37.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B37 connect rect (at 38.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 35 /N_LVDS_5_P))
    (pad B38 connect rect (at 39.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 34 /N_LVDS_5_N))
    (pad B39 connect rect (at 40.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B40 connect rect (at 41.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B41 connect rect (at 42.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 23 /N_IO2))
    (pad B42 connect rect (at 43.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 24 /N_IO1))
    (pad B43 connect rect (at 44.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B44 connect rect (at 45.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B45 connect rect (at 46.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 25 /N_SDA))
    (pad B46 connect rect (at 47.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 26 /N_SCL))
    (pad B47 connect rect (at 48.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B48 connect rect (at 49.69882 -3.70088) (size 0.65024 3.59918) (layers F.Cu F.Mask)
      (net 1 /PRSTN))
    (pad B49 connect rect (at 50.69882 -3.20088) (size 0.65024 4.59994) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B1 connect circle (at 0.69922 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B2 connect circle (at 1.69998 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B3 connect circle (at 2.6982 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 3 /VCC12V))
    (pad B4 connect circle (at 3.69896 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B5 connect circle (at 4.69972 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 6 /SMCLK))
    (pad B6 connect circle (at 5.69794 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 7 /SMDAT))
    (pad B7 connect circle (at 6.6987 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B8 connect circle (at 7.69946 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 4 /VCC3V3))
    (pad B9 connect circle (at 8.69768 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 8 /S_IO5))
    (pad B10 connect circle (at 9.69844 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 4 /VCC3V3))
    (pad B11 connect circle (at 10.6992 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 27 /N_IO5))
    (pad B12 connect circle (at 13.69894 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 9 /N_IO4))
    (pad B13 connect circle (at 14.6997 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B14 connect circle (at 15.69792 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 39 /N_LVDS_0_P))
    (pad B15 connect circle (at 16.69868 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 38 /N_LVDS_0_N))
    (pad B16 connect circle (at 17.69944 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B18 connect circle (at 19.69842 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B19 connect circle (at 20.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 37 /N_LVDS_1_P))
    (pad B20 connect circle (at 21.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 40 /N_LVDS_1_N))
    (pad B21 connect circle (at 22.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B22 connect circle (at 23.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B23 connect circle (at 24.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 41 /N_LVDS_2_P))
    (pad B24 connect circle (at 25.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 36 /N_LVDS_2_N))
    (pad B25 connect circle (at 26.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B26 connect circle (at 27.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B27 connect circle (at 28.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 30 /N_LVDS_3_P))
    (pad B28 connect circle (at 29.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 31 /N_LVDS_3_N))
    (pad B29 connect circle (at 30.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B30 connect circle (at 31.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 22 /N_IO3))
    (pad B32 connect circle (at 33.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B33 connect circle (at 34.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 32 /N_LVDS_4_P))
    (pad B34 connect circle (at 35.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 33 /N_LVDS_4_N))
    (pad B35 connect circle (at 36.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B36 connect circle (at 37.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B37 connect circle (at 38.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 35 /N_LVDS_5_P))
    (pad B38 connect circle (at 39.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 34 /N_LVDS_5_N))
    (pad B39 connect circle (at 40.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B40 connect circle (at 41.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B41 connect circle (at 42.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 23 /N_IO2))
    (pad B42 connect circle (at 43.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 24 /N_IO1))
    (pad B43 connect circle (at 44.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B44 connect circle (at 45.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B45 connect circle (at 46.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 25 /N_SDA))
    (pad B46 connect circle (at 47.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 26 /N_SCL))
    (pad B47 connect circle (at 48.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad B49 connect circle (at 50.69882 -0.89964) (size 0.65024 0.65024) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad A1 connect rect (at 0.69922 -3.70126) (size 0.65024 3.59918) (layers B.Cu B.Mask)
      (net 1 /PRSTN))
    (pad A2 connect rect (at 1.69998 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 3 /VCC12V))
    (pad A3 connect rect (at 2.6982 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 3 /VCC12V))
    (pad A4 connect rect (at 3.69896 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A5 connect rect (at 4.69972 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 10 /S_IO7))
    (pad A6 connect rect (at 5.69794 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 11 /S_IO6))
    (pad A7 connect rect (at 6.6987 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 12 /N_IO7))
    (pad A8 connect rect (at 7.69946 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 13 /N_IO6))
    (pad A9 connect rect (at 8.69768 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 4 /VCC3V3))
    (pad A10 connect rect (at 9.69844 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 4 /VCC3V3))
    (pad A11 connect rect (at 10.6992 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 2 /RESET))
    (pad A12 connect rect (at 13.69894 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A13 connect rect (at 14.6997 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 15 /N_IO0))
    (pad A14 connect rect (at 15.69792 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 14 /S_IO0))
    (pad A15 connect rect (at 16.69868 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A16 connect rect (at 17.69944 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 42 /S_LVDS_0_P))
    (pad A17 connect rect (at 18.69766 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 43 /S_LVDS_0_N))
    (pad A18 connect rect (at 19.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A19 connect rect (at 20.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 16 /S_IO4))
    (pad A20 connect rect (at 21.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A21 connect rect (at 22.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 44 /S_LVDS_1_P))
    (pad A22 connect rect (at 23.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 45 /S_LVDS_1_N))
    (pad A23 connect rect (at 24.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A24 connect rect (at 25.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A25 connect rect (at 26.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 46 /S_LVDS_2_P))
    (pad A26 connect rect (at 27.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 47 /S_LVDS_2_N))
    (pad A27 connect rect (at 28.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A28 connect rect (at 29.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A29 connect rect (at 30.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 48 /S_LVDS_3_P))
    (pad A30 connect rect (at 31.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 49 /S_LVDS_3_N))
    (pad A31 connect rect (at 32.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A32 connect rect (at 33.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 17 /S_IO3))
    (pad A33 connect rect (at 34.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 29 "Net-(TOFE1-PadA33)"))
    (pad A34 connect rect (at 35.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A35 connect rect (at 36.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 50 /S_LVDS_4_P))
    (pad A36 connect rect (at 37.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 51 /S_LVDS_4_N))
    (pad A37 connect rect (at 38.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A38 connect rect (at 39.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A39 connect rect (at 40.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 52 /S_LVDS_5_P))
    (pad A40 connect rect (at 41.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 53 /S_LVDS_5_N))
    (pad A41 connect rect (at 42.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A42 connect rect (at 43.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A43 connect rect (at 44.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 18 /S_IO2))
    (pad A44 connect rect (at 45.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 19 /S_IO1))
    (pad A45 connect rect (at 46.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A46 connect rect (at 47.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A47 connect rect (at 48.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 20 /S_SDA))
    (pad A48 connect rect (at 49.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 21 /S_SCL))
    (pad A49 connect rect (at 50.69882 -3.20088) (size 0.65024 4.59994) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A2 connect oval (at 1.69998 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 3 /VCC12V))
    (pad A3 connect oval (at 2.6982 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 3 /VCC12V))
    (pad A4 connect oval (at 3.69896 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A5 connect oval (at 4.69972 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 10 /S_IO7))
    (pad A6 connect oval (at 5.69794 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 11 /S_IO6))
    (pad A7 connect oval (at 6.6987 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 12 /N_IO7))
    (pad A8 connect oval (at 7.69946 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 13 /N_IO6))
    (pad A9 connect oval (at 8.69768 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 4 /VCC3V3))
    (pad A10 connect oval (at 9.69844 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 4 /VCC3V3))
    (pad A11 connect oval (at 10.6992 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 2 /RESET))
    (pad A12 connect oval (at 13.69894 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A13 connect oval (at 14.6997 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 15 /N_IO0))
    (pad A14 connect oval (at 15.69792 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 14 /S_IO0))
    (pad A15 connect oval (at 16.69868 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A16 connect oval (at 17.69944 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 42 /S_LVDS_0_P))
    (pad A17 connect oval (at 18.69766 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 43 /S_LVDS_0_N))
    (pad A18 connect oval (at 19.69842 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A19 connect oval (at 20.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 16 /S_IO4))
    (pad A20 connect oval (at 21.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A21 connect oval (at 22.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 44 /S_LVDS_1_P))
    (pad A22 connect oval (at 23.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 45 /S_LVDS_1_N))
    (pad A23 connect oval (at 24.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A24 connect oval (at 25.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A25 connect oval (at 26.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 46 /S_LVDS_2_P))
    (pad A26 connect oval (at 27.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 47 /S_LVDS_2_N))
    (pad A27 connect oval (at 28.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A28 connect oval (at 29.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A29 connect oval (at 30.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 48 /S_LVDS_3_P))
    (pad A30 connect oval (at 31.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 49 /S_LVDS_3_N))
    (pad A31 connect oval (at 32.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A32 connect oval (at 33.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 17 /S_IO3))
    (pad A33 connect oval (at 34.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 29 "Net-(TOFE1-PadA33)"))
    (pad A34 connect oval (at 35.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A35 connect oval (at 36.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 50 /S_LVDS_4_P))
    (pad A36 connect oval (at 37.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 51 /S_LVDS_4_N))
    (pad A37 connect oval (at 38.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A38 connect oval (at 39.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A39 connect oval (at 40.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 52 /S_LVDS_5_P))
    (pad A40 connect oval (at 41.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 53 /S_LVDS_5_N))
    (pad A41 connect oval (at 42.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A42 connect oval (at 43.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A43 connect oval (at 44.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 18 /S_IO2))
    (pad A44 connect oval (at 45.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 19 /S_IO1))
    (pad A45 connect oval (at 46.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A46 connect oval (at 47.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad A47 connect oval (at 48.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 20 /S_SDA))
    (pad A48 connect oval (at 49.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 21 /S_SCL))
    (pad A49 connect oval (at 50.69882 -0.89964 90) (size 0.65024 0.65024) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad "" smd rect (at -1.92618 -13.25088) (size 4 1) (layers B.Cu))
    (pad "" smd rect (at -1.92618 -13.25088) (size 4 1) (layers F.Cu))
  )
  (gr_text "v0.2-3-gc8a8df7" (at 189.624 177.668) (layer F.SilkS))
  (gr_text "TOFE to AXIOM Adapter\ntofe.io" (at 189.624 173.918) (layer F.SilkS))
  (gr_text "TO BE INCLUDED ON ALL BOARDS." (at 54.864 137.668) (layer Dwgs.User))
  (gr_text "8. MANUFACTURER'S UL LOGO AND DATE CODE" (at 51.054 131.318) (layer Dwgs.User))
  (gr_text "FOR SHORT AND OPEN CIRCUITS." (at 54.864 124.968) (layer Dwgs.User))
  (gr_text "7. FINISHED PCB TO BE ELECTRICALLY TESTED" (at 51.054 118.618) (layer Dwgs.User))
  (gr_text "NON-CONDUCTIVE INK." (at 54.864 112.268) (layer Dwgs.User))
  (gr_text "6. SILKSCREEN TOP WITH WHITE, PERMANENT," (at 51.054 105.918) (layer Dwgs.User))
  (gr_text " " (at 54.864 80.518) (layer Dwgs.User))
  (gr_text "PCB SURFACE FINISH TO BE HASL." (at 54.864 80.518) (layer Dwgs.User))
  (gr_text "OVER BARE COPPER.  COLOR: GREEN." (at 54.864 99.568) (layer Dwgs.User))
  (gr_text "5. SOLDERMASK BOTH SIDES PER IPC-SM-840 CLASS 3" (at 51.054 93.218) (layer Dwgs.User))
  (gr_text "PLATED HOLES TO HAVE 1/4 OZ MINIMUM." (at 54.864 86.868) (layer Dwgs.User))
  (gr_text "4. FINISHED CU, ALL 4 LAYERS, TO BE 1/2 OZ AFTER PLATING." (at 51.054 74.168) (layer Dwgs.User))
  (gr_text "3. PCB MATERIAL MUST MEET UL 94V-0 FLAMMABILITY RATING." (at 51.054 67.818) (layer Dwgs.User))
  (gr_text "CLASS 2, PER IPC-6011 USING SUPPLIED DATA FILES." (at 54.864 61.468) (layer Dwgs.User))
  (gr_text "2. FABRICATE PCB IN ACCORDANCE WITH IPC 6012-A " (at 51.054 55.118) (layer Dwgs.User))
  (gr_text "4 LAYERS, 1/2 +/- 10% OZ FINISHED ." (at 54.864 48.768) (layer Dwgs.User))
  (gr_text "1. PCB LAMINATE IN ACCORDANCE WITH IPE-4101B/21," (at 51.054 42.418) (layer Dwgs.User))
  (gr_text "NOTES :  (DIMENSIONS IN MM)" (at 44.704 33.528) (layer Dwgs.User))
  (gr_text .75 (at 304.292 176.149) (layer Dwgs.User))
  (gr_text "TYP 2" (at 314.071 161.798) (layer Dwgs.User))
  (gr_text "30 DEGREES" (at 314.071 157.607) (layer Dwgs.User))
  (gr_text "NO SCALE" (at 308.102 191.262) (layer Dwgs.User))
  (gr_text "VIEW A-A" (at 306.959 186.309) (layer Dwgs.User))
  (gr_text A (at 271.907 189.738) (layer Dwgs.User))
  (gr_text A (at 271.653 182.245) (layer Dwgs.User))
  (gr_text "5.75 REF" (at 83.693 176.784) (layer Dwgs.User))
  (gr_text "5.75 REF" (at 149.606 178.689) (layer Dwgs.User))
  (gr_text "NO SCALE" (at 108.966 201.295) (layer Dwgs.User))
  (gr_text "DETAIL A" (at 108.966 197.104) (layer Dwgs.User))
  (gr_text 2.40R (at 103.378 167.132) (layer Dwgs.User))
  (gr_text 4.10 (at 94.361 177.038 90) (layer Dwgs.User))
  (gr_text "3.75 REF" (at 103.759 190.119) (layer Dwgs.User))
  (gr_text 1.90 (at 103.632 185.039) (layer Dwgs.User))
  (gr_text "DETAIL A" (at 149.86 197.231) (layer Dwgs.User))
  (gr_text "DRILL ORIGIN" (at 149.987 188.468) (layer Dwgs.User))
  (gr_text 31.90 (at 259.715 172.847 90) (layer Dwgs.User))
  (gr_text 22.90 (at 252.095 167.132 90) (layer Dwgs.User))
  (gr_text 21.00 (at 244.602 167.132 90) (layer Dwgs.User))
  (gr_text 10.75 (at 236.22 161.798 90) (layer Dwgs.User))
  (gr_text 38.25 (at 204.597 200.533) (layer Dwgs.User))
  (gr_text 11.25 (at 179.07 200.533) (layer Dwgs.User))
  (gr_text 8.00 (at 165.862 200.533) (layer Dwgs.User))
  (gr_text 1.75 (at 193.294 193.04) (layer Dwgs.User))
  (gr_text 3.75 (at 172.466 193.04 90) (layer Dwgs.User))
  (gr_text 25.00 (at 137.541 168.402 90) (layer Dwgs.User))
  (gr_text 19.25 (at 145.288 165.989 90) (layer Dwgs.User))
  (gr_text 13.05 (at 152.781 162.814 90) (layer Dwgs.User))
  (gr_text TOP (at 141.351 138.811) (layer Dwgs.User))
  (gr_text 9.15 (at 224.155 138.684) (layer Dwgs.User))
  (gr_text 4.40 (at 172.72 150.495) (layer Dwgs.User))
  (gr_text 9.15 (at 201.676 146.685) (layer Dwgs.User))
  (gr_text 28.90 (at 176.784 144.272) (layer Dwgs.User))
  (gr_text 57.49 (at 195.199 139.192) (layer Dwgs.User))
  (gr_text 68.95 (at 195.326 133.985) (layer Dwgs.User))
  (gr_line (start 187 179.15) (end 185.25 179.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 185.25 179.15) (end 185.25 188.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 187 188.15) (end 187 179.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 174 175.67736) (end 173.75 175.42736) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 174 175.72006) (end 174 188.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 162.25 156.2481) (end 162.25 181.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 170.22572 175.4886) (end 170.22572 181.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 170.17238 181.25) (end 162.25 181.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 225.2472 177.25) (end 231.1654 177.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 231.16286 156.2481) (end 162.25 156.2481) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 231.1654 177.2412) (end 231.1654 156.2481) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 185.25 188.15) (end 174 188.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 225.25 188.15) (end 187 188.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 225.25 177.25) (end 225.25 188.15) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 172.01524 177.1926) (end 170.26524 175.4426) (angle 91) (layer Edge.Cuts) (width 0.381))
  (zone (net 5) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.306 156.21) (xy 231.14 156.21) (xy 231.14 177.292) (xy 225.298 177.292) (xy 225.298 188.214)
        (xy 187.071 188.214) (xy 187.071 179.07) (xy 185.166 179.07) (xy 185.166 188.214) (xy 174.117 188.214)
        (xy 174.117 174.625) (xy 170.053 174.625) (xy 170.053 181.229) (xy 162.306 181.229) (xy 162.306 156.337)
      )
    )
  )
  (zone (net 3) (net_name /VCC12V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.244 186.944) (xy 177.038 186.944) (xy 177.038 169.672) (xy 176.784 168.783) (xy 162.179 168.783)
        (xy 162.306 181.356) (xy 170.18 181.356) (xy 170.18 174.244) (xy 174.244 174.244)
      )
    )
  )
  (zone (net 4) (net_name /VCC3V3) (layer In2.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.14 177.292) (xy 225.298 177.292) (xy 225.298 186.944) (xy 177.038 186.944) (xy 177.038 164.592)
        (xy 231.14 164.592) (xy 231.14 177.292)
      )
    )
  )
  (zone (net 55) (net_name /VCC5V0) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 230.759 164.338) (xy 201.549 164.338) (xy 200.914 164.338) (xy 194.564 164.338) (xy 193.294 164.338)
        (xy 176.784 164.338) (xy 176.784 168.148) (xy 162.814 168.148) (xy 162.814 156.718) (xy 230.759 156.718)
        (xy 230.759 164.338)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.14 177.292) (xy 225.298 177.292) (xy 225.298 182.397345) (xy 187.071 182.396014) (xy 187.071 179.07)
        (xy 185.166 179.07) (xy 185.166 182.397179) (xy 174.117 182.38942) (xy 174.117 174.625) (xy 170.053 174.625)
        (xy 170.053 181.229) (xy 162.306 181.229) (xy 162.306 156.21) (xy 231.14 156.21) (xy 231.14 177.292)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 231.1146 177.292) (xy 225.2726 177.292) (xy 225.2726 182.397345) (xy 187.0456 182.396014) (xy 187.0456 179.07)
        (xy 185.1406 179.07) (xy 185.1406 182.397179) (xy 174.0916 182.38942) (xy 174.0916 174.625) (xy 170.0276 174.625)
        (xy 170.0276 181.229) (xy 162.2806 181.229) (xy 162.2806 156.21) (xy 231.1146 156.21) (xy 231.1146 177.292)
      )
    )
  )
)
