(kicad_pcb (version 20171130) (host pcbnew "(6.0.0-rc1-dev-1538-g72c885797)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 98)
    (zones 0)
    (modules 5)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 142.127 93.127)
    (grid_origin 142.127 93.127)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "BMA253-ribbon-gerbers/"))
  )
  (net 0 "")
  (net 1 /VDD)
  (net 2 /GND)
  (net 3 /CSB)
  (net 4 /SCK)
  (net 5 /SDO)
  (net 6 /SDI)
  (net 7 /INT1)
  (net 8 /INT2)
  (net 9 "Net-(C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CSB)
    (add_net /GND)
    (add_net /INT1)
    (add_net /INT2)
    (add_net /SCK)
    (add_net /SDI)
    (add_net /SDO)
    (add_net /VDD)
    (add_net "Net-(C1-Pad1)")
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 142.966 98.3764 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.35 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 148.046 98.817 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -1.566 -0.0508 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 142.957 100.383 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 2.2182 0.0172 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module izzy:conn-2x4-1.27mm-0.5in-pad (layer F.Cu) (tedit 5D3772A0)
    (at 145.455 94.5156)
    (attr smd)
    (fp_text reference J1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Counter_Clockwise (at 0 -2.54) (layer F.Fab))
    (pad 8 smd oval (at -1.905 0) (size 1 2.54) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 7 smd oval (at -0.635 0) (size 1 2.54) (layers B.Cu B.Paste B.Mask)
      (net 3 /CSB))
    (pad 6 smd oval (at 0.635 0) (size 1 2.54) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCK))
    (pad 5 smd oval (at 1.905 0) (size 1 2.54) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDO))
    (pad 4 smd oval (at 1.905 0) (size 1 2.54) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDI))
    (pad 3 smd oval (at 0.635 0) (size 1 2.54) (layers F.Cu F.Paste F.Mask)
      (net 7 /INT1))
    (pad 2 smd oval (at -0.635 0) (size 1 2.54) (layers F.Cu F.Paste F.Mask)
      (net 8 /INT2))
    (pad 1 smd rect (at -1.905 0) (size 1 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
  )
  (module izzy:LGA-12 (layer F.Cu) (tedit 5D377292)
    (at 145.853 100.434 180)
    (attr smd)
    (fp_text reference U1 (at -0.0078 2.227 180) (layer F.SilkS))
    (fp_text value BMA253 (at 0 -2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.065 -0.75 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 /SDO))
    (pad 2 smd rect (at -1.065 -0.25 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDI))
    (pad 3 smd rect (at -1.065 0.25 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 /VDD))
    (pad 4 smd rect (at -1.065 0.75 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.25 1.065 180) (size 0.28 0.91) (layers F.Cu F.Paste F.Mask)
      (net 7 /INT1))
    (pad 6 smd rect (at 0.25 1.065 180) (size 0.28 0.91) (layers F.Cu F.Paste F.Mask)
      (net 8 /INT2))
    (pad 7 smd rect (at 1.065 0.75 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at 1.065 0.25 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 9 smd rect (at 1.065 -0.25 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 10 smd rect (at 1.065 -0.75 180) (size 0.91 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 /CSB))
    (pad 11 smd rect (at 0.25 -1.065 180) (size 0.28 0.91) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 12 smd rect (at -0.25 -1.065 180) (size 0.28 0.91) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCK))
  )
  (gr_line (start 148.7822 103.5326) (end 142.127 103.5326) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.7822 93.127) (end 148.7822 103.5326) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.127 93.127) (end 148.7822 93.127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.127 103.5326) (end 142.127 93.127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.457101 101.043) (xy 146.457102 99.8238) (xy 145.237902 99.8238) (xy 145.237902 101.043)
      )
    )
  )
)
