<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="67.564" y2="0" width="0" layer="20"/>
<wire x1="67.564" y1="0" x2="67.564" y2="47.879" width="0" layer="20"/>
<wire x1="67.564" y1="47.879" x2="0" y2="47.879" width="0" layer="20"/>
<wire x1="0" y1="47.879" x2="0" y2="0" width="0" layer="20"/>
<text>Power and Voltage Sensors
See Insights, LLC November, 2018
chip@seeinsights.com</text>
<hole x="23.368" y="17.526" drill="0.35"/>
<hole x="23.368" y="12.954" drill="0.35"/>
<hole x="23.368" y="6.604" drill="0.35"/>
<hole x="23.368" y="1.778" drill="0.35"/>
<wire x1="23.368" y1="6.604" x2="23.368" y2="1.778" width="1.016" layer="46"/>
<wire x1="23.368" y1="17.526" x2="23.368" y2="12.7" width="1.016" layer="46"/>
<wire x1="18.288" y1="46.228" x2="18.288" y2="20.828" width="1.016" layer="46"/>
<hole x="18.288" y="46.228" drill="0.35"/>
<hole x="18.288" y="20.828" drill="0.35"/>
<text>AC/L</text>
<text>AC/N</text>
<text>~</text>
<text>~</text>
<text>AC1</text>
<text>~</text>
<text>~</text>
<text>AC2</text>
<text>VCC</text>
<text>AC2</text>
<text>AC1</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
<text>5V @ 2A DC
Power to Electron</text>
<text>Vcc from Electron</text>
<text>Shock Hazard!</text>
<text>Shock Hazard!</text>
<text>Shock Hazard!</text>
<text>Shock Hazard!</text>
<text>Shock Hazard!</text>
<text>Shock Hazard!</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="old-adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL4-SMD">
<description>&lt;b&gt;Dual  In Line SMD&lt;/b&gt; 4 pol.&lt;p&gt;
Source: LITE-ON ELECTRONICS, LTV816.pdf</description>
</package>
</packages>
</library>
<library name="PJS">
<packages>
<package name="3.2-MOUNT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-4">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Custom Components">
<packages>
<package name="TSSOP-8">
</package>
<package name="IRM-10-TH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="OK1" library="optocoupler" package="DIL4-SMD" value="LTV-8141S-TA1">
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="MPN" value="SFH6206-3"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469585"/>
<attribute name="OC_NEWARK" value="58K2214"/>
</element>
<element name="C1" library="adafruit" package="C0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="old-adafruit" package="M1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R2" library="old-adafruit" package="M1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R4" library="old-adafruit" package="M1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="R5" library="old-adafruit" package="M1206" value="22k">
<attribute name="NAME"/>
</element>
<element name="U$1" library="PJS" package="3.2-MOUNT" value=""/>
<element name="C6" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U$4" library="PJS" package="3.2-MOUNT" value=""/>
<element name="OK2" library="optocoupler" package="DIL4-SMD" value="LTV-8141S-TA1">
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="MPN" value="SFH6206-3"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1469585"/>
<attribute name="OC_NEWARK" value="58K2214"/>
</element>
<element name="R6" library="old-adafruit" package="R0805" value="100K">
<attribute name="NAME"/>
</element>
<element name="R3" library="old-adafruit" package="R0805" value="100K">
<attribute name="NAME"/>
</element>
<element name="R11" library="old-adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R12" library="old-adafruit" package="R0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="SCHMITT-INVERTER" library="Custom Components" package="TSSOP-8" value="74AHC3G14">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="old-adafruit" package="R0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R8" library="old-adafruit" package="R0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="IRM-10-TH" library="Custom Components" package="IRM-10-TH" value="IRM-10-TH">
<attribute name="NAME"/>
</element>
<element name="DC-OUT" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="AC1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="AC2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="AC-IN" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08399"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="2xCONN-08399"/>
<attribute name="SF_ID" value="2xPRT-08084"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="PJS" package="3.2-MOUNT" value=""/>
<element name="U$6" library="PJS" package="3.2-MOUNT" value=""/>
</elements>
<signals>
<signal name="N$12">
<contactref element="R1" pad="1"/>
<contactref element="AC1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="AC1" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="OK1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="SCHMITT-INVERTER" pad="4"/>
<contactref element="SCHMITT-INVERTER" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="IRM-10-TH" pad="-V"/>
<contactref element="DC-OUT" pad="1"/>
</signal>
<signal name="AC1-RAW">
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="SCHMITT-INVERTER" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="OK1" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="1"/>
<contactref element="AC2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="AC2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="AC2-RAW">
<contactref element="C2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="SCHMITT-INVERTER" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="OK2" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="OK1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="2"/>
<contactref element="OK2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="OK1" pad="4"/>
<contactref element="OK2" pad="4"/>
<contactref element="SCHMITT-INVERTER" pad="8"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="AC1-OUT">
<contactref element="SCHMITT-INVERTER" pad="7"/>
<contactref element="LED1" pad="C"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="AC2-OUT">
<contactref element="SCHMITT-INVERTER" pad="5"/>
<contactref element="LED2" pad="C"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="A"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="AC/L">
<contactref element="AC-IN" pad="2"/>
<contactref element="IRM-10-TH" pad="AC/L"/>
</signal>
<signal name="AC/N">
<contactref element="AC-IN" pad="1"/>
<contactref element="IRM-10-TH" pad="AC/N"/>
</signal>
<signal name="N$15">
<contactref element="IRM-10-TH" pad="+V"/>
<contactref element="DC-OUT" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
