(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 102)
    (no_connects 0)
    (area 50.216999 28.556999 226.135001 103.707001)
    (thickness 1.6002)
    (drawings 58)
    (tracks 342)
    (zones 0)
    (modules 46)
    (nets 56)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.5 1.5)
    (mod_text_width 0.3)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 50.292 103.632)
    (grid_origin 50.292 103.632)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 IN+A)
  (net 2 IN-A)
  (net 3 VSS-B)
  (net 4 VCC-B)
  (net 5 J1-A)
  (net 6 J2-A)
  (net 7 J1-C)
  (net 8 J2-C)
  (net 9 J3-A)
  (net 10 J4-A)
  (net 11 J3-C)
  (net 12 J4-C)
  (net 13 J5-A)
  (net 14 J6-A)
  (net 15 J5-C)
  (net 16 J6-C)
  (net 17 J7-A)
  (net 18 VCC-A)
  (net 19 VSS-A)
  (net 20 IN+B)
  (net 21 IN-B)
  (net 22 J1-B)
  (net 23 J2-B)
  (net 24 J3-B)
  (net 25 J4-B)
  (net 26 J5-B)
  (net 27 J6-B)
  (net 28 GND-A)
  (net 29 OUT-A)
  (net 30 OUT+A)
  (net 31 OUT+B)
  (net 32 OUT-B)
  (net 33 +12V)
  (net 34 -12V)
  (net 35 +5V)
  (net 36 -5V)
  (net 37 IN-)
  (net 38 IN+)
  (net 39 OUT-)
  (net 40 OUT+)
  (net 41 GNDPWR)
  (net 42 VDD)
  (net 43 VPP)
  (net 44 GND-A2)
  (net 45 J6-A2)
  (net 46 J4-A2)
  (net 47 J2-A2)
  (net 48 J7-A2)
  (net 49 VSS-A2)
  (net 50 VCC-A2)
  (net 51 IN+A2)
  (net 52 IN-A2)
  (net 53 J1-A2)
  (net 54 J3-A2)
  (net 55 J5-A2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND-A)
    (add_net GND-A2)
    (add_net IN+)
    (add_net IN+A)
    (add_net IN+A2)
    (add_net IN+B)
    (add_net IN-)
    (add_net IN-A)
    (add_net IN-A2)
    (add_net IN-B)
    (add_net J1-A)
    (add_net J1-A2)
    (add_net J1-B)
    (add_net J1-C)
    (add_net J2-A)
    (add_net J2-A2)
    (add_net J2-B)
    (add_net J2-C)
    (add_net J3-A)
    (add_net J3-A2)
    (add_net J3-B)
    (add_net J3-C)
    (add_net J4-A)
    (add_net J4-A2)
    (add_net J4-B)
    (add_net J4-C)
    (add_net J5-A)
    (add_net J5-A2)
    (add_net J5-B)
    (add_net J5-C)
    (add_net J6-A)
    (add_net J6-A2)
    (add_net J6-B)
    (add_net J6-C)
    (add_net J7-A)
    (add_net J7-A2)
    (add_net OUT+)
    (add_net OUT+A)
    (add_net OUT+B)
    (add_net OUT-)
    (add_net OUT-A)
    (add_net OUT-B)
    (add_net VCC-A)
    (add_net VCC-A2)
    (add_net VCC-B)
    (add_net VDD)
    (add_net VPP)
    (add_net VSS-A)
    (add_net VSS-A2)
    (add_net VSS-B)
  )
  (net_class Thick ""
    (clearance 0.1524)
    (trace_width 0.3302)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +12V)
    (add_net +5V)
    (add_net -12V)
    (add_net -5V)
    (add_net GNDPWR)
  )
  (net_class Thin ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer Top) (tedit 58D16748)
    (at 131.572 61.976 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 4.064 7.112 360) (layer F.SilkS))
    (fp_text value U3 (at 3.81 12.7 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 J5-B))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 OUT+B))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 J6-B))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC-B))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VSS-B))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer Top) (tedit 58D16737)
    (at 81.28 69.596 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 6.858 360) (layer F.SilkS))
    (fp_text value U2 (at 3.81 -5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 J2-B))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 J4-B))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 IN-B))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC-B))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VSS-B))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer Top) (tedit 58D166F5)
    (at 81.28 54.864 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 4.064 6.604 360) (layer F.SilkS))
    (fp_text value U1 (at 3.81 -5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 J1-B))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 J3-B))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 IN+B))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC-B))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VSS-B))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LOGO (layer Top) (tedit 0)
    (at 110.236 66.04)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer Top) (tedit 58C07DE3)
    (at 220.98 35.652)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer Top) (tedit 58C07DEC)
    (at 205.74 35.652)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer Top) (tedit 58C07DF5)
    (at 220.98 96.612)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connectors_Molex:Molex_PicoBlade_53398-0971_09x1.25mm_Straight (layer Top) (tedit 58A3B79E)
    (at 185.928 66.294)
    (descr "Molex PicoBlade, single row, top entry type, surface mount, PN:53398-0971")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P3 (at 0 -3.25) (layer F.SilkS))
    (fp_text value "3PDT Switch" (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -5 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at -3.75 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 42 VDD))
    (pad 3 smd rect (at -2.5 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 35 +5V))
    (pad 4 smd rect (at -1.25 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask))
    (pad 5 smd rect (at 0 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 42 VDD))
    (pad 6 smd rect (at 1.25 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask))
    (pad 7 smd rect (at 2.5 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 34 -12V))
    (pad 8 smd rect (at 3.75 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 43 VPP))
    (pad 9 smd rect (at 5 -1.375) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 36 -5V))
    (pad "" smd rect (at -7.5 1.375) (size 2.2 3.1) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at 7.5 1.375) (size 2.2 3.1) (layers Top F.Paste F.Mask))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53398-0971_09x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA63)
    (at 70.104 45.212)
    (fp_text reference R1-A1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R1-A (at 0 4.445) (layer Eco2.User))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 7 J1-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA67)
    (at 85.344 45.212)
    (fp_text reference R1-B1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R1-B (at 0 4.445) (layer Eco2.User))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 9 J3-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA78)
    (at 70.104 86.868)
    (fp_text reference R2-A1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R2-A (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 8 J2-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA7D)
    (at 85.344 86.868)
    (fp_text reference R2-B1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R2-B (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 10 J4-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA6A)
    (at 95.504 45.212)
    (fp_text reference R3-A1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R3-A (at 0 4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 11 J3-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA6E)
    (at 110.744 45.212)
    (fp_text reference R3-B1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R3-B (at 0 4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 13 J5-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA7F)
    (at 95.504 86.868)
    (fp_text reference R4-A1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R4-A (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 12 J4-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA81)
    (at 110.744 86.868)
    (fp_text reference R4-B1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R4-B (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 14 J6-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA70)
    (at 120.904 45.212)
    (fp_text reference R5-A1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R5-A (at 0 4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 15 J5-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA73)
    (at 135.636 45.212)
    (fp_text reference R5-B1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value R5-B (at 0 4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 17 J7-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA84)
    (at 120.904 86.868)
    (fp_text reference R6-A1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R6-A (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 16 J6-C))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA88)
    (at 135.636 86.868)
    (fp_text reference R6-B1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value R6-B (at 0.127 -5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 32 OUT-B))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA99)
    (at 62.484 55.372)
    (fp_text reference RG-A1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value RG-A (at -0.635 -4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 5 J1-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:0393-0-15-01-07-27-10-0" (layer Top) (tedit 58B4AA97)
    (at 62.484 76.708)
    (fp_text reference RG-B1 (at 0 4.064) (layer F.SilkS) hide)
    (fp_text value RG-B (at 0 4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.66) (layers *.Cu *.Mask)
      (net 6 J2-A))
    (model C:/Users/tjames/0393-0-15-01-07-27-10-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53398-0871_08x1.25mm_Straight (layer Bottom) (tedit 58B5CC0E)
    (at 162.56 67.437 270)
    (descr "Molex PicoBlade, single row, top entry type, surface mount, PN:53398-0871")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P1 (at 0 3.25 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -4.25 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer B.Fab))
    (pad "" smd rect (at 6.875 -1.375 270) (size 2.2 3.1) (layers Bottom B.Paste B.Mask))
    (pad "" smd rect (at -6.875 -1.375 270) (size 2.2 3.1) (layers Bottom B.Paste B.Mask))
    (pad 8 smd rect (at 4.375 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask))
    (pad 7 smd rect (at 3.125 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 29 OUT-A))
    (pad 6 smd rect (at 1.875 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 30 OUT+A))
    (pad 5 smd rect (at 0.625 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 19 VSS-A))
    (pad 4 smd rect (at -0.625 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 28 GND-A))
    (pad 3 smd rect (at -1.875 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 18 VCC-A))
    (pad 2 smd rect (at -3.125 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 1 IN+A))
    (pad 1 smd rect (at -4.375 1.375 270) (size 0.8 1.5) (layers Bottom B.Paste B.Mask)
      (net 2 IN-A))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53398-0871_08x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:71661-7040" (layer Top) (tedit 58B5CC15)
    (at 156.464 78.232 270)
    (fp_text reference P2 (at -12.192 7.62 270) (layer F.SilkS) hide)
    (fp_text value DIL40 (at -12.192 -2.921 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.04 5.058 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.94 2.858 270) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 OUT-B))
    (pad 2 thru_hole circle (at -1.27 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 J6-C))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 J6-A))
    (pad 4 thru_hole circle (at -3.81 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 J4-C))
    (pad 5 thru_hole circle (at -5.08 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 J4-A))
    (pad 6 thru_hole circle (at -6.35 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 J2-C))
    (pad 7 thru_hole circle (at -7.62 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 OUT-A))
    (pad 8 thru_hole circle (at -8.89 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 OUT+A))
    (pad 9 thru_hole circle (at -10.16 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VSS-A))
    (pad 10 thru_hole circle (at -11.43 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 GND-A))
    (pad 11 thru_hole circle (at -12.7 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 VCC-A))
    (pad 12 thru_hole circle (at -13.97 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 IN+A))
    (pad 13 thru_hole circle (at -15.24 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 IN-A))
    (pad 14 thru_hole circle (at -16.51 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -17.78 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 J1-C))
    (pad 16 thru_hole circle (at -19.05 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 J3-A))
    (pad 17 thru_hole circle (at -20.32 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 J3-C))
    (pad 18 thru_hole circle (at -21.59 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 J5-A))
    (pad 19 thru_hole circle (at -22.86 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 J5-C))
    (pad 20 thru_hole circle (at -24.13 1.905 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 J7-A))
    (pad 21 thru_hole circle (at 0 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -1.27 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VSS-B))
    (pad 23 thru_hole circle (at -2.54 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 J4-B))
    (pad 24 thru_hole circle (at -3.81 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 IN-B))
    (pad 25 thru_hole circle (at -5.08 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 J2-B))
    (pad 26 thru_hole circle (at -6.35 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -7.62 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -8.89 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 OUT+B))
    (pad 29 thru_hole circle (at -10.16 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at -11.43 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 J2-A))
    (pad 31 thru_hole circle (at -12.7 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at -13.97 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 J1-A))
    (pad 33 thru_hole circle (at -15.24 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -16.51 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at -17.78 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 J5-B))
    (pad 36 thru_hole circle (at -19.05 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 J6-B))
    (pad 37 thru_hole circle (at -20.32 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 J3-B))
    (pad 38 thru_hole circle (at -21.59 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 IN+B))
    (pad 39 thru_hole circle (at -22.86 3.81 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 J1-B))
    (pad 40 thru_hole circle (at -24.13 5.715 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC-B))
    (pad "" np_thru_hole circle (at -28.065 2.858 270) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (model "C:/Users/tjames/Documents/Work - Teaching Lab Coordinator/ME370 Op Amp/716617040.wrl"
      (at (xyz -0.95 -0.225 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58D14759)
    (at 178.054 48.514 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J1 (at 6.096 0 360) (layer F.SilkS))
    (fp_text value LEDGND (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58D1475F)
    (at 178.054 39.624 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J2 (at 6.096 0.254 360) (layer F.SilkS))
    (fp_text value IN (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 IN+))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 IN-))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:Molex_PicoBlade_53398-0871_08x1.25mm_Straight" (layer Top) (tedit 58D1476A)
    (at 192.532 50.8 90)
    (descr "Molex PicoBlade, single row, top entry type, surface mount, PN:53398-0871")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference J3 (at -9.144 1.016 360) (layer F.SilkS))
    (fp_text value PCB (at 0 4.25 90) (layer F.Fab))
    (fp_text user %R (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -4.375 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at -3.125 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 39 OUT-))
    (pad 3 smd rect (at -1.875 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 40 OUT+))
    (pad 4 smd rect (at -0.625 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 43 VPP))
    (pad 5 smd rect (at 0.625 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 6 smd rect (at 1.875 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 42 VDD))
    (pad 7 smd rect (at 3.125 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 38 IN+))
    (pad 8 smd rect (at 4.375 -1.375 90) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 37 IN-))
    (pad "" smd rect (at -6.875 1.375 90) (size 2.2 3.1) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at 6.875 1.375 90) (size 2.2 3.1) (layers Top F.Paste F.Mask))
    (model "../../../../../../Users/tjames/Documents/Work - Teaching Lab Coordinator/ME370 Op Amp/533908711.wrl"
      (at (xyz 0 -0.015 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "../../../../../../Users/tjames/Documents/Work - Teaching Lab Coordinator/ME370 Op Amp/533980871.wrl"
      (at (xyz 0 -0.015 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58D1475B)
    (at 178.054 57.404 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J4 (at 6.096 0.254 360) (layer F.SilkS))
    (fp_text value OUT (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 OUT-))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 OUT+))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer Top) (tedit 58C069AF)
    (at 177.8 75.692 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer Top) (tedit 58C069B2)
    (at 184.658 75.692 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.08 0.127 180) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 +5V))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer Top) (tedit 58C05E7B)
    (at 178.308 93.472 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 0.762 -3.81 90) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 -12V))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer Top) (tedit 58C069B7)
    (at 194.564 87.122 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 0.762 4.572 180) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 -5V))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_3pol (layer Top) (tedit 58D14784)
    (at 177.8 80.264 270)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P4 (at -3.048 2.794 360) (layer F.SilkS))
    (fp_text value VIN (at 3.5 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 GNDPWR))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 -12V))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 +12V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_3pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:SOIC-8-N" (layer Top) (tedit 58D14828)
    (at 186.182 83.058 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at -3.81 1.27 360) (layer F.SilkS))
    (fp_text value 78L05C (at 0 1.27 270) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 33 +12V))
    (pad 2 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 2 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 35 +5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:SOIC-8-N" (layer Top) (tedit 58D1482D)
    (at 186.182 89.154 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at -3.81 -1.524 180) (layer F.SilkS))
    (fp_text value 79L05C (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 34 -12V))
    (pad 2 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 34 -12V))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 41 GNDPWR))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask))
    (pad 2 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 34 -12V))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 34 -12V))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 36 -5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:BreakAway75mm" (layer Top) (tedit 58BD85DB)
    (at 171.5135 66.04 90)
    (fp_text reference REF** (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text value BreakAway75mm (at 0 -8.89 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.524 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 21 np_thru_hole circle (at -0.508 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 31 np_thru_hole circle (at 0.508 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 41 np_thru_hole circle (at 1.524 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 12 np_thru_hole circle (at -1.524 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 22 np_thru_hole circle (at -0.508 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 32 np_thru_hole circle (at 0.508 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 42 np_thru_hole circle (at 1.524 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module "Custom Library:BreakAway75mm" (layer Top) (tedit 58BD85DB)
    (at 199.39 66.04 90)
    (fp_text reference REF** (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text value BreakAway75mm (at 0 -8.89 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.524 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 21 np_thru_hole circle (at -0.508 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 31 np_thru_hole circle (at 0.508 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 41 np_thru_hole circle (at 1.524 -1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 12 np_thru_hole circle (at -1.524 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 22 np_thru_hole circle (at -0.508 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 32 np_thru_hole circle (at 0.508 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad 42 np_thru_hole circle (at 1.524 1.016 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer Top) (tedit 58C07DFD)
    (at 205.74 96.612)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module "Custom Library:71660-7040" (layer Top) (tedit 58C06A7A)
    (at 210.82 78.232 90)
    (fp_text reference P5 (at 12.192 7.62 90) (layer F.SilkS))
    (fp_text value DIL40 (at 12.192 -2.921 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.04 5.058 90) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.94 2.858 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 GND-A2))
    (pad 2 thru_hole circle (at 1.27 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 J6-A2))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 J6-A2))
    (pad 4 thru_hole circle (at 3.81 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 J4-A2))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 J4-A2))
    (pad 6 thru_hole circle (at 6.35 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 J2-A2))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 GND-A2))
    (pad 8 thru_hole circle (at 8.89 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 J7-A2))
    (pad 9 thru_hole circle (at 10.16 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 VSS-A2))
    (pad 10 thru_hole circle (at 11.43 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 GND-A2))
    (pad 11 thru_hole circle (at 12.7 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 VCC-A2))
    (pad 12 thru_hole circle (at 13.97 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 IN+A2))
    (pad 13 thru_hole circle (at 15.24 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 IN-A2))
    (pad 14 thru_hole circle (at 16.51 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 17.78 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 J1-A2))
    (pad 16 thru_hole circle (at 19.05 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 J3-A2))
    (pad 17 thru_hole circle (at 20.32 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 J3-A2))
    (pad 18 thru_hole circle (at 21.59 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 J5-A2))
    (pad 19 thru_hole circle (at 22.86 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 J5-A2))
    (pad 20 thru_hole circle (at 24.13 1.905 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 J7-A2))
    (pad 21 thru_hole circle (at 0 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 1.27 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 VSS-A2))
    (pad 23 thru_hole circle (at 2.54 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 J4-A2))
    (pad 24 thru_hole circle (at 3.81 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 IN-A2))
    (pad 25 thru_hole circle (at 5.08 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 J2-A2))
    (pad 26 thru_hole circle (at 6.35 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 7.62 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 8.89 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 J7-A2))
    (pad 29 thru_hole circle (at 10.16 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 11.43 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 J2-A2))
    (pad 31 thru_hole circle (at 12.7 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 13.97 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 J1-A2))
    (pad 33 thru_hole circle (at 15.24 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 16.51 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 17.78 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 J5-A2))
    (pad 36 thru_hole circle (at 19.05 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 J6-A2))
    (pad 37 thru_hole circle (at 20.32 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 J3-A2))
    (pad 38 thru_hole circle (at 21.59 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 IN+A2))
    (pad 39 thru_hole circle (at 22.86 3.81 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 J1-A2))
    (pad 40 thru_hole circle (at 24.13 5.715 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 VCC-A2))
    (pad "" np_thru_hole circle (at 28.065 2.858 90) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (model "../../../../../../Users/tjames/Documents/Work - Teaching Lab Coordinator/ME370 Op Amp/716607040.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:POT93YA" (layer Top) (tedit 58D16640)
    (at 61.468 66.04)
    (fp_text reference RGain1 (at 1.27 -6.985) (layer F.SilkS) hide)
    (fp_text value RGain (at -8.128 -1.016 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0) (size 2.03962 2.03962) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 J2-A))
    (pad 1 thru_hole rect (at 0 -2.54) (size 2.24028 2.24028) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 J1-A))
    (pad 3 thru_hole circle (at 0 2.54) (size 2.24028 2.24028) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3296W.wrl
      (at (xyz 0 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D16824)
    (at 82.804 37.592 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -7.62 180) (layer F.SilkS))
    (fp_text value R1 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 J3-A))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 J1-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D16774)
    (at 82.804 94.488 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 7.62 180) (layer F.SilkS))
    (fp_text value R2 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 J4-A))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 J2-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D16820)
    (at 108.204 37.592 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.334 -7.62 180) (layer F.SilkS))
    (fp_text value R3 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 J5-A))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 J3-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D16774)
    (at 108.204 94.488 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 7.62 180) (layer F.SilkS))
    (fp_text value R4 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 J6-A))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 J4-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D1681D)
    (at 133.35 37.592 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 4.826 -7.62 180) (layer F.SilkS))
    (fp_text value R5 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 J7-A))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 J5-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Library:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer Top) (tedit 58D16774)
    (at 133.35 94.488 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 7.62 180) (layer F.SilkS))
    (fp_text value R6 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 OUT-B))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 J6-C))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text OUTPUT (at 141.732 70.104 90) (layer F.SilkS))
  (gr_text INPUT (at 65.278 66.04 90) (layer F.SilkS))
  (gr_text V+ (at 78.74 59.944 90) (layer B.SilkS))
  (gr_text V+ (at 78.74 74.93 90) (layer B.SilkS))
  (gr_text OUT (at 76.454 59.436 90) (layer B.SilkS))
  (gr_text OUT (at 76.454 74.422 90) (layer B.SilkS))
  (gr_text IN+ (at 76.2 66.802 90) (layer B.SilkS))
  (gr_text IN- (at 78.74 66.802 90) (layer B.SilkS))
  (gr_text IN- (at 78.74 52.07 90) (layer B.SilkS))
  (gr_text IN+ (at 76.2 52.07 90) (layer B.SilkS))
  (gr_text V- (at 73.66 66.802 90) (layer B.SilkS))
  (gr_text V- (at 73.66 52.07 90) (layer B.SilkS))
  (gr_text V+ (at 129.032 67.056 90) (layer B.SilkS))
  (gr_text OUT (at 126.492 66.548 90) (layer B.SilkS))
  (gr_text V- (at 123.952 58.674 90) (layer B.SilkS))
  (gr_text IN+ (at 126.746 58.674 90) (layer B.SilkS))
  (gr_text IN- (at 129.286 58.674 90) (layer B.SilkS))
  (gr_text +5V (at 187.452 79.248) (layer F.SilkS))
  (gr_text -5V (at 187.198 92.964) (layer F.SilkS))
  (gr_text "OUT+\nOUT-" (at 183.642 59.182) (layer F.SilkS))
  (gr_text "LED\nGND" (at 183.134 50.292) (layer F.SilkS))
  (gr_text "IN-\nIN+" (at 183.388 41.402) (layer F.SilkS))
  (gr_text "IN-\nIN+\nVCC\nGND\nVSS\nOUT+\nOUT-\nNC" (at 188.468 50.8) (layer F.SilkS))
  (gr_line (start 170.292 68.072) (end 170.292 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 68.072) (end 170.292 68.072) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 103.632) (end 172.72 68.072) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 103.632) (end 172.72 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 68.072) (end 198.12 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 68.072) (end 198.12 68.072) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 103.632) (end 200.66 68.072) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 103.632) (end 226.06 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 226.06 28.632) (end 226.06 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 28.632) (end 226.06 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 64.008) (end 200.66 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 64.008) (end 200.66 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 28.632) (end 198.12 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 28.632) (end 198.12 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 64.008) (end 172.72 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.292 64.008) (end 172.72 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.292 28.632) (end 170.292 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.292 103.632) (end 50.292 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.292 28.632) (end 170.292 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.292 103.632) (end 50.292 28.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RGAIN B" (at 62.484 81.788) (layer F.SilkS))
  (gr_text "RGAIN A" (at 62.484 50.292) (layer F.SilkS))
  (gr_text "R6 B" (at 135.636 91.948) (layer F.SilkS))
  (gr_text "R6 A" (at 120.904 91.948) (layer F.SilkS))
  (gr_text "R4 B" (at 110.744 91.948) (layer F.SilkS))
  (gr_text "R4 A" (at 95.504 91.948) (layer F.SilkS))
  (gr_text "R2 B" (at 85.344 91.948) (layer F.SilkS))
  (gr_text "R2 A" (at 70.104 91.948) (layer F.SilkS))
  (gr_text "R5 B" (at 135.636 40.132) (layer F.SilkS))
  (gr_text "R5 A" (at 120.904 40.132) (layer F.SilkS))
  (gr_text "R3 B" (at 110.744 40.132) (layer F.SilkS))
  (gr_text "R3 A" (at 95.504 40.132) (layer F.SilkS))
  (gr_text "R1 B" (at 85.344 40.132) (layer F.SilkS))
  (gr_text "R1 A" (at 70.104 40.132) (layer F.SilkS))
  (gr_text "IN-\nIN+\nVCC\nGND\nVSS\nOUT+\nOUT-\nNC" (at 158.75 67.564) (layer B.SilkS))
  (zone (net 4) (net_name VCC-B) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 96.52) (xy 57.658 96.52) (xy 57.658 34.798) (xy 160.02 34.798)
      )
    )
  )
  (zone (net 3) (net_name VSS-B) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 96.52) (xy 57.658 96.52) (xy 57.658 34.798) (xy 160.02 34.798)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads no (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.18 103.632) (xy 50.292 103.632) (xy 50.292 28.956) (xy 170.18 28.956)
      )
    )
    (polygon
      (pts        (xy 56.896 34.036) (xy 56.896 97.536) (xy 161.036 97.536) (xy 161.036 34.036)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads no (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.18 103.632) (xy 50.292 103.632) (xy 50.292 28.956) (xy 170.18 28.956)
      )
    )
    (polygon
      (pts        (xy 56.896 34.036) (xy 56.896 97.536) (xy 161.036 97.536) (xy 161.036 34.036)
      )
    )
  )
  (zone (net 41) (net_name GNDPWR) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 103.632) (xy 172.72 103.632) (xy 172.72 28.956) (xy 198.12 28.956)
      )
    )
  )
  (zone (net 41) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 103.632) (xy 172.72 103.632) (xy 172.72 92.964) (xy 198.12 92.964)
      )
    )
  )
  (zone (net 33) (net_name +12V) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 81.534) (xy 172.72 81.534) (xy 172.72 70.358) (xy 198.12 70.358)
      )
    )
  )
  (zone (net 41) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 69.596) (xy 172.72 69.596) (xy 172.72 28.702) (xy 198.12 28.702)
      )
    )
  )
  (zone (net 41) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 84.836) (xy 184.912 84.836) (xy 184.912 87.63) (xy 181.356 87.63) (xy 181.356 85.344)
        (xy 172.72 85.344) (xy 172.72 82.042) (xy 198.12 82.042)
      )
    )
  )
  (zone (net 34) (net_name -12V) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.848 88.138) (xy 198.12 88.138) (xy 198.12 92.456) (xy 172.72 92.456) (xy 172.72 85.852)
        (xy 180.848 85.852)
      )
    )
  )
)
