(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Manufacturing Output/")
		)
	)
	(net 0 "")
	(net 1 "Net-(IC1-C1-)")
	(net 2 "Net-(IC1-C1+)")
	(net 3 "Net-(IC1-C2-)")
	(net 4 "Net-(IC1-C2+)")
	(net 5 "GND")
	(net 6 "/V+")
	(net 7 "/V-")
	(net 8 "+2V5")
	(net 9 "Net-(D1-A)")
	(net 10 "/TX232")
	(net 11 "Net-(IC1-T2IN)")
	(net 12 "/TX")
	(net 13 "/RX232")
	(net 14 "Net-(IC1-R2IN)")
	(net 15 "/RX")
	(net 16 "Net-(IC1-R2OUT)")
	(net 17 "Net-(IC1-T2OUT)")
	(net 18 "unconnected-(J2-Pad1)")
	(net 19 "unconnected-(J2-Pad7)")
	(net 20 "unconnected-(J2-Pad8)")
	(net 21 "unconnected-(J2-Pad4)")
	(net 22 "unconnected-(J2-Pad9)")
	(net 23 "unconnected-(J2-Pad6)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 120.96 56.8 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/TX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/RX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+2V5")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 125.8 50.6)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 137.8 41.4)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H2"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at -1.5 1.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "SamacSys_Parts:SOP65P778X199-16N"
		(layer "F.Cu")
		(at 125.6 44.8)
		(descr "16-SSOP-5.3_MM")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX3316EEAE+"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:SOP65P778X199-16N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/MAX3316EEAE+.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "+/-15kV ESD-Protected, 2.5V, 1A, 460kbps, RS-232-Compatible Transceivers"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.99"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "700-MAX3316EEAE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=700-MAX3316EEAE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "MAX3316EEAE+"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.498 -2.275 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(IC1-C1+)")
			(pinfunction "C1+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.498 -1.625 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/V+")
			(pinfunction "V+")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.498 -0.975 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(IC1-C1-)")
			(pinfunction "C1-")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -3.498 -0.325 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(IC1-C2+)")
			(pinfunction "C2+")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.498 0.325 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(IC1-C2-)")
			(pinfunction "C2-")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -3.498 0.975 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/V-")
			(pinfunction "V-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -3.498 1.625 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(IC1-T2OUT)")
			(pinfunction "T2OUT")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -3.498 2.275 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(IC1-R2IN)")
			(pinfunction "R2IN")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.498 2.275 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(IC1-R2OUT)")
			(pinfunction "R2OUT")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 3.498 1.625 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(IC1-T2IN)")
			(pinfunction "T2IN")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 3.498 0.975 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/TX")
			(pinfunction "T1IN")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 3.498 0.325 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/RX")
			(pinfunction "R1OUT")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 3.498 -0.325 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/RX232")
			(pinfunction "R1IN")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 3.498 -0.975 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/TX232")
			(pinfunction "T1OUT")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 3.498 -1.625 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 3.498 -2.275 90)
			(size 0.45 1.705)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "+2V5")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "C:\\Users\\jmwau\\OneDrive\\Documents\\Projects\\UART to RS232 2.5V\\SamacSys_Parts.3dshapes\\MAX3316EEAE+.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 116.1 42.8625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -2.3625 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(IC1-C1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(IC1-C1-)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 116.1 46.3625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 2 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(IC1-C2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(IC1-C2-)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 125.8 53.1125 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -0.05 -1.63 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+2V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 131.2 42.7375 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+2V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 137.8 58.7)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H3"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 118.9625 43)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/V+")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm"
		(locked yes)
		(layer "F.Cu")
		(at 119.46 34.8 180)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
		(property "Reference" "J2"
			(at -5.54 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "DE9_Receptacle_MountingHoles"
			(at -5.54 15.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9-pin female receptacle socket D-SUB connector, Mounting Hole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Female*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 11.265 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 0.3 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6.96 0.3 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J2-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/RX232")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/TX232")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J2-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J2-Pad6)")
			(pinfunction "6")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J2-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J2-Pad8)")
			(pinfunction "8")
			(pintype "passive+no_connect")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J2-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 118.9375 46 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/V-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
		(layer "B.Cu")
		(at 118.6 49 180)
		(descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
		(tags "Through Hole Mount Test Points")
		(property "Reference" "TP3"
			(at 0 2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.4 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(IC1-T2OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
		(layer "B.Cu")
		(at 132.4 52.4)
		(descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
		(tags "Through Hole Mount Test Points")
		(property "Reference" "TP2"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(IC1-R2OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
		(layer "B.Cu")
		(at 118.6 52.4)
		(descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
		(tags "Through Hole Mount Test Points")
		(property "Reference" "TP4"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at -2.5 6.05 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(IC1-R2IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
		(layer "B.Cu")
		(at 132.4 49 180)
		(descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
		(tags "Through Hole Mount Test Points")
		(property "Reference" "TP1"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Keystone_5000-5004_Miniature"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(IC1-T2IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "B.Cu")
		(at 112.2 41.4 180)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H1"
			(at 0 2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -3.35 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "B.Cu")
		(at 112.2 58.7 180)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "H4"
			(at 0 3.35 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -3.35 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "UART to RS232.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(gr_rect
		(start 108.8 27)
		(end 141.2 62.1)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "Waughtal's 2.5V UART to RS232 Adapter"
		(at 137.1 27.85 0)
		(layer "B.SilkS")
	)
	(gr_text "Rx"
		(locked yes)
		(at 124.2 61 90)
		(layer "F.SilkS")
	)
	(gr_text "2V5"
		(locked yes)
		(at 127 62 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(locked yes)
		(at 129.6 62 90)
		(layer "F.SilkS")
	)
	(gr_text "Tx"
		(locked yes)
		(at 121.8 61 90)
		(layer "F.SilkS")
	)
	(zone
		(net 5)
		(net_name "GND")
		(locked yes)
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 141.2 62.1) (xy 108.8 62.1) (xy 108.8 27) (xy 141.2 27)
			)
		)
	)
)
