(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 112)
    (zones 0)
    (modules 15)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 ICSPCLK)
  (net 7 ICSPDAT)
  (net 8 -MCLR)
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(U1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net -MCLR)
    (add_net GND)
    (add_net ICSPCLK)
    (add_net ICSPDAT)
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(U1-Pad2)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C2C8C6C)
    (at 135.509 100.203 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.127 -1.8542 180) (layer B.SilkS))
    (fp_text value ,1u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C2C8C74)
    (at 133.604 105.791 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.3462) (layer B.SilkS))
    (fp_text value .1u (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5C2AD2A3)
    (at 133.223 109.474 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at -3.2766 0.254 270) (layer F.SilkS))
    (fp_text value BAS40-04 (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C2ACF19)
    (at 133.985 90.17 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at -2.8448 0.0254 270) (layer F.SilkS) hide)
    (fp_text value R/G (at 1.27 2.96 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C2ACF16)
    (at 129.54 90.17 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at -2.8448 -0.2032 270) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C2ACF1C)
    (at 138.43 92.71 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 5.2832 0.0508 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5C2ACEEE)
    (at 128.905 95.25)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at -2.667 5.1816) (layer F.SilkS) hide)
    (fp_text value ICSP (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ICSPCLK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 ICSPDAT))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 -MCLR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C2C8C70)
    (at 139.0396 107.3404 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.048 -0.2032 180) (layer B.SilkS))
    (fp_text value 10M (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C2ACE5F)
    (at 129.032 109.728 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.9304 -1.5748 270) (layer F.SilkS))
    (fp_text value 5K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C2C8CB0)
    (at 138.43 107.315 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.19532 -0.60452 270) (layer F.SilkS))
    (fp_text value 10M (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C2C8C66)
    (at 133.2992 96.774)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.1016 1.6764 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 ICSPCLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5C2C8CCF)
    (at 133.7564 101.0412 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.44704 0.4572 180) (layer F.SilkS))
    (fp_text value PIC12F1822 (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 ICSPDAT))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 ICSPCLK))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 -MCLR))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5C2C8CB6)
    (at 133.604 105.791)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U2 (at 2.78892 -0.01016 90) (layer F.SilkS))
    (fp_text value MCP6L91R (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5C2ACED7)
    (at 128.905 113.919 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at -2.2098 4.9022 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C2ACED4)
    (at 139.065 99.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 2.4638 1.3208) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 -MCLR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PROBE (at 134.1628 96.86544) (layer F.SilkS))
  (gr_text LOGIC (at 134.09676 94.87408) (layer F.SilkS))
  (gr_text iC31 (at 134.0104 94.996) (layer B.SilkS))
  (gr_text S (at 136.3472 111.8616) (layer F.SilkS))
  (gr_text - (at 133.858 111.9124) (layer F.SilkS))
  (gr_text + (at 131.4196 111.7092) (layer F.SilkS))
  (gr_text IN (at 136.4996 111.3028 270) (layer B.SilkS))
  (gr_text VCC (at 131.1656 110.3884 270) (layer B.SilkS))
  (gr_text GND (at 133.9088 110.2868 270) (layer B.SilkS))
  (gr_text TTL (at 139.446 95.758 90) (layer F.SilkS))
  (gr_line (start 140.462 88.9) (end 127.508 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 115.316) (end 140.462 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.508 115.316) (end 127.508 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 115.316) (end 127.508 115.316) (angle 90) (layer Edge.Cuts) (width 0.15))
)
